[DEPARTMENT] Aggregates

[CATEGORY] Sampling and Preparation of Aggregates
Sampling and preparation of aggregates and fillers is necessary for a variety of reasons including research, design and quality control. The main aim of sampling is to obtain a sample representative of the average quality. Sampling techniques and procedures are described in various standards including BS 812: Part 101 and 102 and ASTM D75. Individual items of equipment necessary for sampling and preparation are described in the soils section of the catalogue.

[CATEGORY] Drying, Weighing and Moisture Content
Most test techniques involve the use of drying ovens and balances. The moisture content of aggregate is of importance e.g. when batching concrete or when compacting unbound materials to achieve a specified density. Accurate means of determining moisture content are specified in various Standards and include methods suitable for use in the laboratory or on the construction site.

[PRODUCT GROUP] Oven Drying Method
The standard method for determining the moisture content of soil is the Oven Drying Method, which is recommended for a Soils Laboratory.

[GROUPED PRODUCT MATRIX]
Model No.
	Voltage
	Desc
	Fluctuation
	Shelves
	Positions
	Capacity, litres
	Int. Dimensions
	Temp. Range °C
	
78-1225/01
	220-240 V 50/60Hz
	Drying Oven
	+/- 0.75 °C
	3
	4
	100
	460 x 490 x 450 mm
	40 - 250 °C
	
78-1235/01
	220-240 V 50/60 Hz
	Drying Oven
	+/- 0.75 °C
	3
	5
	150
	540 x 490 x 550 mm
	40 - 250 °C
	
78-1250/01
	220-240 V 50/60 Hz
	Drying Oven
	+/- 0.75 °C
	3
	4
	225
	440 x 920 x 600 mm
	0 - 200 °C
	
78-0135/01
	220-240 V 50/60 Hz
	Drying Oven
	+/- 0.75 °C
	4
	5
	425
	640 x 920 x 760 mm
	0 - 200 °C
	
78-1215/01
	220-240 V 50/60 Hz
	Drying Oven
	+/- 0.75 °C
	2
	3
	50
	330 x 490 x 330 mm
	40 - 250 °C

[PRODUCT GROUP] Rapid method by Speedy Moisture Tester
*Reliable and accurate moisture measurement in the field*Direct reading in percent moisture*Rapid results in minutes*New versions with heavy duty plastic carrying caseand portable electronic balanceThe new range of Speedy Moisture testers now includes an electronic balance and a heavy duty plastic case. Designed for the most demanding on-site conditions, the new waterproof and durable case offers high levels of protection. The new model comprises: Speedy Moisture tester, electronic balance, beaker, cleaning cloth, cap, washer, scoop, steel pulverising balls, and cleaning brushes. Used to weigh a sample before placing it in the Speedy Moisture Tester, the portable battery powered balance includes LCD display with a measuring range 0 - 200 g x 0 g. The % moisture content of the sample is read directly from the calibrated pressure gauge.

[GROUPED PRODUCT MATRIX]
Model No.
	Model
	Moisture range
	Gauge div.
	Sample wgt.
	
23-7452
	D2 Large
	0 to 20
	0.2
	20
	
23-7462
	G2 Large
	0 to 50
	0.5
	8
	
23-7502
	D2 Small
	0 to 20
	0.2
	6

[PRODUCT GROUP] Accessories for the Speedy Moisture Tester

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	
23-7600
	Speedy Calibration Unit
	
23-7700
	Calcium carbide powder - 500g
	
23-7702
	Calcium carbide powder - 12 x 500 g

[CATEGORY] Particle Size and Shape
Among many of the applications to which aggregate lends itself is its use in economical concrete mixes, impervious, durable asphalts, macadams and road bases. Particle size, shape and texture can have considerable effects on various design properties and are generally specified within certain limits. Rounded aggregate can lead to instability in a bituminous mixture yet be ideal as a concrete aggregate where good workability of the mix is essential for placing and compaction.

[PRODUCT GROUP] Sand Equivalent Value

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	
24-4919
	Sand equivalent apparatus ASTM D2419
	
24-4925
	Syphon assembly
	
24-4930
	Calcium chloride
	
24-4932
	Formaldehyde
	
24-4934
	Glycerol analar
	
24-4945/01
	Motorised sand equivalent shaker

[PRODUCT GROUP] 200mm Diameter BS Sieves

[GROUPED PRODUCT MATRIX]
Model No.
	Ap. Size
	Type
	
79-0010
	-
	Lid
	
79-0020
	-
	Receiver
	
79-0050
	45 μm
	Mesh
	
79-0060
	53 μm
	Mesh
	
79-0070
	63 μm
	Mesh
	
79-0080
	75 μm
	Mesh
	
79-0085
	80 μm
	Mesh
	
79-0090
	90 μm
	Mesh
	
79-0095
	100 μm
	Mesh
	
79-0100
	106 μm
	Mesh
	
79-0110
	125 μm
	Mesh
	
79-0120
	150 μm
	Mesh
	
79-0125
	160 μm
	Mesh
	
79-0140
	212 μm
	Mesh
	
79-0150
	250 μm
	Mesh
	
79-0160
	300 μm
	Mesh
	
79-0175
	400 μm
	Mesh
	
79-0180
	425 μm
	Mesh
	
79-0190
	500 μm
	Mesh
	
79-0200
	600 μm
	Mesh
	
79-0210
	710 μm
	Mesh
	
79-0220
	850 μm
	Mesh
	
79-0230
	1 mm
	Mesh
	
79-0240
	1.18 mm
	Mesh
	
79-0245
	1.25 mm
	Mesh
	
79-0250
	1.40 mm
	Mesh
	
79-0255
	1.60 mm
	Mesh
	
79-0260
	1.70 mm
	Mesh
	
79-0270
	2 mm
	Mesh
	
79-0280
	2.36 mm
	Mesh
	
79-0285
	2.50 mm
	Mesh
	
79-0290
	2.80 mm
	Mesh
	
79-0300
	3.35 mm
	Mesh
	
79-0310
	4 mm
	Mesh
	
79-0320
	4.75 mm
	Mesh
	
79-1500
	4 mm
	Perforated
	
79-1510
	4.75 mm
	Perforated
	
79-1515
	5 mm
	Perforated
	
79-1520
	5.60 mm
	Perforated
	
79-1525
	6.30 mm
	Perforated
	
79-1530
	6.70 mm
	Perforated
	
79-1540
	8 mm
	Perforated
	
79-1550
	9.50 mm
	Perforated
	
79-1555
	10 mm
	Perforated
	
79-1560
	11.20 mm
	Perforated
	
79-1565
	12.50 mm
	Perforated
	
79-1570
	13.20 mm
	Perforated
	
79-1575
	14 mm
	Perforated
	
79-1580
	16 mm
	Perforated
	
79-1590
	19 mm
	Perforated
	
79-1595
	20 mm
	Perforated
	
79-1600
	22.40 mm
	Perforated
	
79-1605
	25 mm
	Perforated
	
79-1610
	26.50 mm
	Perforated
	
79-1615
	28 mm
	Perforated
	
79-1630
	31.50 mm
	Perforated
	
79-1640
	37.50 mm
	Perforated
	
79-1655
	50 mm
	Perforated
	
79-1660
	53 mm
	Perforated
	
79-1670
	63 mm
	Perforated
	
79-1680
	75 mm
	Perforated

[PRODUCT GROUP] 300mm Diameter BS Sieves

[GROUPED PRODUCT MATRIX]
Model No.
	Ap. Size
	Type
	
79-2010
	-
	Lid
	
79-2020
	-
	Receiver
	
79-2070
	63 μm
	Mesh
	
79-2080
	75 μm
	Mesh
	
79-2085
	80 μm
	Mesh
	
79-2090
	90 μm
	Mesh
	
79-2095
	100 μm
	Mesh
	
79-2110
	125 μm
	Mesh
	
79-2120
	150 μm
	Mesh
	
79-2135
	200 μm
	Mesh
	
79-2140
	212 μm
	Mesh
	
79-2150
	250 μm
	Mesh
	
79-2160
	300 μm
	Mesh
	
79-2165
	315 μm
	Mesh
	
79-2180
	425 μm
	Mesh
	
79-2190
	500 μm
	Mesh
	
79-2200
	600 μm
	Mesh
	
79-2205
	630 μm
	Mesh
	
79-2220
	850 μm
	Mesh
	
79-2230
	1 mm
	Mesh
	
79-2240
	1.18 mm
	Mesh
	
79-2245
	1.25 mm
	Mesh
	
79-2255
	1.60 mm
	Mesh
	
79-2260
	1.70 mm
	Mesh
	
79-2270
	2 mm
	Mesh
	
79-2280
	2.36 mm
	Mesh
	
79-2285
	2.50 mm
	Mesh
	
79-2300
	3.35 mm
	Mesh
	
79-2320
	4.75 mm
	Mesh
	
79-2500
	4 mm
	Perforated
	
79-2510
	4.75 mm
	Perforated
	
79-2515
	5 mm
	Perforated
	
79-2525
	6.30 mm
	Perforated
	
79-2530
	6.70 mm
	Perforated
	
79-2540
	8 mm
	Perforated
	
79-2550
	9.50 mm
	Perforated
	
79-2555
	10 mm
	Perforated
	
79-2565
	12.50 mm
	Perforated
	
79-2570
	13.20 mm
	Perforated
	
79-2575
	14 mm
	Perforated
	
79-2580
	16 mm
	Perforated
	
79-2590
	19 mm
	Perforated
	
79-2595
	20 mm
	Perforated
	
79-2600
	22.40 mm
	Perforated
	
79-2605
	25 mm
	Perforated
	
79-2610
	26.50 mm
	Perforated
	
79-2615
	28 mm
	Perforated
	
79-2630
	31.50 mm
	Perforated
	
79-2640
	37.50 mm
	Perforated
	
79-2645
	40 mm
	Perforated
	
79-2655
	50 mm
	Perforated
	
79-2660
	53 mm
	Perforated
	
79-2670
	63 mm
	Perforated
	
79-2680
	75 mm
	Perforated
	
79-2684
	80 mm
	Perforated
	
79-2710
	125 mm
	Perforated

[PRODUCT GROUP] 8" Diameter ASTM Sieves

[GROUPED PRODUCT MATRIX]
Model No.
	Ap. Size
	Type
	
79-5400
	-
	Lid
	
79-5410
	-
	Receiver
	
79-5290
	45 µm
	Mesh
	
79-5270
	63 µm
	Mesh
	
79-5260
	75 µm
	Mesh
	
79-5250
	90 µm
	Mesh
	
79-5240
	106 µm
	Mesh
	
79-5230
	125 µm
	Mesh
	
79-5220
	150 µm
	Mesh
	
79-5210
	180 µm
	Mesh
	
79-5200
	121 µm
	Mesh
	
79-5190
	250 µm
	Mesh
	
79-5180
	300 µm
	Mesh
	
79-5160
	425 µm
	Mesh
	
79-5150
	500 µm
	Mesh
	
79-5140
	600 µm
	Mesh
	
79-5120
	850 µm
	Mesh
	
79-5110
	1 mm
	Mesh
	
79-5100
	1.18 mm
	Mesh
	
79-5090
	1.40 mm
	Mesh
	
79-5080
	1.70 mm
	Mesh
	
79-5070
	2 mm
	Mesh
	
79-5060
	2.36 mm
	Mesh
	
79-5050
	2.80 mm
	Mesh
	
79-5040
	3.35 mm
	Mesh
	
79-5000
	6.30 mm
	Mesh
	
79-5030
	4 mm
	Mesh
	
79-5020
	4.75 mm
	Mesh
	
79-5010
	5.60 mm
	Mesh
	
79-5490
	6.70 mm
	Mesh
	
79-5500
	8 mm
	Mesh
	
79-5510
	9.50 mm
	Mesh
	
79-5520
	11.20 mm
	Mesh
	
79-5530
	12.50 mm
	Mesh
	
79-5540
	13.20 mm
	Mesh
	
79-5550
	16 mm
	Mesh
	
79-5560
	19 mm
	Mesh
	
79-5570
	22.40 mm
	Mesh
	
79-5580
	25 mm
	Mesh
	
79-5610
	37.50 mm
	Mesh
	
79-5630
	50 mm
	Mesh
	
79-5650
	63 mm
	Mesh
	
79-5660
	75 mm
	Mesh

[PRODUCT GROUP] 12" Diameter ASTM Sieves

[GROUPED PRODUCT MATRIX]
Model No.
	Ap. Size
	Type
	
79-5800
	6.30 mm
	Mesh
	
79-5810
	5.60 mm
	Mesh
	
79-5820
	4.75 mm
	Mesh
	
79-5830
	4 mm
	Mesh
	
79-5840
	3.35 mm
	Mesh
	
79-5850
	2.80 mm
	Mesh
	
79-5860
	2.36 mm
	Mesh
	
79-5870
	2 mm
	Mesh
	
79-5880
	1.70 mm
	Mesh
	
79-5890
	1.40 mm
	Mesh
	
79-5900
	1.18 mm
	Mesh
	
79-5910
	1 mm
	Mesh
	
79-5920
	850 µm
	Mesh
	
79-5930
	710 µm
	Mesh
	
79-5940
	600 µm
	Mesh
	
79-5950
	500 µm
	Mesh
	
79-5960
	425 µm
	Mesh
	
79-5970
	355 µm
	Mesh
	
79-5980
	300 µm
	Mesh
	
79-5990
	250 µm
	Mesh
	
79-6000
	212 µm
	Mesh
	
79-6010
	180 µm
	Mesh
	
79-6020
	150 µm
	Mesh
	
79-6030
	125 µm
	Mesh
	
79-6040
	106 µm
	Mesh
	
79-6050
	90 µm
	Mesh
	
79-6060
	75 µm
	Mesh
	
79-6070
	63 µm
	Mesh
	
79-6080
	53 µm
	Mesh
	
79-6090
	45 µm
	Mesh
	
79-6100
	38 µm
	Mesh
	
79-6150
	-
	Lid
	
79-6160
	-
	Receiver
	
79-6190
	6.70 mm
	Mesh
	
79-6200
	8 mm
	Mesh
	
79-6210
	9.50 mm
	Mesh
	
79-6220
	11.20 mm
	Mesh
	
79-6230
	12.50 mm
	Mesh
	
79-6240
	13.20 mm
	Mesh
	
79-6250
	16 mm
	Mesh
	
79-6260
	19 mm
	Mesh
	
79-6270
	22.40 mm
	Mesh
	
79-6280
	25 mm
	Mesh
	
79-6290
	26.50 mm
	Mesh
	
79-6300
	31.50 mm
	Mesh
	
79-6310
	37.50 mm
	Mesh
	
79-6320
	45 mm
	Mesh
	
79-6330
	50 mm
	Mesh
	
79-6340
	53 mm
	Mesh
	
79-6350
	63 mm
	Mesh
	
79-6360
	75 mm
	Mesh
	
79-6370
	90 mm
	Mesh
	
79-6380
	100 mm
	Mesh
	
79-6400
	125 mm
	Mesh

[CATEGORY] Determination of Flakiness and Elongation
Aggregates which are flaky and/or elongated will often lower the workability of a concrete mix and may also affect long term durability. In bituminous mixtures flaky aggregate makes for a harsh mix and may also crack and break up during compaction by rolling.

[PRODUCT GROUP] Determination of the Shape Index
This method described in EN933-4 measures the ratio of length to width of individual aggregate particles using a vernier calliper and a specially designed 3:1 length gauge.

[PRODUCT] 3.1 Shape Index Caliper. (42-0821)
Designed to measure the ratio of length to width of individual aggregate particles.

_Standards_
EN 933-4

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Weight, kg
	1
	
Description
	3:1 Shape Index Calliper

_Related Products_
Accessory: 200 mm Diameter Lid (79-0010)
Accessory: 200 mm Diameter Receiver (79-0020)
Accessory: 200mm Dia BS Sieve 1.00mm Stainless Steel Mesh. (79-0230)
Accessory: 200mm Dia BS Sieve 125Mic Stainless Steel Mesh. (79-0110)
Accessory: 200mm Dia BS Sieve 2.00mm Stainless Steel Mesh. (79-0270)
Accessory: 200mm Dia BS Sieve 250Mic Stainless Steel Mesh. (79-0150)
Accessory: 200mm Dia BS Sieve 4.00mm Perforated Plate. (79-1500)
Accessory: 200mm Dia BS Sieve 500Mic Stainless Steel Mesh. (79-0190)
Accessory: 200mm Dia BS Sieve 63 Mic Stainless Steel Mesh. (79-0070)
Accessory: 200mm Dia BS Sieve 8.00mm Perforated Plate. (79-1540)
Accessory: 300mm Dia BS Sieve 125mm Perforated Plate. (79-2710)
Accessory: 300mm Dia BS Sieve 16.0mm Perforated Plate. (79-2580)
Accessory: 300mm Dia BS Sieve 31.5mm Perforated Plate. (79-2630)
Accessory: 300mm Dia BS Sieve 63.0mm Perforated Plate. (79-2670)
Accessory: 300mm Dia Lid. (79-2010)
Accessory: 300mm Dia Receiver. (79-2020)
Accessory: ELE Sieve Shaker (80-0200/06)
Accessory: ELE Sieve Shaker (80-0200/01)
Accessory: Sample Tray - 406 x 406 x 50 mm (81-4030)
Accessory: Sieve Brush Nylon (79-7210)

[PRODUCT] Vernier Caliper Range 0 to 200mm X 0.02mm. (81-0588)
Vernier callipers 200 x 0.002mm. Graduated in mm and inches.

_Standards_
EN 933-4, BS 1377

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Vernier caliper
	
Measuring Range mm
	0 - 200 mm x 0.02 mm

_Related Products_
Main: Shrinkage Mould to BS 1377 (24-1800)

[PRODUCT] Vernier Caliper (LCD) Range 0 to 200mm X 0.01mm (81-0590)
Dual measuring range highly accurate vernier caliper 0 to 200mm x 0.01mm (8 inch x 0.001 inch) to comply with bs 887 and bs 6365. Complete with liquid crystal display.

_Standards_
EN 933-4

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Vernier caliper
	
Weight, kg
	0.1
	
Measuring Range mm
	0 - 200 x 0.01 mm

_Related Products_
Accessory: Vibrating Hammer (47-0455/01)

[GROUPED PRODUCT MATRIX]
Model No.
	Measuring Range
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Elongation Index
This method classifies aggregate elongation by measuring the length of individual particles. The test is not applicable to material retained on a 63.0 mm BS test sieve.

[PRODUCT] Length Gauge (42-0820)
Manufactured to the dimensions specified in BS 182.

_Standards_
BS 812-105

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Length Gauge
	
Weight, kg
	0.7

_Related Products_
Accessory: 300mm Dia BS Sieve 10.0mm Perforated Plate. (79-2555)
Accessory: 300mm Dia BS Sieve 14.0mm Perforated Plate. (79-2575)
Accessory: 300mm Dia BS Sieve 20.0mm Perforated Plate. (79-2595)
Accessory: 300mm Dia BS Sieve 28.0mm Perforated Plate. (79-2615)
Accessory: 300mm Dia BS Sieve 37.5mm Perforated Plate. (79-2640)
Accessory: 300mm Dia BS Sieve 50.0mm Perforated Plate. (79-2655)
Accessory: 300mm Dia BS Sieve 6.30mm Perforated Plate. (79-2525)
Accessory: 300mm Dia BS Sieve 63.0mm Perforated Plate. (79-2670)
Accessory: 300mm Dia Lid. (79-2010)
Accessory: 300mm Dia Receiver. (79-2020)
Accessory: ELE Sieve Shaker (80-0200/06)
Accessory: ELE Sieve Shaker (80-0200/01)
Main: Flakiness Gauge. (42-0410)
Accessory: Sample Tray - 1200 x 1160 x 50 mm (81-4230)
Accessory: Sample Tray - 406 x 406 x 50 mm (81-4030)
Main: Set of Flakiness Sieves Comprising 1 Ea 4.9mm 7.2mm 10.2mm 14.4mm 19.7mm 26.3mm and 33.9mm (42-0600)
Accessory: Shovel - With flat blade (81-0240)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Flakiness Sieves and Gauges

[PRODUCT] Flakiness Gauge. (42-0410)
Constructed of heavy gauge sheet steel to the dimensions specified in BS 812.

_Standards_
BS 812

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Weight, kg
	0.06
	
Description
	Flakiness Gauge

_Related Products_
Main: Length Gauge (42-0820)

[PRODUCT] Set of Flakiness Sieves Comprising 1 Ea 4.9mm 7.2mm 10.2mm 14.4mm 19.7mm 26.3mm and 33.9mm (42-0600)
Comprising of 1 each, 4.9 mm, 7.2 mm, 10.2 mm, 14.4 mm,19.7 mm, 26.3 mm and 33.9 mm.

_Standards_
BS 813

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Set of Flakiness Sieves

_Related Products_
Main: Length Gauge (42-0820)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Grid Sieves
A series of grid sieves formed from 5 mm diameter steel parallel bars securely fixed in a metal frame.

[PRODUCT] Grid Sieve 2.5mm Slot Width for EN Aggregate Flakiness Test. (42-0300)
2.5mm

_Standards_
EN 933-3

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA** Passing Size - 5 mm Retained Size - 4 mm

_Attributes_
Slot width, mm
	2.5
	
Passing Size, mm
	5
	
Retained Size, mm
	4

_Related Products_
Accessory: 300mm Dia BS Sieve 10.0mm Perforated Plate. (79-2555)
Accessory: 300mm Dia BS Sieve 12.5mm Perforated Plate (79-2565)
Accessory: 300mm Dia BS Sieve 16.0mm Perforated Plate. (79-2580)
Accessory: 300mm Dia BS Sieve 20.0mm Perforated Plate. (79-2595)
Accessory: 300mm Dia BS Sieve 25.0mm Perforated Plate. (79-2605)
Accessory: 300mm Dia BS Sieve 31.5mm Perforated Plate. (79-2630)
Accessory: 300mm Dia BS Sieve 4.00mm Perforated Plate. (79-2500)
Accessory: 300mm Dia BS Sieve 40.0mm Perforated Plate (79-2645)
Accessory: 300mm Dia BS Sieve 5.00mm Perforated Plate. (79-2515)
Accessory: 300mm Dia BS Sieve 50.0mm Perforated Plate. (79-2655)
Accessory: 300mm Dia BS Sieve 6.30mm Perforated Plate. (79-2525)
Accessory: 300mm Dia BS Sieve 63.0mm Perforated Plate. (79-2670)
Accessory: 300mm Dia BS Sieve 8.00mm Perforated Plate. (79-2540)
Accessory: 300mm Dia BS Sieve 80mm Perforated Plate (79-2684)
Accessory: 300mm Dia Lid. (79-2010)
Accessory: 300mm Dia Receiver. (79-2020)
Main: Grid Sieve 10mm Slot Width for EN Aggregate Flakiness Test. (42-0314)
Main: Grid Sieve 12.5mm Slot Width for EN Aggregate Flakiness Test. (42-0316)
Main: Grid Sieve 16mm Slot Width for EN Aggregate Flakiness Test. (42-0318)
Main: Grid Sieve 20mm Slot Width for EN Aggregate Flakiness Test. (42-0320)
Main: Grid Sieve 25mm Slot Width for EN Aggregate Flakiness Test. (42-0322)
Main: Grid Sieve 3.15mm Slot Width for EN Aggregate Flakiness Test. (42-0302)
Main: Grid Sieve 31.5mm Slot Width for EN Aggregate Flakiness Test. (42-0324)
Main: Grid Sieve 40mm Slot Width for EN Aggregate Flakiness Test. (42-0326)
Main: Grid Sieve 4mm Slot Width for EN Aggregate Flakiness Test. (42-0304)
Main: Grid Sieve 5mm Slot Width for EN Aggregate Flakiness Test. (42-0306)
Main: Grid Sieve 6.3mm Slot Width for EN Aggregate Flakiness Test. (42-0308)
Main: Grid Sieve 8mm Slot Width for EN Aggregate Flakiness Test. (42-0310)
Accessory: Sample Tray - 406 x 406 x 50 mm (81-4030)

[PRODUCT] Grid Sieve 3.15mm Slot Width for EN Aggregate Flakiness Test. (42-0302)
3.15mm

_Standards_
EN 933-3

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA** Passing Size - 6.3 mm Retained Size - 5 mm

_Attributes_
Slot width, mm
	3.15
	
Passing Size, mm
	6.3
	
Retained Size, mm
	5

_Related Products_
Accessory: 300mm Dia BS Sieve 10.0mm Perforated Plate. (79-2555)
Accessory: 300mm Dia BS Sieve 12.5mm Perforated Plate (79-2565)
Accessory: 300mm Dia BS Sieve 16.0mm Perforated Plate. (79-2580)
Accessory: 300mm Dia BS Sieve 20.0mm Perforated Plate. (79-2595)
Accessory: 300mm Dia BS Sieve 25.0mm Perforated Plate. (79-2605)
Accessory: 300mm Dia BS Sieve 31.5mm Perforated Plate. (79-2630)
Accessory: 300mm Dia BS Sieve 4.00mm Perforated Plate. (79-2500)
Accessory: 300mm Dia BS Sieve 40.0mm Perforated Plate (79-2645)
Accessory: 300mm Dia BS Sieve 5.00mm Perforated Plate. (79-2515)
Accessory: 300mm Dia BS Sieve 50.0mm Perforated Plate. (79-2655)
Accessory: 300mm Dia BS Sieve 6.30mm Perforated Plate. (79-2525)
Accessory: 300mm Dia BS Sieve 63.0mm Perforated Plate. (79-2670)
Accessory: 300mm Dia BS Sieve 8.00mm Perforated Plate. (79-2540)
Accessory: 300mm Dia BS Sieve 80mm Perforated Plate (79-2684)
Accessory: 300mm Dia Lid. (79-2010)
Accessory: 300mm Dia Receiver. (79-2020)
Main: Grid Sieve 10mm Slot Width for EN Aggregate Flakiness Test. (42-0314)
Main: Grid Sieve 12.5mm Slot Width for EN Aggregate Flakiness Test. (42-0316)
Main: Grid Sieve 16mm Slot Width for EN Aggregate Flakiness Test. (42-0318)
Main: Grid Sieve 2.5mm Slot Width for EN Aggregate Flakiness Test. (42-0300)
Main: Grid Sieve 20mm Slot Width for EN Aggregate Flakiness Test. (42-0320)
Main: Grid Sieve 25mm Slot Width for EN Aggregate Flakiness Test. (42-0322)
Main: Grid Sieve 31.5mm Slot Width for EN Aggregate Flakiness Test. (42-0324)
Main: Grid Sieve 40mm Slot Width for EN Aggregate Flakiness Test. (42-0326)
Main: Grid Sieve 4mm Slot Width for EN Aggregate Flakiness Test. (42-0304)
Main: Grid Sieve 5mm Slot Width for EN Aggregate Flakiness Test. (42-0306)
Main: Grid Sieve 6.3mm Slot Width for EN Aggregate Flakiness Test. (42-0308)
Main: Grid Sieve 8mm Slot Width for EN Aggregate Flakiness Test. (42-0310)
Accessory: Sample Tray - 406 x 406 x 50 mm (81-4030)

[PRODUCT] Grid Sieve 4mm Slot Width for EN Aggregate Flakiness Test. (42-0304)
4mm

_Standards_
EN 933-3

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA** Passing Size - 8 mm Retained Size - 6.3 mm

_Attributes_
Slot width, mm
	4
	
Passing Size, mm
	8
	
Retained Size, mm
	6.3

_Related Products_
Accessory: 300mm Dia BS Sieve 10.0mm Perforated Plate. (79-2555)
Accessory: 300mm Dia BS Sieve 12.5mm Perforated Plate (79-2565)
Accessory: 300mm Dia BS Sieve 16.0mm Perforated Plate. (79-2580)
Accessory: 300mm Dia BS Sieve 20.0mm Perforated Plate. (79-2595)
Accessory: 300mm Dia BS Sieve 25.0mm Perforated Plate. (79-2605)
Accessory: 300mm Dia BS Sieve 31.5mm Perforated Plate. (79-2630)
Accessory: 300mm Dia BS Sieve 4.00mm Perforated Plate. (79-2500)
Accessory: 300mm Dia BS Sieve 40.0mm Perforated Plate (79-2645)
Accessory: 300mm Dia BS Sieve 5.00mm Perforated Plate. (79-2515)
Accessory: 300mm Dia BS Sieve 50.0mm Perforated Plate. (79-2655)
Accessory: 300mm Dia BS Sieve 6.30mm Perforated Plate. (79-2525)
Accessory: 300mm Dia BS Sieve 63.0mm Perforated Plate. (79-2670)
Accessory: 300mm Dia BS Sieve 8.00mm Perforated Plate. (79-2540)
Accessory: 300mm Dia BS Sieve 80mm Perforated Plate (79-2684)
Accessory: 300mm Dia Lid. (79-2010)
Accessory: 300mm Dia Receiver. (79-2020)
Main: Grid Sieve 10mm Slot Width for EN Aggregate Flakiness Test. (42-0314)
Main: Grid Sieve 12.5mm Slot Width for EN Aggregate Flakiness Test. (42-0316)
Main: Grid Sieve 16mm Slot Width for EN Aggregate Flakiness Test. (42-0318)
Main: Grid Sieve 2.5mm Slot Width for EN Aggregate Flakiness Test. (42-0300)
Main: Grid Sieve 20mm Slot Width for EN Aggregate Flakiness Test. (42-0320)
Main: Grid Sieve 25mm Slot Width for EN Aggregate Flakiness Test. (42-0322)
Main: Grid Sieve 3.15mm Slot Width for EN Aggregate Flakiness Test. (42-0302)
Main: Grid Sieve 31.5mm Slot Width for EN Aggregate Flakiness Test. (42-0324)
Main: Grid Sieve 40mm Slot Width for EN Aggregate Flakiness Test. (42-0326)
Main: Grid Sieve 5mm Slot Width for EN Aggregate Flakiness Test. (42-0306)
Main: Grid Sieve 6.3mm Slot Width for EN Aggregate Flakiness Test. (42-0308)
Main: Grid Sieve 8mm Slot Width for EN Aggregate Flakiness Test. (42-0310)
Accessory: Sample Tray - 406 x 406 x 50 mm (81-4030)

[PRODUCT] Grid Sieve 5mm Slot Width for EN Aggregate Flakiness Test. (42-0306)
5mm

_Standards_
EN 933-3

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA** Passing Size - 10 mm Retained Size - 8 mm

_Attributes_
Slot width, mm
	5
	
Passing Size, mm
	10
	
Retained Size, mm
	8

_Related Products_
Accessory: 300mm Dia BS Sieve 10.0mm Perforated Plate. (79-2555)
Accessory: 300mm Dia BS Sieve 12.5mm Perforated Plate (79-2565)
Accessory: 300mm Dia BS Sieve 16.0mm Perforated Plate. (79-2580)
Accessory: 300mm Dia BS Sieve 20.0mm Perforated Plate. (79-2595)
Accessory: 300mm Dia BS Sieve 25.0mm Perforated Plate. (79-2605)
Accessory: 300mm Dia BS Sieve 31.5mm Perforated Plate. (79-2630)
Accessory: 300mm Dia BS Sieve 4.00mm Perforated Plate. (79-2500)
Accessory: 300mm Dia BS Sieve 40.0mm Perforated Plate (79-2645)
Accessory: 300mm Dia BS Sieve 5.00mm Perforated Plate. (79-2515)
Accessory: 300mm Dia BS Sieve 50.0mm Perforated Plate. (79-2655)
Accessory: 300mm Dia BS Sieve 6.30mm Perforated Plate. (79-2525)
Accessory: 300mm Dia BS Sieve 63.0mm Perforated Plate. (79-2670)
Accessory: 300mm Dia BS Sieve 8.00mm Perforated Plate. (79-2540)
Accessory: 300mm Dia BS Sieve 80mm Perforated Plate (79-2684)
Accessory: 300mm Dia Lid. (79-2010)
Accessory: 300mm Dia Receiver. (79-2020)
Main: Grid Sieve 10mm Slot Width for EN Aggregate Flakiness Test. (42-0314)
Main: Grid Sieve 12.5mm Slot Width for EN Aggregate Flakiness Test. (42-0316)
Main: Grid Sieve 16mm Slot Width for EN Aggregate Flakiness Test. (42-0318)
Main: Grid Sieve 2.5mm Slot Width for EN Aggregate Flakiness Test. (42-0300)
Main: Grid Sieve 20mm Slot Width for EN Aggregate Flakiness Test. (42-0320)
Main: Grid Sieve 25mm Slot Width for EN Aggregate Flakiness Test. (42-0322)
Main: Grid Sieve 3.15mm Slot Width for EN Aggregate Flakiness Test. (42-0302)
Main: Grid Sieve 31.5mm Slot Width for EN Aggregate Flakiness Test. (42-0324)
Main: Grid Sieve 40mm Slot Width for EN Aggregate Flakiness Test. (42-0326)
Main: Grid Sieve 4mm Slot Width for EN Aggregate Flakiness Test. (42-0304)
Main: Grid Sieve 6.3mm Slot Width for EN Aggregate Flakiness Test. (42-0308)
Main: Grid Sieve 8mm Slot Width for EN Aggregate Flakiness Test. (42-0310)
Accessory: Sample Tray - 406 x 406 x 50 mm (81-4030)

[PRODUCT] Grid Sieve 6.3mm Slot Width for EN Aggregate Flakiness Test. (42-0308)
6.3mm

_Standards_
EN 933-3

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA** Passing Size - 12.5 mm Retained Size - 10mm

_Attributes_
Slot width, mm
	6.3
	
Passing Size, mm
	12.5
	
Retained Size, mm
	10

_Related Products_
Accessory: 300mm Dia BS Sieve 10.0mm Perforated Plate. (79-2555)
Accessory: 300mm Dia BS Sieve 12.5mm Perforated Plate (79-2565)
Accessory: 300mm Dia BS Sieve 16.0mm Perforated Plate. (79-2580)
Accessory: 300mm Dia BS Sieve 20.0mm Perforated Plate. (79-2595)
Accessory: 300mm Dia BS Sieve 25.0mm Perforated Plate. (79-2605)
Accessory: 300mm Dia BS Sieve 31.5mm Perforated Plate. (79-2630)
Accessory: 300mm Dia BS Sieve 4.00mm Perforated Plate. (79-2500)
Accessory: 300mm Dia BS Sieve 40.0mm Perforated Plate (79-2645)
Accessory: 300mm Dia BS Sieve 5.00mm Perforated Plate. (79-2515)
Accessory: 300mm Dia BS Sieve 50.0mm Perforated Plate. (79-2655)
Accessory: 300mm Dia BS Sieve 6.30mm Perforated Plate. (79-2525)
Accessory: 300mm Dia BS Sieve 63.0mm Perforated Plate. (79-2670)
Accessory: 300mm Dia BS Sieve 8.00mm Perforated Plate. (79-2540)
Accessory: 300mm Dia BS Sieve 80mm Perforated Plate (79-2684)
Accessory: 300mm Dia Lid. (79-2010)
Accessory: 300mm Dia Receiver. (79-2020)
Main: Grid Sieve 10mm Slot Width for EN Aggregate Flakiness Test. (42-0314)
Main: Grid Sieve 12.5mm Slot Width for EN Aggregate Flakiness Test. (42-0316)
Main: Grid Sieve 16mm Slot Width for EN Aggregate Flakiness Test. (42-0318)
Main: Grid Sieve 2.5mm Slot Width for EN Aggregate Flakiness Test. (42-0300)
Main: Grid Sieve 20mm Slot Width for EN Aggregate Flakiness Test. (42-0320)
Main: Grid Sieve 25mm Slot Width for EN Aggregate Flakiness Test. (42-0322)
Main: Grid Sieve 3.15mm Slot Width for EN Aggregate Flakiness Test. (42-0302)
Main: Grid Sieve 31.5mm Slot Width for EN Aggregate Flakiness Test. (42-0324)
Main: Grid Sieve 40mm Slot Width for EN Aggregate Flakiness Test. (42-0326)
Main: Grid Sieve 4mm Slot Width for EN Aggregate Flakiness Test. (42-0304)
Main: Grid Sieve 5mm Slot Width for EN Aggregate Flakiness Test. (42-0306)
Main: Grid Sieve 8mm Slot Width for EN Aggregate Flakiness Test. (42-0310)
Accessory: Sample Tray - 406 x 406 x 50 mm (81-4030)

[PRODUCT] Grid Sieve 8mm Slot Width for EN Aggregate Flakiness Test. (42-0310)
8mm

_Standards_
EN 933-3

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA** Passing Size - 16 mm Retained Size - 12.5 mm

_Attributes_
Slot width, mm
	8
	
Passing Size, mm
	16
	
Retained Size, mm
	12.5

_Related Products_
Accessory: 300mm Dia BS Sieve 10.0mm Perforated Plate. (79-2555)
Accessory: 300mm Dia BS Sieve 12.5mm Perforated Plate (79-2565)
Accessory: 300mm Dia BS Sieve 16.0mm Perforated Plate. (79-2580)
Accessory: 300mm Dia BS Sieve 20.0mm Perforated Plate. (79-2595)
Accessory: 300mm Dia BS Sieve 25.0mm Perforated Plate. (79-2605)
Accessory: 300mm Dia BS Sieve 31.5mm Perforated Plate. (79-2630)
Accessory: 300mm Dia BS Sieve 4.00mm Perforated Plate. (79-2500)
Accessory: 300mm Dia BS Sieve 40.0mm Perforated Plate (79-2645)
Accessory: 300mm Dia BS Sieve 5.00mm Perforated Plate. (79-2515)
Accessory: 300mm Dia BS Sieve 50.0mm Perforated Plate. (79-2655)
Accessory: 300mm Dia BS Sieve 6.30mm Perforated Plate. (79-2525)
Accessory: 300mm Dia BS Sieve 63.0mm Perforated Plate. (79-2670)
Accessory: 300mm Dia BS Sieve 8.00mm Perforated Plate. (79-2540)
Accessory: 300mm Dia BS Sieve 80mm Perforated Plate (79-2684)
Accessory: 300mm Dia Lid. (79-2010)
Accessory: 300mm Dia Receiver. (79-2020)
Main: Grid Sieve 10mm Slot Width for EN Aggregate Flakiness Test. (42-0314)
Main: Grid Sieve 12.5mm Slot Width for EN Aggregate Flakiness Test. (42-0316)
Main: Grid Sieve 16mm Slot Width for EN Aggregate Flakiness Test. (42-0318)
Main: Grid Sieve 2.5mm Slot Width for EN Aggregate Flakiness Test. (42-0300)
Main: Grid Sieve 20mm Slot Width for EN Aggregate Flakiness Test. (42-0320)
Main: Grid Sieve 25mm Slot Width for EN Aggregate Flakiness Test. (42-0322)
Main: Grid Sieve 3.15mm Slot Width for EN Aggregate Flakiness Test. (42-0302)
Main: Grid Sieve 31.5mm Slot Width for EN Aggregate Flakiness Test. (42-0324)
Main: Grid Sieve 40mm Slot Width for EN Aggregate Flakiness Test. (42-0326)
Main: Grid Sieve 4mm Slot Width for EN Aggregate Flakiness Test. (42-0304)
Main: Grid Sieve 5mm Slot Width for EN Aggregate Flakiness Test. (42-0306)
Main: Grid Sieve 6.3mm Slot Width for EN Aggregate Flakiness Test. (42-0308)
Accessory: Sample Tray - 406 x 406 x 50 mm (81-4030)

[PRODUCT] Grid Sieve 10mm Slot Width for EN Aggregate Flakiness Test. (42-0314)
10mm

_Standards_
EN 933-3

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA** Passing Size - 20 mm Retained Size - 16 mm

_Attributes_
Slot width, mm
	10
	
Passing Size, mm
	20
	
Retained Size, mm
	16

_Related Products_
Accessory: 300mm Dia BS Sieve 10.0mm Perforated Plate. (79-2555)
Accessory: 300mm Dia BS Sieve 12.5mm Perforated Plate (79-2565)
Accessory: 300mm Dia BS Sieve 16.0mm Perforated Plate. (79-2580)
Accessory: 300mm Dia BS Sieve 20.0mm Perforated Plate. (79-2595)
Accessory: 300mm Dia BS Sieve 25.0mm Perforated Plate. (79-2605)
Accessory: 300mm Dia BS Sieve 31.5mm Perforated Plate. (79-2630)
Accessory: 300mm Dia BS Sieve 4.00mm Perforated Plate. (79-2500)
Accessory: 300mm Dia BS Sieve 40.0mm Perforated Plate (79-2645)
Accessory: 300mm Dia BS Sieve 5.00mm Perforated Plate. (79-2515)
Accessory: 300mm Dia BS Sieve 50.0mm Perforated Plate. (79-2655)
Accessory: 300mm Dia BS Sieve 6.30mm Perforated Plate. (79-2525)
Accessory: 300mm Dia BS Sieve 63.0mm Perforated Plate. (79-2670)
Accessory: 300mm Dia BS Sieve 8.00mm Perforated Plate. (79-2540)
Accessory: 300mm Dia BS Sieve 80mm Perforated Plate (79-2684)
Accessory: 300mm Dia Lid. (79-2010)
Accessory: 300mm Dia Receiver. (79-2020)
Main: Grid Sieve 12.5mm Slot Width for EN Aggregate Flakiness Test. (42-0316)
Main: Grid Sieve 16mm Slot Width for EN Aggregate Flakiness Test. (42-0318)
Main: Grid Sieve 2.5mm Slot Width for EN Aggregate Flakiness Test. (42-0300)
Main: Grid Sieve 20mm Slot Width for EN Aggregate Flakiness Test. (42-0320)
Main: Grid Sieve 25mm Slot Width for EN Aggregate Flakiness Test. (42-0322)
Main: Grid Sieve 3.15mm Slot Width for EN Aggregate Flakiness Test. (42-0302)
Main: Grid Sieve 31.5mm Slot Width for EN Aggregate Flakiness Test. (42-0324)
Main: Grid Sieve 40mm Slot Width for EN Aggregate Flakiness Test. (42-0326)
Main: Grid Sieve 4mm Slot Width for EN Aggregate Flakiness Test. (42-0304)
Main: Grid Sieve 5mm Slot Width for EN Aggregate Flakiness Test. (42-0306)
Main: Grid Sieve 6.3mm Slot Width for EN Aggregate Flakiness Test. (42-0308)
Main: Grid Sieve 8mm Slot Width for EN Aggregate Flakiness Test. (42-0310)
Accessory: Sample Tray - 406 x 406 x 50 mm (81-4030)

[PRODUCT] Grid Sieve 12.5mm Slot Width for EN Aggregate Flakiness Test. (42-0316)
12.5mm

_Standards_
EN 933-3

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA** Passing Size - 25 mm Retained Size - 20 mm

_Attributes_
Slot width, mm
	12.5
	
Passing Size, mm
	25
	
Retained Size, mm
	20

_Related Products_
Accessory: 300mm Dia BS Sieve 10.0mm Perforated Plate. (79-2555)
Accessory: 300mm Dia BS Sieve 12.5mm Perforated Plate (79-2565)
Accessory: 300mm Dia BS Sieve 16.0mm Perforated Plate. (79-2580)
Accessory: 300mm Dia BS Sieve 20.0mm Perforated Plate. (79-2595)
Accessory: 300mm Dia BS Sieve 25.0mm Perforated Plate. (79-2605)
Accessory: 300mm Dia BS Sieve 31.5mm Perforated Plate. (79-2630)
Accessory: 300mm Dia BS Sieve 4.00mm Perforated Plate. (79-2500)
Accessory: 300mm Dia BS Sieve 40.0mm Perforated Plate (79-2645)
Accessory: 300mm Dia BS Sieve 5.00mm Perforated Plate. (79-2515)
Accessory: 300mm Dia BS Sieve 50.0mm Perforated Plate. (79-2655)
Accessory: 300mm Dia BS Sieve 6.30mm Perforated Plate. (79-2525)
Accessory: 300mm Dia BS Sieve 63.0mm Perforated Plate. (79-2670)
Accessory: 300mm Dia BS Sieve 8.00mm Perforated Plate. (79-2540)
Accessory: 300mm Dia BS Sieve 80mm Perforated Plate (79-2684)
Accessory: 300mm Dia Lid. (79-2010)
Accessory: 300mm Dia Receiver. (79-2020)
Main: Grid Sieve 10mm Slot Width for EN Aggregate Flakiness Test. (42-0314)
Main: Grid Sieve 16mm Slot Width for EN Aggregate Flakiness Test. (42-0318)
Main: Grid Sieve 2.5mm Slot Width for EN Aggregate Flakiness Test. (42-0300)
Main: Grid Sieve 20mm Slot Width for EN Aggregate Flakiness Test. (42-0320)
Main: Grid Sieve 25mm Slot Width for EN Aggregate Flakiness Test. (42-0322)
Main: Grid Sieve 3.15mm Slot Width for EN Aggregate Flakiness Test. (42-0302)
Main: Grid Sieve 31.5mm Slot Width for EN Aggregate Flakiness Test. (42-0324)
Main: Grid Sieve 40mm Slot Width for EN Aggregate Flakiness Test. (42-0326)
Main: Grid Sieve 4mm Slot Width for EN Aggregate Flakiness Test. (42-0304)
Main: Grid Sieve 5mm Slot Width for EN Aggregate Flakiness Test. (42-0306)
Main: Grid Sieve 6.3mm Slot Width for EN Aggregate Flakiness Test. (42-0308)
Main: Grid Sieve 8mm Slot Width for EN Aggregate Flakiness Test. (42-0310)
Accessory: Sample Tray - 406 x 406 x 50 mm (81-4030)

[PRODUCT] Grid Sieve 16mm Slot Width for EN Aggregate Flakiness Test. (42-0318)
16mm

_Standards_
EN 933-3

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA** Passing Size - 31.5 mm Retained Size - 25 mm

_Attributes_
Slot width, mm
	16
	
Passing Size, mm
	31.5
	
Retained Size, mm
	25

_Related Products_
Accessory: 300mm Dia BS Sieve 10.0mm Perforated Plate. (79-2555)
Accessory: 300mm Dia BS Sieve 12.5mm Perforated Plate (79-2565)
Accessory: 300mm Dia BS Sieve 16.0mm Perforated Plate. (79-2580)
Accessory: 300mm Dia BS Sieve 20.0mm Perforated Plate. (79-2595)
Accessory: 300mm Dia BS Sieve 25.0mm Perforated Plate. (79-2605)
Accessory: 300mm Dia BS Sieve 31.5mm Perforated Plate. (79-2630)
Accessory: 300mm Dia BS Sieve 4.00mm Perforated Plate. (79-2500)
Accessory: 300mm Dia BS Sieve 40.0mm Perforated Plate (79-2645)
Accessory: 300mm Dia BS Sieve 5.00mm Perforated Plate. (79-2515)
Accessory: 300mm Dia BS Sieve 50.0mm Perforated Plate. (79-2655)
Accessory: 300mm Dia BS Sieve 6.30mm Perforated Plate. (79-2525)
Accessory: 300mm Dia BS Sieve 63.0mm Perforated Plate. (79-2670)
Accessory: 300mm Dia BS Sieve 8.00mm Perforated Plate. (79-2540)
Accessory: 300mm Dia BS Sieve 80mm Perforated Plate (79-2684)
Accessory: 300mm Dia Lid. (79-2010)
Accessory: 300mm Dia Receiver. (79-2020)
Main: Grid Sieve 10mm Slot Width for EN Aggregate Flakiness Test. (42-0314)
Main: Grid Sieve 12.5mm Slot Width for EN Aggregate Flakiness Test. (42-0316)
Main: Grid Sieve 2.5mm Slot Width for EN Aggregate Flakiness Test. (42-0300)
Main: Grid Sieve 20mm Slot Width for EN Aggregate Flakiness Test. (42-0320)
Main: Grid Sieve 25mm Slot Width for EN Aggregate Flakiness Test. (42-0322)
Main: Grid Sieve 3.15mm Slot Width for EN Aggregate Flakiness Test. (42-0302)
Main: Grid Sieve 31.5mm Slot Width for EN Aggregate Flakiness Test. (42-0324)
Main: Grid Sieve 40mm Slot Width for EN Aggregate Flakiness Test. (42-0326)
Main: Grid Sieve 4mm Slot Width for EN Aggregate Flakiness Test. (42-0304)
Main: Grid Sieve 5mm Slot Width for EN Aggregate Flakiness Test. (42-0306)
Main: Grid Sieve 6.3mm Slot Width for EN Aggregate Flakiness Test. (42-0308)
Main: Grid Sieve 8mm Slot Width for EN Aggregate Flakiness Test. (42-0310)
Accessory: Sample Tray - 406 x 406 x 50 mm (81-4030)

[PRODUCT] Grid Sieve 20mm Slot Width for EN Aggregate Flakiness Test. (42-0320)
20mm

_Standards_
EN 933-3

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA** Passing Size - 40 mm Retained Size - 31.5 mm

_Attributes_
Slot width, mm
	20
	
Passing Size, mm
	40
	
Retained Size, mm
	31.5

_Related Products_
Accessory: 300mm Dia BS Sieve 10.0mm Perforated Plate. (79-2555)
Accessory: 300mm Dia BS Sieve 12.5mm Perforated Plate (79-2565)
Accessory: 300mm Dia BS Sieve 16.0mm Perforated Plate. (79-2580)
Accessory: 300mm Dia BS Sieve 20.0mm Perforated Plate. (79-2595)
Accessory: 300mm Dia BS Sieve 25.0mm Perforated Plate. (79-2605)
Accessory: 300mm Dia BS Sieve 31.5mm Perforated Plate. (79-2630)
Accessory: 300mm Dia BS Sieve 4.00mm Perforated Plate. (79-2500)
Accessory: 300mm Dia BS Sieve 40.0mm Perforated Plate (79-2645)
Accessory: 300mm Dia BS Sieve 5.00mm Perforated Plate. (79-2515)
Accessory: 300mm Dia BS Sieve 50.0mm Perforated Plate. (79-2655)
Accessory: 300mm Dia BS Sieve 6.30mm Perforated Plate. (79-2525)
Accessory: 300mm Dia BS Sieve 63.0mm Perforated Plate. (79-2670)
Accessory: 300mm Dia BS Sieve 8.00mm Perforated Plate. (79-2540)
Accessory: 300mm Dia BS Sieve 80mm Perforated Plate (79-2684)
Accessory: 300mm Dia Lid. (79-2010)
Accessory: 300mm Dia Receiver. (79-2020)
Main: Grid Sieve 10mm Slot Width for EN Aggregate Flakiness Test. (42-0314)
Main: Grid Sieve 12.5mm Slot Width for EN Aggregate Flakiness Test. (42-0316)
Main: Grid Sieve 16mm Slot Width for EN Aggregate Flakiness Test. (42-0318)
Main: Grid Sieve 2.5mm Slot Width for EN Aggregate Flakiness Test. (42-0300)
Main: Grid Sieve 25mm Slot Width for EN Aggregate Flakiness Test. (42-0322)
Main: Grid Sieve 3.15mm Slot Width for EN Aggregate Flakiness Test. (42-0302)
Main: Grid Sieve 31.5mm Slot Width for EN Aggregate Flakiness Test. (42-0324)
Main: Grid Sieve 40mm Slot Width for EN Aggregate Flakiness Test. (42-0326)
Main: Grid Sieve 4mm Slot Width for EN Aggregate Flakiness Test. (42-0304)
Main: Grid Sieve 5mm Slot Width for EN Aggregate Flakiness Test. (42-0306)
Main: Grid Sieve 6.3mm Slot Width for EN Aggregate Flakiness Test. (42-0308)
Main: Grid Sieve 8mm Slot Width for EN Aggregate Flakiness Test. (42-0310)
Accessory: Sample Tray - 406 x 406 x 50 mm (81-4030)

[PRODUCT] Grid Sieve 25mm Slot Width for EN Aggregate Flakiness Test. (42-0322)
25mm

_Standards_
EN 933-3

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA** Passing Size - 50 mm Retained Size - 40 mm

_Attributes_
Slot width, mm
	25
	
Passing Size, mm
	50
	
Retained Size, mm
	40

_Related Products_
Accessory: 300mm Dia BS Sieve 10.0mm Perforated Plate. (79-2555)
Accessory: 300mm Dia BS Sieve 12.5mm Perforated Plate (79-2565)
Accessory: 300mm Dia BS Sieve 16.0mm Perforated Plate. (79-2580)
Accessory: 300mm Dia BS Sieve 20.0mm Perforated Plate. (79-2595)
Accessory: 300mm Dia BS Sieve 25.0mm Perforated Plate. (79-2605)
Accessory: 300mm Dia BS Sieve 31.5mm Perforated Plate. (79-2630)
Accessory: 300mm Dia BS Sieve 4.00mm Perforated Plate. (79-2500)
Accessory: 300mm Dia BS Sieve 40.0mm Perforated Plate (79-2645)
Accessory: 300mm Dia BS Sieve 5.00mm Perforated Plate. (79-2515)
Accessory: 300mm Dia BS Sieve 50.0mm Perforated Plate. (79-2655)
Accessory: 300mm Dia BS Sieve 6.30mm Perforated Plate. (79-2525)
Accessory: 300mm Dia BS Sieve 63.0mm Perforated Plate. (79-2670)
Accessory: 300mm Dia BS Sieve 8.00mm Perforated Plate. (79-2540)
Accessory: 300mm Dia BS Sieve 80mm Perforated Plate (79-2684)
Accessory: 300mm Dia Lid. (79-2010)
Accessory: 300mm Dia Receiver. (79-2020)
Main: Grid Sieve 10mm Slot Width for EN Aggregate Flakiness Test. (42-0314)
Main: Grid Sieve 12.5mm Slot Width for EN Aggregate Flakiness Test. (42-0316)
Main: Grid Sieve 16mm Slot Width for EN Aggregate Flakiness Test. (42-0318)
Main: Grid Sieve 2.5mm Slot Width for EN Aggregate Flakiness Test. (42-0300)
Main: Grid Sieve 20mm Slot Width for EN Aggregate Flakiness Test. (42-0320)
Main: Grid Sieve 3.15mm Slot Width for EN Aggregate Flakiness Test. (42-0302)
Main: Grid Sieve 31.5mm Slot Width for EN Aggregate Flakiness Test. (42-0324)
Main: Grid Sieve 40mm Slot Width for EN Aggregate Flakiness Test. (42-0326)
Main: Grid Sieve 4mm Slot Width for EN Aggregate Flakiness Test. (42-0304)
Main: Grid Sieve 5mm Slot Width for EN Aggregate Flakiness Test. (42-0306)
Main: Grid Sieve 6.3mm Slot Width for EN Aggregate Flakiness Test. (42-0308)
Main: Grid Sieve 8mm Slot Width for EN Aggregate Flakiness Test. (42-0310)
Accessory: Sample Tray - 406 x 406 x 50 mm (81-4030)

[PRODUCT] Grid Sieve 31.5mm Slot Width for EN Aggregate Flakiness Test. (42-0324)
31.5mm

_Standards_
EN 933-3

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA** Passing Size - 63 mm Retained Size - 50 mm

_Attributes_
Slot width, mm
	31.5
	
Passing Size, mm
	63
	
Retained Size, mm
	50

_Related Products_
Accessory: 300mm Dia BS Sieve 10.0mm Perforated Plate. (79-2555)
Accessory: 300mm Dia BS Sieve 12.5mm Perforated Plate (79-2565)
Accessory: 300mm Dia BS Sieve 16.0mm Perforated Plate. (79-2580)
Accessory: 300mm Dia BS Sieve 20.0mm Perforated Plate. (79-2595)
Accessory: 300mm Dia BS Sieve 25.0mm Perforated Plate. (79-2605)
Accessory: 300mm Dia BS Sieve 31.5mm Perforated Plate. (79-2630)
Accessory: 300mm Dia BS Sieve 4.00mm Perforated Plate. (79-2500)
Accessory: 300mm Dia BS Sieve 40.0mm Perforated Plate (79-2645)
Accessory: 300mm Dia BS Sieve 5.00mm Perforated Plate. (79-2515)
Accessory: 300mm Dia BS Sieve 50.0mm Perforated Plate. (79-2655)
Accessory: 300mm Dia BS Sieve 6.30mm Perforated Plate. (79-2525)
Accessory: 300mm Dia BS Sieve 63.0mm Perforated Plate. (79-2670)
Accessory: 300mm Dia BS Sieve 8.00mm Perforated Plate. (79-2540)
Accessory: 300mm Dia BS Sieve 80mm Perforated Plate (79-2684)
Accessory: 300mm Dia Lid. (79-2010)
Accessory: 300mm Dia Receiver. (79-2020)
Main: Grid Sieve 10mm Slot Width for EN Aggregate Flakiness Test. (42-0314)
Main: Grid Sieve 12.5mm Slot Width for EN Aggregate Flakiness Test. (42-0316)
Main: Grid Sieve 16mm Slot Width for EN Aggregate Flakiness Test. (42-0318)
Main: Grid Sieve 2.5mm Slot Width for EN Aggregate Flakiness Test. (42-0300)
Main: Grid Sieve 20mm Slot Width for EN Aggregate Flakiness Test. (42-0320)
Main: Grid Sieve 25mm Slot Width for EN Aggregate Flakiness Test. (42-0322)
Main: Grid Sieve 3.15mm Slot Width for EN Aggregate Flakiness Test. (42-0302)
Main: Grid Sieve 40mm Slot Width for EN Aggregate Flakiness Test. (42-0326)
Main: Grid Sieve 4mm Slot Width for EN Aggregate Flakiness Test. (42-0304)
Main: Grid Sieve 5mm Slot Width for EN Aggregate Flakiness Test. (42-0306)
Main: Grid Sieve 6.3mm Slot Width for EN Aggregate Flakiness Test. (42-0308)
Main: Grid Sieve 8mm Slot Width for EN Aggregate Flakiness Test. (42-0310)
Accessory: Sample Tray - 406 x 406 x 50 mm (81-4030)

[PRODUCT] Grid Sieve 40mm Slot Width for EN Aggregate Flakiness Test. (42-0326)
40mm

_Standards_
EN 933-3

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA** Passing Size - 80 mm Retained Size - 63 mm

_Attributes_
Slot width, mm
	40
	
Passing Size, mm
	80
	
Retained Size, mm
	63

_Related Products_
Accessory: 300mm Dia BS Sieve 10.0mm Perforated Plate. (79-2555)
Accessory: 300mm Dia BS Sieve 12.5mm Perforated Plate (79-2565)
Accessory: 300mm Dia BS Sieve 16.0mm Perforated Plate. (79-2580)
Accessory: 300mm Dia BS Sieve 20.0mm Perforated Plate. (79-2595)
Accessory: 300mm Dia BS Sieve 25.0mm Perforated Plate. (79-2605)
Accessory: 300mm Dia BS Sieve 31.5mm Perforated Plate. (79-2630)
Accessory: 300mm Dia BS Sieve 4.00mm Perforated Plate. (79-2500)
Accessory: 300mm Dia BS Sieve 40.0mm Perforated Plate (79-2645)
Accessory: 300mm Dia BS Sieve 5.00mm Perforated Plate. (79-2515)
Accessory: 300mm Dia BS Sieve 50.0mm Perforated Plate. (79-2655)
Accessory: 300mm Dia BS Sieve 6.30mm Perforated Plate. (79-2525)
Accessory: 300mm Dia BS Sieve 63.0mm Perforated Plate. (79-2670)
Accessory: 300mm Dia BS Sieve 8.00mm Perforated Plate. (79-2540)
Accessory: 300mm Dia BS Sieve 80mm Perforated Plate (79-2684)
Accessory: 300mm Dia Lid. (79-2010)
Accessory: 300mm Dia Receiver. (79-2020)
Main: Grid Sieve 10mm Slot Width for EN Aggregate Flakiness Test. (42-0314)
Main: Grid Sieve 12.5mm Slot Width for EN Aggregate Flakiness Test. (42-0316)
Main: Grid Sieve 16mm Slot Width for EN Aggregate Flakiness Test. (42-0318)
Main: Grid Sieve 2.5mm Slot Width for EN Aggregate Flakiness Test. (42-0300)
Main: Grid Sieve 20mm Slot Width for EN Aggregate Flakiness Test. (42-0320)
Main: Grid Sieve 25mm Slot Width for EN Aggregate Flakiness Test. (42-0322)
Main: Grid Sieve 3.15mm Slot Width for EN Aggregate Flakiness Test. (42-0302)
Main: Grid Sieve 31.5mm Slot Width for EN Aggregate Flakiness Test. (42-0324)
Main: Grid Sieve 4mm Slot Width for EN Aggregate Flakiness Test. (42-0304)
Main: Grid Sieve 5mm Slot Width for EN Aggregate Flakiness Test. (42-0306)
Main: Grid Sieve 6.3mm Slot Width for EN Aggregate Flakiness Test. (42-0308)
Main: Grid Sieve 8mm Slot Width for EN Aggregate Flakiness Test. (42-0310)
Accessory: Sample Tray - 406 x 406 x 50 mm (81-4030)

[GROUPED PRODUCT MATRIX]
Model No.
	Passing Size
	Retained Size
	Slot width, mm
	N/A for this Product Group

[CATEGORY] Density, Voids and Bulking
As with many porous material, the value obtained for the particle density of an aggregate will depend on the method of test and apparatus used. Different particle sizes within a sample often have different particle densities. The termparticle density expressed in Mg/m³ is numerically equal to the specific gravity. Various methods, depending upon the type and size of material to be tested, are specified in standards for testing aggregate.

[PRODUCT GROUP] Bulk Density Measures
Manufactured from heavy gauge steel these bulk density measures comply with the requirements of either BS 812 or ASTM C-29. Other than the 3 litre size, all measures incorporate carrying handles as standard.

[PRODUCT] Bulk Density Measure 3 Litre. (42-1995)
3 litre capacity

_Standards_
BS 812, ASTM C29

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Capacity, litres
	3

[PRODUCT] Bulk Density Measure 7 Litre (42-2000)
7 litre capacity

_Standards_
BS 812

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Capacity, litres
	7

[PRODUCT] Bulk Density Measure 30 Litre (34-2800)
Manufactured from heavy gauge steel these bulk density measures comply with the requirements of either BS 812, EN 1097-3, 12350-6 or ASTM C138. All measures incorporate carrying handles as standard.

_Standards_
BS 812, EN 1097-3, EN 12350-6, ASTM C138

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA** For other bulk density measures see the aggregates section

_Attributes_
Capacity, litres
	30

_Related Products_
Accessory: Compacting Bar 25mm Sq X 380mm (34-2910)
Accessory: Tamping Rod 16mm Dia X 600mm Long Hemispherical At Both Ends. (34-0130)

[PRODUCT] Bulk Density Measure 15 Litre (34-2820)
Manufactured from heavy gauge steel these bulk density measures comply with the requirements of either BS 812, EN 1097-3, 12350-6 or ASTM C138. All measures incorporate carrying handles as standard.

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA** For other bulk density measures see the aggregates section

_Attributes_
Capacity, litres
	15

[PRODUCT] Bulk Density Measure 10 Litre (34-2830)
Manufactured from heavy gauge steel these bulk density measures comply with the requirements of either BS 812, EN 1097-3, 12350-6 or ASTM C138. All measures incorporate carrying handles as standard.

_Standards_
EN 12350-6

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA** For other bulk density measures see the aggregates section

_Attributes_
Capacity, litres
	10

_Related Products_
Accessory: Aluminium Scoop Large (81-0220)
Accessory: Compacting Bar 25mm Sq X 380mm (34-2910)
Accessory: Float - Plasterer’s type (81-0340)
Accessory: Glass Plate. (24-0430)
Accessory: Sample Tray - 1200 x 1160 x 50 mm (81-4230)
Accessory: Shovel - With flat blade (81-0240)
Main: Soft Headed Mallet. (29-5020)
Accessory: Straight Edge 300mm. (24-9010)

[GROUPED PRODUCT MATRIX]
Model No.
	Capacity, litres
	N/A for this Product Group

[PRODUCT GROUP] Particle Density (specific gravity) and Water Absorption for Coarse Aggregates
Method for Aggregate between 63 mm and 5 mm

[PRODUCT] Buoyancy Balance 6Kg X 0.1G. Supplied with Support Frame Water Tank & Suspension Hook. (42-1000/01)
The buoyancy balance system developed by ELE consists of a rigid support frame, incorporating a water tank mounted on a platform. A mechanical lifting device is used to raise the water tank through the frame height immersing the specimen suspended below the balance. The balance supplied may also be used as a standard weighing device, thus providing a versatile and comprehensive weighing system in the laboratory.6000 g x 0.1 g supplied with frame, water tank and suspension hook.

_Standards_
EN 1097-6, EN 12697-6, BS 812, ASTM C127, AASHTO T85

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA** For 220 - 240 V AC, 50 - 60 Hz, 1 ph.

_Attributes_
Description
	Buoyancy Balance
	
Power Supply
	220 - 240 V AC, 50 - 60 Hz

_Related Products_
Accessory: 200 mm Diameter Lid (79-0010)
Accessory: 200 mm Diameter Receiver (79-0020)
Accessory: 200mm Dia BS Sieve 31.5mm Perforated Plate. (79-1630)
Accessory: 200mm Dia BS Sieve 4.00mm Stainless Steel Mesh. (79-0310)
Accessory: 200mm Dia BS Sieve 63 Mic Stainless Steel Mesh. (79-0070)
Accessory: 200mm Dia BS Sieve 63.0mm Perforated Plate. (79-1670)
Accessory: Digital Pocket Thermometer (82-5420)
Accessory: Sample Container - Tinned Steel 10 litres (81-3060)
Accessory: Sample Tray - 406 x 406 x 50 mm (81-4030)
Accessory: Timer Clock (81-0518)
Accessory: Wire Basket Brass with Handle Nominal 6000Cm³ Capacity with 1.7mm Wire Mesh. (42-1005)

[PRODUCT] Wire Basket Brass with Handle Nominal 6000Cm³ Capacity with 1.7mm Wire Mesh. (42-1005)
For BS 812 Relative Density. 200 mm diameter x 190 mm deep, 1.70 mm wire mesh.

_Standards_
EN 1097-6, EN 12697-6, BS 812, ASTM C127, AASHTO T85

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Wire Basket
	
Main body length, arm, operating length mm
	200 x 190

_Related Products_
Main: Buoyancy Balance 6Kg X 0.1G. Supplied with Support Frame Water Tank & Suspension Hook. (42-1000/01)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Particle Density (specific gravity) and Water Absorption for Fine Aggregates
Method for aggregate 20 mm and smaller The gas jar method described in BS 812 is suitable for all aggregates smaller than 20 mm in size and is particularly suited to friable aggregates. The pyknometer method described in ASTM C128 is suitable for determining the particle density of samples of fine aggregates. The particle density of fillers can be determined using the density bottle method specified for testing cement.

[PRODUCT] Sand Absorption Cone. (42-1700)
Made of brass to the dimensions given in BS 812, ASTM C128 and AASHTO T84.

_Standards_
BS 812, ASTM C128, AASHTO T84

_Attributes_
Description
	Sand Absorption Cone
	
Dimensions, diameter x height ”
	90 mm x 75 mm

_Related Products_
Accessory: 200mm Dia BS Sieve 75 Mic Stainless Steel Mesh. (79-0080)
Accessory: Funnel (82-2660)
Main: Pyknometer Complete with Non-Corrodable Cone and Rubber Seal 1Kg Capacity (24-2885)
Accessory: Sample Container - Plastic 10 litres (81-3540)
Accessory: Sample Container - Tinned Steel 10 litres (81-3060)
Accessory: Sample Tray - 305 mm Diameter x 50 mm (81-4700)
Main: Sand Absorption Cone and Tamper (42-1725)
Accessory: Tamping Rod. (42-1720)

[PRODUCT] Tamping Rod. (42-1720)
For use with cone. Tamping face is 25mm diameter and complies with BS 812, ASTM C128 and AASHTO T84.

_Standards_
BS 812, ASTM C128, AASHTO T84

_Attributes_
Description
	Tamping Rod
	
Dimensions, diameter x height ”
	25.4 mm x 168 mm

_Related Products_
Main: Sand Absorption Cone and Tamper (42-1725)
Main: Sand Absorption Cone. (42-1700)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[CATEGORY] Soundness and Chemical Tests
The presence of organic matter and certain chemicals can have a considerable influence on the strength and durability of concrete. The ability of aggregates to resist excessive changes in volume due to physical changees in the environment is also of importance. Knowledge of these potentially harmful factors will ensure that precautions can be taken at the mix design stage of a project.

[PRODUCT GROUP] Chloride Content: Rapid Method
Quantab chloride titrators can be used for estimating the chloride content of aqueous solutions. They are suitable for site testing and quality control of aggregates requiring less than 30 minutes to obtain a result.

[PRODUCT] Quantab Chloride Titrator Type 1175 Titration Range 0.005% - 0.1% 30-600ppm Nacl Pack of 40 Strips. (42-2950)
Type 1175 titration range 0.005% to 0.1% (30 to 600 ppm) NaCl. Pack of 50.

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Range ppm
	30 - 600
	
Weight, kg
	0.01

[PRODUCT] Quantab Chloride Titrator Strips Type 1176 Titration Range 0.05%-1% (300-6000 ppm) Nacl Pack of 40. (42-2952)
Type 1176 titration range 0.05% to 1% (300 to 6000 ppm) NaCl. Pack of 40.

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Range ppm
	300 - 6000
	
Weight, kg
	0.01

[GROUPED PRODUCT MATRIX]
Model No.
	Range
	N/A for this Product Group

[PRODUCT GROUP] Organic Impurities in Fine Aggregate
If aggregate contains organic impurities it may not be suitable for inclusion in concrete. Organic impurities, usually tannic acid and its derivatives, may interfere with the chemical reactions of hydration. Impurities are more likely to be found in fine (sand) aggregate.

[PRODUCT] Colour Standard to ASTM C40 (42-3040)
With five organic colour transparencies mounted in a holder.

_Standards_
ASTM C40, AASHTO T21

_Attributes_
Description
	Colour Standard
	
Colour Standards
	Five, on non-fading glass.

_Specification_
Color Standards
	Five, on non-fading glass.
	
Dimensions
	3â€ w. x 2-7/8â€ d. x 4â€ h. (76 x 73 x 102 mm).
	
Weight
	Net 4 oz. (113 g).

_Related Products_
Main: Round Graduated Bottle (42-3000A)
Spare/Consumable: Sodium Hydroxide Solution (42-3050)

[PRODUCT] Glass Bottle Approx.300Ml (42-3000)
12 ounce (300 ml approx) capacity, graduated at 2 , 4 and 7 ounce positions. Sodium Hydroxide pellets are required but not supplied by ELE.Complete with screw cap.

_Standards_
ASTM C40

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Glass Bottle
	
Weight, kg
	0.34

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Soundness of Aggregates
The soundness of aggregates to physical changes caused by the environment is important to the long-term durability characteristics of concrete. Excessive changes in volume can be caused by freezing and thawing, thermal changes at temperatures greater than freezing, and cycles of wetting and drying. Hydrometers and Wire Baskets see Laboratory Equipment Section.

[PRODUCT] Wire Basket - 150 μm wire mesh (81-4819)

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Wire Basket - 150 μm wire mesh
	
Aperture Size
	150 μm

[PRODUCT] Wire Basket - 600 μm wire mesh (81-4821)

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Wire Basket - 600 μm wire mesh
	
Aperture Size
	600 μm

[PRODUCT] Wire Basket - 1.18 mm wire mesh (81-4823)

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Wire Basket - 1.18 mm wire mesh
	
Aperture Size
	1.18 mm

[PRODUCT] Wire Basket - 3.35 mm wire mesh (81-4825)

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Wire Basket - 3.35 mm wire mesh
	
Aperture Size
	3.35 mm

[PRODUCT] Hydrometer (82-3505)
Type L50, ASTM C 88 graduated 1150 to 1200 relative density (used with sodium sulphate method).

_Standards_
BS 812, EN 1367-2, ASTM C88, AASHTO T104

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Hydrometer used with sodium sulphate method

[PRODUCT] Hydrometer (82-3510)
Type L50, ASTM C 88 graduated 1150 to 1200 relative density (used with magnesium sulphate method).

_Standards_
BS 812, EN 1367-2, ASTM C88, AASHTO T104

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Hydrometer used with magnesium sulphate method

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Sulphate Content: Rapid Method
A qualitative or semi-quantitative test is recommended for determining sulphate ions in aqueous solutions. Sulphate test strips are convenient measuring devices for preliminary assessment of sulphate content.

[PRODUCT] Sulphate Test Strips (42-2958)
Detection range 200 to 900 mg/l. Pack of 100.

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Sulphate Test Strips
	
Weight, kg
	0.01

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[CATEGORY] Mechanical Properties
The diverse range of aggregates available to the engineer makes it essential to select a material that is adequate for a given application. The following equipment is designed to determine various mechanical characteristics that need to be known in order to select the most suitable type of aggregate.

[PRODUCT GROUP] Aggregate Crushing Value (ACV) and Ten Percent Fines Value (TFV)
These tests are a measure of the crushing properties of aggregate and use the same basic equipment. The ACV test requires a standard load of 400 kN to be applied over a period of 10 minutes while the TFV test measures the force required to produce a specified depth of plunger penetration.

[PRODUCT] 150mm Aggregate Crushing Value Apparatus. Supplied Complete with Metal Measure and Tamping Rod. (42-4300)
Comprising of 150 mm nominal diameter steel cylinder, plunger and base plate supplied complete with metal measure and tamping rod.

_Standards_
BS 812-112

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	150 mm Aggregate Crushing Value Apparatus
	
Weight, kg
	16.6

_Related Products_
Main: 75mm Aggregate Crushing Value Apparatus. Supplied Complete with Metal Measure and Tamping Rod. (42-4500)
Accessory: Tamping Rod 16mm Dia X 600mm Long Hemispherical At Both Ends. (34-0130)

[PRODUCT] 75mm Aggregate Crushing Value Apparatus. Supplied Complete with Metal Measure and Tamping Rod. (42-4500)
Comprising of 75 mm nominal diameter steel cylinder, plunger and base plate supplied complete with metal measure and tamping rod.

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	75 mm Aggregate Crushing Value Apparatus
	
Weight, kg
	3.5

_Related Products_
Main: 150mm Aggregate Crushing Value Apparatus. Supplied Complete with Metal Measure and Tamping Rod. (42-4300)
Accessory: Tamping Rod 8mm Dia X 300mm. (42-4580)

[PRODUCT] Tamping Rod 8mm Dia X 300mm. (42-4580)
Spare: 8mm diameter x 300mm long with rounded end.

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Tamping Rod
	
Main body length, arm, operating length mm
	8 x 300

_Related Products_
Main: 75mm Aggregate Crushing Value Apparatus. Supplied Complete with Metal Measure and Tamping Rod. (42-4500)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Aggregate Impact Value (AIV)
The apparatus has been designed in a particularly heavy duty form, with specially hardened steel surfaces for minimum wear. The assembly is heavily plated to ensure corrosion resistance and forms a rigid frame around the quick-release trigger mechanism which ensures an effective free fall of the hammer when released. A built-in counter automatically indicates the number of blows delivered. The apparatus is supplied complete with cylindrical measure 75 mm diameter x 50 mm deep, and a steel tamping rod 16 mm diameter x 600 mm long.

[PRODUCT] Aggregate Impact Value Apparatus Complete with 16mm Dia X 600mm Long Rod (42-4000)
Heavy duty construction, heavily plated assembly ensures corrosion resistance.

_Standards_
BS 812-112

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Aggregate Impact Value Apparatus
	
Main body length, arm, operating length mm
	75 x 50, 16 x 600

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Los Angeles Abrasion Machine
* European and ASTM methods* Revolution counter* Safety cut-out* Full width coverThe Los Angeles Machine comprises a heavy steel cylinder, rotated about its horizontal axis. The cylinder incorporates a removable internal shelf, as specified in the ASTM and EN test methods. The steel cylinder is manufactured from structural steel plate conforming to S275 of EN 10025:1993.The filling aperture is provided with a cover and a safety stop button is prominently positioned. The machine is fitted with a revolution counter and steel tray for specimen unloading. Supplied without abrasive charges which should be ordered separately.

[PRODUCT] Set of 12 Abrasive Charges EN) (42-5305/10)
EN Set of 12.

_Standards_
EN 1097-2, ASTM C131, ASTM C535

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	12 EN Abrasive Charges

_Related Products_
Main: Los Angeles Abrasion Machine Meets ASTM and European Standards.  220-240V 50Hz 1Ph. (42-5305/01)
Main: Los Angeles Abrasion Machine with CE Safety Cabinet W/ Microswitches.  220-240V 50Hz 1Ph. (42-5310/01)

[PRODUCT] Los Angeles Abrasion Machine with CE Safety Cabinet W/ Microswitches.  220-240V 50Hz 1Ph. (42-5310/01)
The machine consists of a closed hollow cylindrical steel drum rotating around its horizontal axis on ball bearing units mounted on a sturdy base framework.The drum is driven at a speed of between 30 - 33 rpm via an enclosed belt drive arrangement from an electric motor/gearbox unit situated on the base frame. Inside the drum a full length steel shelf is attached, accessed by a dust-proof opening. The cylinder incorporates a removable internal shelf, one shelf position is provided to meet the requirements of both the ASTM and EN test standards. Controls are located easily on the right-hand side of the machine at convenient operator height. Start and stop push buttons and a subtracting revolution counter allows the user to preset the number of revolutions before an automatic stop.

_Standards_
EN 1097-2, ASTM C131, ASTM C535, NF P18-573

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Los Angeles Abrasion Machine with CE Safety Cabinet 220 - 240 V 50Hz
	
Power Supply
	220 - 240 V AC, 50 Hz, 1 ph

_Related Products_
Main: Los Angeles Abrasion Machine Meets ASTM and European Standards.  220-240V 50Hz 1Ph. (42-5305/01)
Accessory: Set of 12 Abrasive Charges (ASTM). (42-5300/10)
Accessory: Set of 12 Abrasive Charges EN) (42-5305/10)

[PRODUCT] Los Angeles Abrasion Machine Meets ASTM and European Standards.  220-240V 50Hz 1Ph. (42-5305/01)
The machine consists of a closed hollow cylindrical steel drum rotating around its horizontal axis on ball bearing units mounted on a sturdy base framework.The drum is driven at a speed of between 30 - 33 rpm via an enclosed belt drive arrangement from an electric motor/gearbox unit situated on the base frame. Inside the drum a full length steel shelf is attached, accessed by a dust-proof opening. The cylinder incorporates a removable internal shelf, one shelf position is provided to meet the requirements of both the ASTM and EN test standards. Controls are located easily on the right-hand side of the machine at convenient operator height. Start and stop push buttons and a subtracting revolution counter allows the user to preset the number of revolutions before an automatic stop.

_Standards_
EN 1097-2, ASTM C131, ASTM C535, AASHTO T96, NF P18-573

_Further Information_
Less charges. For 220 - 240 V AC, 50 Hz, 1ph.

_Attributes_
Description
	Los Angeles Abrasion Machine 220- 240 V AC 50Hz
	
Motor hp, amp
	1 HP

_Specification_
Capacity
	5,000 g each of aggregate and charge.
	
Drum Speed
	30-33 rpm.
	
Frame
	Welded structural steel.
	
Counter
	Adjustable; automatic shut-off; push-buttonreset and adjustment.
	
Controls
	Magnetic motor starter with overload protection and integral On-Off switches.
	
Dimensions
	38.6” w. x 36.2” d. x 38.6” h. (980 x 920 x 980 mm).
	
Weight
	Net 882 lbs. (400 kg).
	
Motor
	1 HP

_Related Products_
Main: Los Angeles Abrasion Machine with CE Safety Cabinet W/ Microswitches.  220-240V 50Hz 1Ph. (42-5310/01)
Accessory: Set of 12 Abrasive Charges (ASTM). (42-5300/10)
Accessory: Set of 12 Abrasive Charges EN) (42-5305/10)

[PRODUCT] Set of 12 Abrasive Charges (ASTM). (42-5300/10)
ASTM Set of 12.

_Standards_
EN 1097-2, ASTM C131, ASTM C535, AASHTO T96

_Attributes_
Description
	12 ASTM Abrasive Charges
	
Weight, lbs
	11.3

_Related Products_
Main: Los Angeles Abrasion Machine (42-5305/02)
Main: Los Angeles Abrasion Machine (42-5305/06)
Main: Los Angeles Abrasion Machine Meets ASTM and European Standards.  220-240V 50Hz 1Ph. (42-5305/01)
Main: Los Angeles Abrasion Machine with CE Safety Cabinet W/ Microswitches.  220-240V 50Hz 1Ph. (42-5310/01)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Skid Resistance Testing
The Pendulum Skid Resistance Tester was originally designed in the 40s in the USA, and further developed in the 1960s at the TRL (Transport Research Laboratory) for the testing of road surfaces. The device measures the frictional resistance between a rubber slider mounted on the end of a pendulum arm and the surface to be tested. This provides road engineers with a method of checking the resistance of wet and dry surfaces to slipping and skidding, both in the lab and insitu. It operates by a pendulum rotating about a spindle which is attached to a vertical pillar. At the end of the tubular arm a head of known mass is fitted with a rubber slider. The pendulum is released from a horizontal position so that it strikes the sample surface at a constant speed. The distance travelled by the head after hitting the sample is determined by the friction of the sample surface. 
http://localhost//cms-files/56d9/56d9b1ce806cc.jpg

[PRODUCT] Pendulum Skid Resistance Tester (42-6000)
The Pendulum Skid Resistance Tester was originally designed in the 1940s in the USA, and further developed in the 1960s at the TRL (Transport Research Laboratory) for the testing of road surfaces. The device measures the frictional resistance between a rubber slider mounted on the end of a pendulum arm and the surface to be tested. This provides road engineers with a method of checking the resistance of wet and dry surfaces to slipping and skidding, both in the lab and insitu. It operates by a pendulum rotating about a spindle which is attached to a vertical pillar. At the end of the tubular arm a head of known mass is fitted with a rubber slider. The pendulum is released from a horizontal position so that it strikes the sample surface at a constant speed. The distance travelled by the head after hitting the sample is determined by the friction of the sample surface. 

_Further Information_
Applications:  	* Assessment of surface friction and skid resistance properties  	* Testing of aggregates in the PSV (Polished Stone Value) test  	* Testing of new road surface materials 	* Testing of pedestrian pavements 	* RTA (road traffic accidents)  	* Litigation investigations Features:  	* Designed for lab and on site road surface testing  	* Factory calibrated to EN1097-8  	* Low friction arm, and lightweight pointer  	* Supplied with 'F' scale for use with small slider set for 76mm slide length (PSV test)  	* Highly repeatable 	* Supplied with carrying case 

_Attributes_
Description
	Pendulum Skid Resistance Tester

_Specification_
Dimensions (WxDxH)
	695 x 295 x 695 mm
	
Volume
	0.15m3
	
Weight
	30 kg

_Related Products_
Accessory: 1.25” Rubber Mounted PSV Slider for 42-6000 (42-6000/11)
Accessory: 3.00” Rubber Mounted CEN Slider for 42-6000 (42-6000/14)
Accessory: 3.00” Rubber Mounted Four S (96) Slider for 42-6000 (42-6000/13)
Accessory: 3.00” Rubber Mounted TRL (55) Slider for 42-6000 (42-6000/12)
Accessory: Base Plate for Skid Resistance Tester for lab testing (42-6200)
Accessory: First traceable calibration for 42-6000 (42-6000/15)
Accessory: Set of 3 Spreader Feet for Skid Resistance Tester for in-situ testing (42-6000/10)

[PRODUCT] Set of 3 Spreader Feet for Skid Resistance Tester for in-situ testing (42-6000/10)

_Attributes_
Description
	Set of 3 Spreader Feet for Skid Resistance Tester for in-situ testing

_Related Products_
Main: Pendulum Skid Resistance Tester (42-6000)

[PRODUCT] Base Plate for Skid Resistance Tester for lab testing (42-6200)

_Attributes_
Description
	Base Plate for Skid Resistance Tester for lab testing

_Related Products_
Main: Pendulum Skid Resistance Tester (42-6000)

[PRODUCT] 1.25” Rubber Mounted PSV Slider for 42-6000 (42-6000/11)
Slider for polished stones

_Attributes_
Description
	1.25” Rubber Mounted PSV Slider

_Related Products_
Main: Pendulum Skid Resistance Tester (42-6000)

[PRODUCT] 3.00” Rubber Mounted TRL (55) Slider for 42-6000 (42-6000/12)
Slider for car tyres on asphalt

_Attributes_
Description
	3.00” Rubber Mounted TRL (55) Slider 

_Related Products_
Main: Pendulum Skid Resistance Tester (42-6000)

[PRODUCT] 3.00” Rubber Mounted Four S (96) Slider for 42-6000 (42-6000/13)
Slider for shoes on surfaces

_Attributes_
Description
	3.00” Rubber Mounted Four S (96) Slider

_Related Products_
Main: Pendulum Skid Resistance Tester (42-6000)

[PRODUCT] 3.00” Rubber Mounted CEN Slider for 42-6000 (42-6000/14)

_Attributes_
Description
	3.00” Rubber Mounted CEN Slider

_Related Products_
Main: Pendulum Skid Resistance Tester (42-6000)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group