[DEPARTMENT] Asphalt

[CATEGORY] Analysis and Binder Recovery

[PRODUCT GROUP] Ignition Method
Ever-increasing concern over the harmful, environmental effects of solvent-based asphalt extraction methods has led many countries to support the elimination of their use. The new Asphalt Binder Analyser from ELE International provides for an environmentally-friendly and cost-effective solution for determining asphalt content.

[PRODUCT] Asphalt Binder Analyser 220-240V 50/60 Hz (46-6100/01)
Designed to measure the asphalt binder content of hot mix asphalt (HMA) using loss on ignition, in accordance with AASHTO T 308-10, ASTM D6307-10 and BSEN 12697-39:2012. 

_Further Information_
The integral microprocessor controlled weighing and calculation system is configurable to allow variations to the standard test method. Test result reports are available in both printed and software format. The high temperature afterburner minimises the production of noxious waste fumes. Supplied complete with 2 sets of sample baskets. Features:  	* Designed to measure asphalt binder content by loss on ignition 	* Avoids health, environmental and waste management issues 	* Avoids the expense associated with older solvent extraction methods 	* Reduced emissions due to high temperature afterburner 	* Controlled via a multi-lingual touchscreen interface 	* English, Spanish, French, Chinese, Italian and Russian language display 	* Other languages are available to order 	* Automatic calculation of final sample weight and binder % result 	* Adjustable aggregate correction factor 	* Average test times from 20 mins for 6 mm aggregates, to 45 mins for 40 mm aggregates 	* Permanent (dot-matrix) printed reports 	* USB data output compatible with most spread sheets 	* Easy naming, storage and recall of recipes that can be transferred between units 	* Simplified menu structure with secure 'Supervisor' and 'Operator' settings 	* Metal waste gas extraction pipe 	* Factory fitted thermocouple access port, if temperature calibration is to be carried out  	* Precise weight measurements, displayed to 0.1g resolution 	* Capacity for large sample sizes for more accurate results (max. sample is 4.5kg) 

_Attributes_
Description
	Asphalt Binder Analyser 220-240V 50/60 Hz

_Specification_
Max Temp (°C)
	750
	
Dimensions: Internal (HxWxD)
	220 x 450 x 350 mm
	
Dimensions: External (HxWxD)
	980 x 600 x 775 mm
	
Type
	Bench-top
	
Thermocouple type
	K
	
Max power (W)
	8000

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Asphalt Centrifuge Extractors
* Continuously variable speed control from 0 to 3,600 rpm (1500 g capacity model)* Brake control for rapid deceleration* Available in either 1500 g or 3000 g capacity modelsThe Centrifuge Extractor is used to determine the quantitative amount of bitumen in bituminous paving mixtures whilst providing high safety to the operator.* Continuously variable speed control from 0 to 3,600 rpm (1500 g capacity model)

[PRODUCT] Filter Discs Pack of 100 (45-3803)
248mm outer diameter with 44mm diameter hole.

_Standards_
EN 12697-1, ASTM D2172, AASHTO T164

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Filter Discs Pack of 100
	
Capacity, Grams
	1,500
	
Filter Discs
	100

_Related Products_
Main: Rotatest 1500 (45-3810/01)

[PRODUCT] Filter Discs Pack of 100 (45-3807)
295 mm internal diameter with a 44 mm diameter hole.

_Standards_
EN 12697-1, ASTM D2172, AASHTO T164

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Filter Discs Pack of 100
	
Capacity, Grams
	3,000
	
Filter Discs
	100

_Related Products_
Main: Rotatest 3000 (45-3815/01)

[PRODUCT] Rotatest 1500 (45-3810/01)
Centrifuge extractor used to determine the quantitative amount of bitumen in bituminous paving mixtures. Variable speed control from 0 to 3600 rpm through the front panel mounted control knob and brake control included for rapid deceleration. Precision machined aluminium removable cover with integral cup for adding solvent, with sealed cast aluminium housing. Centrifuge extractor used to determine the quantitative amount of bitumen in bituminous paving mixtures. Variable speed control from 0 to 3600 rpm through the front panel mounted control knob and brake control included for rapid deceleration. Precision machined aluminium removable cover with integral cup for adding solvent, with sealed cast aluminium housing.

_Standards_
EN 12697-1, ASTM D2172, AASHTO T164

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA** 1500 g capacity. Supplied with 100 Filter Discs. For 220 V AC, 50 - 60 Hz, 1ph.

_Attributes_
Description
	Rotatest
	
Capacity, Grams
	1,500

_Related Products_
Accessory: Bowl - 2.5 litre (81-5020)
Accessory: Dessicator - Non-vacuum (82-2100)
Accessory: Evaporating Dish - 100 x 40 mm (82-1970)
Accessory: Filter Discs Pack of 100 (45-3803)
Accessory: Hotplate (78-2950/01)
Accessory: Measuring Cylinder - Glass 100 ml (82-0380)
Accessory: Measuring Cylinder - Glass 1000 ml (82-0500)
Main: Muffle Furnace (83-4170/01)
Main: Rotatest 3000 (45-3815/01)
Accessory: Sample Tray - 306 x 306 x 38 mm (81-4020)
Accessory: Silica Gel (82-7091)
Accessory: Volumetric Flask - 100 ml (82-1000)
Accessory: Volumetric Flask - 1000 ml (82-1060)

[PRODUCT] Replacement bowl for Rotatest 1500 centrifuge extractor (45-3810/10)
Holds 1500 g

_Standards_
EN 12697-1, ASTM D2172, AASHTO T164

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Replacement bowl for Rotatest
	
Capacity, Grams
	1,500

[PRODUCT] Rotatest 3000 (45-3815/01)
Centrifuge extractor used to determine the quantitative amount of bitumen in bituminous paving mixtures. Variable speed control from 0 to 3600 rpm through the front panel mounted control knob and brake control included for rapid deceleration. Precision machined aluminium removable cover with integral cup for adding solvent, with sealed cast aluminium housing. For 220 V AC, 50 - 60 Hz, 1ph.

_Standards_
EN 12697-1, ASTM D2172, AASHTO T164

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA** 3000 g capacity. Supplied with 100 Filter Discs. For 220 V AC, 50 - 60 Hz, 1ph.

_Attributes_
Description
	Rotatest
	
Capacity, Grams
	3,000

_Related Products_
Accessory: Bowl - 2.5 litre (81-5020)
Accessory: Dessicator - Non-vacuum (82-2100)
Accessory: Evaporating Dish - 100 x 40 mm (82-1970)
Accessory: Filter Discs Pack of 100 (45-3807)
Accessory: Hotplate (78-2950/01)
Accessory: Measuring Cylinder - Glass 100 ml (82-0380)
Accessory: Measuring Cylinder - Glass 1000 ml (82-0500)
Main: Muffle Furnace (83-4170/01)
Main: Rotatest 1500 (45-3810/01)
Accessory: Sample Tray - 306 x 306 x 38 mm (81-4020)
Accessory: Silica Gel (82-7091)
Accessory: Volumetric Flask - 100 ml (82-1000)
Accessory: Volumetric Flask - 1000 ml (82-1060)

[PRODUCT] Replacement bowl for Rotatest 3000 centrifuge extractor (45-3815/10)
Holds 3000 g.

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Replacement bowl for Rotatest
	
Capacity, Grams
	3,000

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	Capacity, G
	N/A for this Product Group

[PRODUCT GROUP] Reflux Extraction

[PRODUCT] Reflux Extractor (4000 gram) (45-3855/01)
* 4000 gram capacity* Glass jar for visual observations* Thermostatically controlled hot plateThe 4000 gram capacity of the Reflux Extractor provides higher accuracy for acceptance testing procedures. This extractor has two cone type screens holding 2000 grams each. The unit consists of two cone screens, water condenser, pyrex reflux jar, a thermostatically controlled hot plate and a supply of filter paper.

_Standards_
ASTM D2172, AASHTO T164

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA** For 220 - 240 V AC, 50 - 60 Hz, 1ph.

_Attributes_
Description
	Reflux Extractor
	
Power Supply
	220 - 240 V AC, 50 - 60 Hz, 1 ph

_Related Products_
Accessory: Filter Paper (45-3857)

[PRODUCT] Filter Paper (45-3857)
Filter papers for 4000 gram capacity reflux extractor. Coarse-textured at grade 617 and 40 cm diameter.

_Standards_
ASTM D2172, AASHTO T164

_Further Information_
Pack of 50.

_Attributes_
Description
	Filter Paper
	
Filter Paper
	50

_Related Products_
Main: Reflux Extractor (4000 gram) (45-3855/01)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[CATEGORY] Bitumen and Tar

[PRODUCT GROUP] Asphalt and Bitumen Ovens
The ovens listed here are specifically designed for the testing of bitumen

[PRODUCT] Loss on Heat/Thin-Film Oven 220-240V 50/60 Hz (46-4100/01)
The Thin-Film Oven is used for determining the loss in mass of oil and asphaltic / bituminous compounds when heated with the loss on heating test method or the effect of heat and air on semisolid asphaltic / bituminous materials with the Thin-Film Oven (TFOT) method.

_Further Information_
Features:  	* Complies to the requirements of BS 2000, ASTM D6, D1754 & AASHTO T47, T179 	* The exterior is constructed from sheet steel finished in an easy clean powder-coated paint 	* Interior chamber is made from stainless steel 	* The unit is well insulated and has a double glass door for viewing the test chamber 	* The system is controlled by a microprocessor digital controller and overheat thermostat  	* Calibrated scale and tamper-proof lock 	* Temperature is controlled and pre-set at 163°C +/- 1°C 	* Two rotating platforms of 13.5 inches dia are supplied to perform both the testsSide mounted controls comprise:  	* Microprocessor digital control 	* Independent overheat thermostat 	* Mains switch 	* On/Off switch for the turntable motor 	* Indicator lamps 

_Attributes_
Description
	Loss on Heat/Thin-Film Oven 220-240V 50/60 Hz

_Specification_
Max Temp (°C)
	163
	
Dimensions: Internal (HxWxD)  
	380 x 520 x 460 mm
	
Dimensions: External (HxWxD)
	570 x 870 x 630 mm
	
Insulation
	Double wall
	
Internal material
	304 stainless steel
	
Turntable speed (rpm)
	5.5 
	
Max power (W)
	1500

[PRODUCT] Rolling Thin-Film Oven 220-240V 50/60 Hz (46-4150/01)
The Rolling Thin-Film Oven (RTFO) procedure provides simulated short term aged asphalt binder for physical property testing. Asphalt binder is exposed to elevated temperatures to simulate manufacturing and placement ageing. The RTFO also provides a quantitative measure of the volatiles lost during the ageing process. The exterior is constructed from sheet steel finished in an easy clean powder coated paint and the interior chamber is made from stainless steel. The control system comprises of a microprocessor digital controller and overheat thermostat with calibrated scale and tamper-proof lock.

_Further Information_
 	* Complies to the requirements of ASTM D2872 	* Internal dimensions (mm): 380 high x 480 wide x 440 deep 	* External dimensions (mm): 800 high x 710 wide x 660 deep (add 40mm for door handle) 	* Double wall construction with high density thermal insulation  	* Non-rusting grade 304 stainless steel interior 	* Easy clean powder painted steel exterior in light grey (RAL 7035) textured finish  	* Top mounted fan constructed with an air plenum as described in ASTM D2872  	* Fitted with a squirrel-type fan blade for better uniformity of air and temperature distribution 	* Equipped with air jet for blowing heating air into each bottle at its lowest point of travel 	* Base mounted elements 	* Vented to atmosphere 	* Single front opening, side hinged door with positive quarter turn latching mechanism  	* Double glazed window in door for viewing the test chamberTop mounted controls comprise:  	* Dual display microprocessor digital control 	* Independent overheat thermostat 	* Mains switch 	* Flow meter to control air flow 	* Indicator lamps 	* 1500 watts 	* Supplied with built-in 305mm diameter vertical circulator carriage for 8 sample containers  	* Glass samples rotate at 15 rpm ±0.2rpm (glass containers supplied separately) 	* Temperature is controlled and pre-set at 163°C ± 1°C

_Attributes_
Description
	Rolling Thin-Film Oven 220-240V 50/60 Hz

_Specification_
Max Temp (°C)
	163°C ± 1°C (preset)
	
Dimensions: Internal (HxWxD)
	380 x 480 x 440 mm
	
Dimensions: External (HxWxD)
	800 x 710 x 660 mm
	
Insulation
	Double wall
	
Internal material
	304 stainless steel
	
Max power (W)
	1500

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[CATEGORY] Sampling and Preparation

[PRODUCT GROUP] Hubbard-Carmick Specific Gravity Bottles

[PRODUCT] Hubbard-Carmick Specific Gravity Bottle (46-2190)
Conical type 25 ml.

_Standards_
ISO 3838, BS 4699, ASTM D70, AASHTO T228

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Specific gravity bottle type
	Hubbard-Carmick Specific Gravity Bottle
	
Capacity, ml
	25

[PRODUCT] Hubbard-Carmick Specific Gravity Bottle (46-2191)
Cylindrical type 24 ml.

_Standards_
ISO 3838, BS 4699, ASTM D70, AASHTO T228

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Specific gravity bottle type
	Hubbard-Carmick Specific Gravity Bottle
	
Capacity, ml
	24

[GROUPED PRODUCT MATRIX]
Model No.
	Bottle type
	Capacity, ml
	N/A for this Product Group

[CATEGORY] Flash and Fire Point
There are a number of test methods using different equipment with closed or open cups. The Cleveland Flash Cup Apparatus is used to test cutback bitumen and may sometimes also be used to test penetration grade bitumen. The apparatus utilises the open cup test method. Note that results from different methods cannot be correlated.

[PRODUCT GROUP] Cleveland Flash Cup Apparatus

[PRODUCT] Cleveland Flash Cup Apparatus (46-3310/01)
The ELE Semi-Automatic Cleveland Open Cup flashpoint Tester is equipped with an electrically heated cup (with a variable control to set temperature rise rate), a button operated and electrically driven sweep arm and a test flame for use on natural gas. Bench mounted, the unit is incorporated in an easy to clean stainless steel case.

_Standards_
BS 2000-36, EN ISO 2592, ASTM D92, IP 36

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA** For 220 - 240 V AC, 50 - 60 Hz, 1 ph.

_Attributes_
Description
	Cleveland Flash Cup Apparatus
	
Size (height x width x diameter) cm
	33 x 31 x 29

_Specification_
Temperature Range
	Ambient to 400°C
	
Power
	500 W maximum
	
Ramp rate
	Variable, manually controlled
	
Voltage
	220/240 V, 50/60 Hz
	
Size (HxWxD)
	33 x 31 x 29 cm
	
Weight
	6.5 kg

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[CATEGORY] Softening Point
The test is performed in duplicate under closely controlled conditions. Water is used as the bath medium for binders with softening points below 80ºC. Above this temperature glycerol is used in place of water. The softening point is a fundamental property of binders other than cutbacks and emulsions. The test is often referred to as the Ring and Ball test.

[PRODUCT GROUP] Penetration Test

[PRODUCT] Penetration Needle (46-5340/C)
Hardened steel, supplied with an UKAS verification certificate. For testing to BS 2000-49 and ASTM D5. (Pack contains 1 needle only).

_Standards_
BS 2000-49, EN 1426, EN 13179-2, ASTM D5, AASHTO T49, IP 49

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Penetration Needle - NPL verified
	
Weight, kg
	0.0025

_Related Products_
Main: Semi-Automatic Penetrometer (46-5295/01)

[PRODUCT] Constant Temperature Bath 21 - 56ºC (46-5500/01)
A bench mounting bath specially designed for the conditioning of bitumen samples prior to penetration tests. Incorporating a highly accurate thermostat, the bath maintains a temperature between 21 and 56ºC ± 0.1ºC (at ambient). An integral cover and deep tray for penetration testing are supplied as standard.

_Standards_
BS 2000-49, EN 1426, EN 13179-2, ASTM D5, AASHTO T49, IP 49

_Further Information_
**Not available for sale in the USA**

_Attributes_
Description
	Constant Temperature Bath

_Related Products_
Main: Semi-Automatic Penetrometer (46-5295/01)
Main: Standard Penetrometer (46-5290)

[PRODUCT] Standard Penetrometer (46-5290)
Penetration readings are quickly taken using this simple to operate apparatus. The 150 mm diameter dial is graduated in 400 divisions of 0.1 mm. Supplied without needles and penetration tins.

_Standards_
BS 2000-49, EN 1426, EN 13179-2, IP 49, ASTM D5, AASHTO T49

_Further Information_
Model shown with sample container; not included, order separately.

_Attributes_
Description
	Standard Penetrometer

_Specification_
Dial Indicator
	6” (150 mm) diam.; 400 mm x 0.1 mm.
	
Plunger Weight
	47.5 g.
	
Needle
	ASTM Style (non-certified); one included.
	
Plunger Release
	Manual mechanism.
	
Weight
	Net 18 lbs. (8.2 kg).

_Related Products_
Accessory: ASTM (NIST Certified) Penetration Needle (46-5297)
Spare/Consumable: ASTM (Non-Certified) Penetration Needle (46-5290/10)
Accessory: Constant Temperature Bath 21 - 56ºC (46-5500/01)
Accessory: Penetration Needle (46-5360/10)
Accessory: Penetration Tin (46-5861)
Accessory: Penetration Tin (46-5860)
Accessory: Timer Clock (81-0518)
Accessory: Transfer Dish (46-5800)

[PRODUCT] Semi-Automatic Penetrometer (46-5295/01)
As 46-5290 but incorporates Digital Automatic Controller which releases the needle assembly. The time set is displayed by a bright, easy to read display.

_Standards_
BS 2000-49, EN 1426, EN 13179-2, ASTM D5, AASHTO T49, IP 49

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Semi-Automatic Penetrometer
	
Power Supply
	220 - 240 V AC, 50 - 60 Hz, 1ph

_Related Products_
Accessory: Constant Temperature Bath 21 - 56ºC (46-5500/01)
Accessory: Penetration Needle (46-5340/C)
Accessory: Penetration Needle (46-5360/10)
Accessory: Penetration Tin (46-5861)
Accessory: Transfer Dish (46-5800)

[PRODUCT] Penetration Needle (46-5360/10)
Hardened steel.

_Standards_
BS 2000-49, EN 1426, EN 13179-2, ASTM D5, AASHTO T49, IP 49

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Penetration Needle

_Related Products_
Main: Semi-Automatic Penetrometer (46-5295/01)
Main: Standard Penetrometer (46-5290)

[PRODUCT] Transfer Dish (46-5800)
For use with ELE Penetrometer 46-5295.

_Standards_
BS 2000-49, EN 1426, EN 13179-2, ASTM D5, AASHTO T49, IP 49

_Attributes_
Description
	Transfer Dish

_Related Products_
Main: Semi-Automatic Penetrometer (46-5295/01)
Main: Standard Penetrometer (46-5290)

[PRODUCT] Penetration Tin (46-5860)
For penetrations between 200 and 350, approximately 70 mm diameter x 45 mm deep.

_Standards_
BS 2000-49, EN 1426, EN 13179-2, ASTM D5, AASHTO T49, IP 49

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Penetration Tin for 200 to 350 mm depths
	
Weight, kg
	0.03

_Related Products_
Main: Standard Penetrometer (46-5290)

[PRODUCT] Penetration Tin (46-5861)
For penetrations below 200, approximately 55 mm diameter x 35 mm deep.

_Standards_
BS 2000-49, EN 1426, EN 13179-2, ASTM D5, AASHTO T49, IP 49

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Penetration Tin for less than 200 mm depths
	
Weight, kg
	0.025

_Related Products_
Main: Semi-Automatic Penetrometer (46-5295/01)
Main: Standard Penetrometer (46-5290)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Ring and Ball Apparatus

[PRODUCT] BS/EN Ring and Ball Apparatus (46-4605)
With 2 shouldered pattern rings, 2 ball-centring guides and 2 balls. The apparatus has a support frame and is retained in a heat resistant container.

_Standards_
EN 1427, BS 2000-58

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	BS/EN Ring and Ball Apparatus
	
Weight, kg
	0.56

_Related Products_
Accessory: Magnetic Stirrer (46-4825/01)
Accessory: Thermometer (82-5272)
Accessory: Thermometer (82-5274)

[PRODUCT] Magnetic Stirrer (46-4825/01)
Utilises a rotating magnetic field to induce variable speed stirring action. A built-in regulating transformer provides fine temperature control of liquid up to a maximum temperature of +150°C. The unit is suitable for use with the Ring and Ball Apparatus.

_Standards_
EN 1427, BS 2000-58

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Magnetic Stirrer
	
Power Supply
	220 - 240 V AC, 50 - 60 Hz, 1 ph

_Related Products_
Main: BS/EN Ring and Ball Apparatus (46-4605)

[PRODUCT] Thermometer (82-5272)
Mercury-free with a range of -10.0°C to + 210.0°C and graduated every 1°C. Immersion up to 76 mm

_Standards_
EN 1427, BS 2000-58

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Thermometer - 76 mm immersion
	
Temperature Range °C
	-10 to +210

_Related Products_
Main: BS/EN Ring and Ball Apparatus (46-4605)

[PRODUCT] Thermometer (82-5274)
Mercury-free with a range of -10.0°C to + 210.0°C and graduated every 1°C. Total immersion possible.

_Standards_
EN 1427, BS 2000-58

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Temperature Range °C
	-10 to +210
	
Description
	Thermometer - Total Immersion

_Related Products_
Main: BS/EN Ring and Ball Apparatus (46-4605)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[CATEGORY] Gyratory Compaction
One of the best methods of laboratory compaction is considered to be Gyratory for not only the material's assessment of compactibility, but also the production of test samples. The method achieves this by the application of a vertical stress, typically 600 kPa via platens to a mass of asphaltic mixture inside a 100 or 150mm diameter mould. Whilst platens are kept parallel and horizontal, the longitudinal axis of the mould is gyrated at a fixed angle to the vertical axis. During the test process, the height of the specimen is measured automatically and the mixture density andvoid content are calculated. Compaction data is displayed in real time (graphical and tabular) and is available for download to MS Excel(tm) The operator has the ability to choose whether to compact for a certain number of gyrations or until a target mixture density or void content is achieved.  

[PRODUCT GROUP] Gyratory Compaction
Applications: * Compaction of asphaltic paving material to a target mixture density or void content * Assessment of mixture compactibility * SHRP Superpave asphalt mixture design * Preparation of cylindrical test specimens
http://localhost//resources/images/no-image.png

[PRODUCT] Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 220-240V 50Hz (45-6750/01)
One of the best methods of laboratory compaction is considered to be Gyratory for not only the material's assessment of compactibility, but also the production of test samples. The method achieves this by the application of a vertical stress, typically 600 kPa via platens to a mass of asphaltic mixture inside a 100 or 150mm diameter mould. Whilst platens are kept parallel and horizontal, the longitudinal axis of the mould is gyrated at a fixed angle to the vertical axis. During the test process, the height of the specimen is measured automatically and the mixture density and void content are calculated. Compaction data is displayed in real time (graphical and tabular) and is available for download to MS Excel(tm) The operator has the ability to choose whether to compact for a certain number of gyrations or until a target mixture density or void content is achieved.

_Further Information_
Features:  	* Full compliance to EN 12697 part 10 and 31 	* Configurable to comply with SHRP Superpave  	* Both 150mm and 100mm moulds can be tested without any modification 	* Automatic mould insertion and retraction 	* Cold mix (emulsion) materials can be compacted, with fluid collection facility 	* Data acquisition and control via host desktop PC 	* Export compaction data to MS Excel(tm) 	* UKAS traceable factory calibration 	* Can accept moulds up to 300mm in heightProduct Specification:  	* High stability steel frame with low flex and distortion 	* A 95mm pneumatic cylinder 	* Safety gates with interlock 	* Specimen table 	* Accurate stress control via high precision regulator 	* High quality inverter for accurate speed control 	* Specimen height measurement via linear potentiometer 	* Highly durable wheels for ease of movement 	* 16bit control and data acquisition 	* PC includedSoftware:  	* User-friendly, intuitive and reliable Windows(tm) software 	* 2 methods of compaction - no. of gyrations and target density 	* User guided step-by-step through compaction 	* Real-time display of current height, density and void content 	* Software communicates with the gyratory compactor via USB interface 	* Utilities are included for transducer check, diagnostic routines and calibration

_Attributes_
Description
	Gyratory Compactor
	
Voltage Supply
	220-240 V 50 Hz

_Specification_
Stress
	600 kPa nominal, 1000 kPa Max
	
Mixture types
	Wet and Dry
	
Machine speed
	30 rpm 
	
Angle of gyration
	0.2 to >2°
	
Electrical supply
	220-240 V 50Hz (16 amp)
	
Sample sizes
	100 and 150 mm dia
	
Compressed air supply
	7-10 bar, 350 L p/m
	
Dimensions (WxHxL)
	790 x 995 x 1920

_Related Products_
Accessory: 100mm Dia mould & platens (45-6750/10)
Accessory: 100mm Dia mould & platens inc. specimen temperature measurement (45-6750/23)
Accessory: 100mm Dia mould & platens, slotted for emulsion mix (45-6750/20)
Accessory: 100mm Dia split mould (45-6750/27)
Accessory: 100mm filter papers (pack of 100) (45-6750/24)
Accessory: 150 mm filter papers (pack of 100) (45-6750/22)
Accessory: 150mm Dia  mould & platens inc. specimen temperature measurement (45-6750/21)
Accessory: 150mm Dia mould & platens (45-6750/12)
Accessory: 150mm Dia mould & platens, slotted for emulsion mix (45-6750/15)
Accessory: 2 deg. angle plate (45-6750/17)
Accessory: Calibration kit for internal angle lead (45-6750/11)
Accessory: Display, Shear Force (45-6750/18)
Accessory: Internal angle measuring device (45-6750/13)
Accessory: Internal angle measuring device inc. asphalt Hot Mix Simulator (HMS – Hot Mix Simulator) (45-6750/14)
Accessory: Option for 300mm mould height (cannot be retro-fitted) (45-6750/16)
Accessory: Small air compressor for 45-6750 (45-6750/28)
Accessory: Spacer 100mm to compact 63mm height on 45-6750 (45-6750/25)
Accessory: Spacer 150mm to compact 63mm height on 45-6750 (45-6750/26)
Accessory: Specimen Extruder (45-6710)
Accessory: Specimen Temperature Measurement (45-6750/19)

[PRODUCT] Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 220-240V 60Hz (45-6750/06)
One of the best methods of laboratory compaction is considered to be Gyratory for not only the material's assessment of compactibility, but also the production of test samples. The method achieves this by the application of a vertical stress, typically 600 kPa via platens to a mass of asphaltic mixture inside a 100 or 150mm diameter mould. Whilst platens are kept parallel and horizontal, the longitudinal axis of the mould is gyrated at a fixed angle to the vertical axis. During the test process, the height of the specimen is measured automatically and the mixture density and void content are calculated. Compaction data is displayed in real time (graphical and tabular) and is available for download to MS Excel(tm) The operator has the ability to choose whether to compact for a certain number of gyrations or until a target mixture density or void content is achieved.

_Further Information_
Features:  	* Full compliance to EN 12697 part 10 and 31 	* Configurable to comply with SHRP Superpave  	* Both 150mm and 100mm moulds can be tested without any modification 	* Automatic mould insertion and retraction 	* Cold mix (emulsion) materials can be compacted, with fluid collection facility 	* Data acquisition and control via host desktop PC 	* Export compaction data to MS Excel(tm) 	* UKAS traceable factory calibration 	* Can accept moulds up to 300mm in heightProduct Specification:  	* High stability steel frame with low flex and distortion 	* A 95mm pneumatic cylinder 	* Safety gates with interlock 	* Specimen table 	* Accurate stress control via high precision regulator 	* High quality inverter for accurate speed control 	* Specimen height measurement via linear potentiometer 	* Highly durable wheels for ease of movement 	* 16bit control and data acquisition 	* PC includedSoftware:  	* User-friendly, intuitive and reliable Windows(tm) software 	* 2 methods of compaction - no. of gyrations and target density 	* User guided step-by-step through compaction 	* Real-time display of current height, density and void content 	* Software communicates with the gyratory compactor via USB interface 	* Utilities are included for transducer check, diagnostic routinesand calibration

_Attributes_
Description
	Gyratory Compactor
	
Voltage Supply
	220-240 V 60 Hz

_Specification_
Stress
	600 kPa nominal, 1000 kPa Max
	
Mixture types
	Wet and Dry
	
Machine speed
	30 rpm 
	
Angle of gyration
	0.2 to >2°
	
Electrical supply
	220-240 V 60Hz (16 amp)
	
Sample Sizes
	100 and 150 mm dia
	
Compressed air supply
	7-10 bar, 350 L p/m
	
Dimensions (WxHxL)
	790 x 995 x 1920

_Related Products_
Accessory: 100mm Dia mould & platens (45-6750/10)
Accessory: 100mm Dia mould & platens inc. specimen temperature measurement (45-6750/23)
Accessory: 100mm Dia mould & platens, slotted for emulsion mix (45-6750/20)
Accessory: 100mm Dia split mould (45-6750/27)
Accessory: 100mm filter papers (pack of 100) (45-6750/24)
Accessory: 150 mm filter papers (pack of 100) (45-6750/22)
Accessory: 150mm Dia  mould & platens inc. specimen temperature measurement (45-6750/21)
Accessory: 150mm Dia mould & platens (45-6750/12)
Accessory: 150mm Dia mould & platens, slotted for emulsion mix (45-6750/15)
Accessory: 2 deg. angle plate (45-6750/17)
Accessory: Calibration kit for internal angle lead (45-6750/11)
Accessory: Display, Shear Force (45-6750/18)
Accessory: Internal angle measuring device (45-6750/13)
Accessory: Internal angle measuring device inc. asphalt Hot Mix Simulator (HMS – Hot Mix Simulator) (45-6750/14)
Accessory: Option for 300mm mould height (cannot be retro-fitted) (45-6750/16)
Accessory: Spacer 100mm to compact 63mm height on 45-6750 (45-6750/25)
Accessory: Spacer 150mm to compact 63mm height on 45-6750 (45-6750/26)
Accessory: Specimen Extruder (45-6710)
Accessory: Specimen Temperature Measurement (45-6750/19)

[PRODUCT] Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 110-120V 60Hz (45-6750/02)
One of the best methods of laboratory compaction is considered to be Gyratory for not only the material's assessment of compactibility, but also the production of test samples. The method achieves this by the application of a vertical stress, typically 600 kPa via platens to a mass of asphaltic mixture inside a 100 or 150mm diameter mould. Whilst platens are kept parallel and horizontal, the longitudinal axis of the mould is gyrated at a fixed angle to the vertical axis. During the test process, the height of the specimen is measured automatically and the mixture density and void content are calculated. Compaction data is displayed in real time (graphical and tabular) and is available for download to MS Excel(tm) The operator has the ability to choose whether to compact for a certain number of gyrations or until a target mixture density or void content is achieved.

_Further Information_
Features:  	* Full compliance to EN 12697 part 10 and 31 	* Configurable to comply with SHRP Superpave  	* Both 150mm and 100mm moulds can be tested without any modification 	* Automatic mould insertion and retraction 	* Cold mix (emulsion) materials can be compacted, with fluid collection facility 	* Data acquisition and control via host desktop PC 	* Export compaction data to MS Excel(tm) 	* UKAS traceable factory calibration 	* Can accept moulds up to 300mm in heightProduct Specification:  	* High stability steel frame with low flex and distortion 	* A 95mm pneumatic cylinder 	* Safety gates with interlock 	* Specimen table 	* Accurate stress control via high precision regulator 	* High quality inverter for accurate speed control 	* Specimen height measurement via linear potentiometer 	* Highly durable wheels for ease of movement 	* 16bit control and data acquisition 	* PC includedSoftware:  	* User-friendly, intuitive and reliable Windows(tm) software 	* 2 methods of compaction - no. of gyrations and target density 	* User guided step-by-step through compaction 	* Real-time display of current height, density and void content 	* Software communicates with the gyratory compactor via USB interface 	* Utilities are included for transducer check, diagnostic routines and calibration

_Attributes_
Description
	Gyratory Compactor
	
Voltage Supply
	110-120 V 60 Hz

_Specification_
Stress
	600 kPa nominal, 1000 kPa Max
	
Mixture types
	Wet and Dry
	
Machine speed
	30 rpm 
	
Angle of gyration
	0.2 to >2°
	
Electrical supply
	110-120 V 60Hz 
	
Sample sizes
	100 and 150 mm dia
	
Compressed air supply
	7-10 bar, 350 L p/m
	
Dimensions (WxHxL)
	790 x 995 x 1920

_Related Products_
Accessory: 100mm Dia mould & platens (45-6750/10)
Accessory: 100mm Dia mould & platens inc. specimen temperature measurement (45-6750/23)
Accessory: 100mm Dia mould & platens, slotted for emulsion mix (45-6750/20)
Accessory: 100mm Dia split mould (45-6750/27)
Accessory: 100mm filter papers (pack of 100) (45-6750/24)
Accessory: 150 mm filter papers (pack of 100) (45-6750/22)
Accessory: 150mm Dia  mould & platens inc. specimen temperature measurement (45-6750/21)
Accessory: 150mm Dia mould & platens (45-6750/12)
Accessory: 150mm Dia mould & platens, slotted for emulsion mix (45-6750/15)
Accessory: 2 deg. angle plate (45-6750/17)
Accessory: Calibration kit for internal angle lead (45-6750/11)
Accessory: Display, Shear Force (45-6750/18)
Accessory: Internal angle measuring device (45-6750/13)
Accessory: Internal angle measuring device inc. asphalt Hot Mix Simulator (HMS – Hot Mix Simulator) (45-6750/14)
Accessory: Option for 300mm mould height (cannot be retro-fitted) (45-6750/16)
Accessory: Spacer 100mm to compact 63mm height on 45-6750 (45-6750/25)
Accessory: Spacer 150mm to compact 63mm height on 45-6750 (45-6750/26)
Accessory: Specimen Extruder (45-6710)
Accessory: Specimen Temperature Measurement (45-6750/19)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	Voltage
	N/A for this Product Group

[PRODUCT GROUP] Moulds for Gyratory Compactors
Used for preparation of compaction tests
http://localhost//cms-files/56d9/56d991370d8be.jpg

[PRODUCT] 100mm Dia mould & platens (45-6750/10)
34 x 18.5 x 18.5 cms 

_Attributes_
Description
	Mould & platens
	
Sample diameter
	100 mm

_Related Products_
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 110-120V 60Hz (45-6750/02)
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 220-240V 50Hz (45-6750/01)
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 220-240V 60Hz (45-6750/06)

[PRODUCT] 100mm Dia mould & platens, slotted for emulsion mix (45-6750/20)
34 x 18.5 x 18.5 cms 

_Attributes_
Description
	Mould & platens slotted for emulsion mix
	
Sample diameter
	100 mm

_Related Products_
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 110-120V 60Hz (45-6750/02)
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 220-240V 50Hz (45-6750/01)
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 220-240V 60Hz (45-6750/06)

[PRODUCT] 100mm filter papers (pack of 100) (45-6750/24)
100 x 100 mm 

_Attributes_
Description
	Filter papers (pack of 100)
	
Sample diameter
	100 mm

_Related Products_
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 110-120V 60Hz (45-6750/02)
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 220-240V 50Hz (45-6750/01)
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 220-240V 60Hz (45-6750/06)

[PRODUCT] 100mm Dia split mould (45-6750/27)
34 x 18.5 x 18.5 cms 

_Attributes_
Description
	Split mould
	
Sample diameter
	100 mm

_Related Products_
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 110-120V 60Hz (45-6750/02)
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 220-240V 50Hz (45-6750/01)
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 220-240V 60Hz (45-6750/06)

[PRODUCT] Spacer 100mm to compact 63mm height on 45-6750 (45-6750/25)
34 x 18.5 x 18.5 cms 

_Attributes_
Description
	Spacer to compact 63mm height
	
Sample diameter
	100 mm

_Related Products_
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 110-120V 60Hz (45-6750/02)
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 220-240V 50Hz (45-6750/01)
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 220-240V 60Hz (45-6750/06)

[PRODUCT] 100mm Dia mould & platens inc. specimen temperature measurement (45-6750/23)
34 x 18.5 x 18.5 cms 

_Attributes_
Description
	Mould & platens for specimen temperature measurement
	
Sample diameter
	100 mm

_Related Products_
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 110-120V 60Hz (45-6750/02)
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 220-240V 50Hz (45-6750/01)
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 220-240V 60Hz (45-6750/06)

[PRODUCT] 150mm Dia mould & platens (45-6750/12)
34 x 18.5 x 18.5 cms 

_Attributes_
Description
	Mould & platens
	
Sample diameter
	150 mm

_Related Products_
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 110-120V 60Hz (45-6750/02)
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 220-240V 50Hz (45-6750/01)
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 220-240V 60Hz (45-6750/06)

[PRODUCT] 150mm Dia mould & platens, slotted for emulsion mix (45-6750/15)
34 x 18.5 x 18.5 cms 

_Attributes_
Description
	Mould & platens slotted for emulsion mix
	
Sample diameter
	150 mm

_Related Products_
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 110-120V 60Hz (45-6750/02)
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 220-240V 50Hz (45-6750/01)
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 220-240V 60Hz (45-6750/06)

[PRODUCT] 150mm Dia  mould & platens inc. specimen temperature measurement (45-6750/21)
34 x 18.5 x 18.5 cms 

_Attributes_
Description
	Mould & platens for specimen temperature measurement
	
Sample diameter
	150 mm

_Related Products_
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 110-120V 60Hz (45-6750/02)
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 220-240V 50Hz (45-6750/01)
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 220-240V 60Hz (45-6750/06)

[PRODUCT] Spacer 150mm to compact 63mm height on 45-6750 (45-6750/26)

_Attributes_
Description
	Spacer to compact 63mm height
	
Sample diameter
	150 mm

_Related Products_
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 110-120V 60Hz (45-6750/02)
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 220-240V 50Hz (45-6750/01)
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 220-240V 60Hz (45-6750/06)

[PRODUCT] 150 mm filter papers (pack of 100) (45-6750/22)
150 mm x 150 mm

_Attributes_
Description
	Filter papers (pack of 100)
	
Sample diameter
	150 mm

_Related Products_
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 110-120V 60Hz (45-6750/02)
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 220-240V 50Hz (45-6750/01)
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 220-240V 60Hz (45-6750/06)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	Sample dia.
	N/A for this Product Group

[PRODUCT GROUP] Accessories for Gyratory Compactor

[PRODUCT] Specimen Extruder (45-6710)

_Attributes_
Description
	Specimen Extruder

_Related Products_
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 110-120V 60Hz (45-6750/02)
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 220-240V 50Hz (45-6750/01)
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 220-240V 60Hz (45-6750/06)

[PRODUCT] Calibration kit for internal angle lead (45-6750/11)

_Attributes_
Description
	Calibration kit for internal angle lead
	
Sample diameter
	n/a

_Related Products_
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 110-120V 60Hz (45-6750/02)
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 220-240V 50Hz (45-6750/01)
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 220-240V 60Hz (45-6750/06)

[PRODUCT] Internal angle measuring device (45-6750/13)

_Attributes_
Description
	Internal angle measuring device

_Related Products_
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 110-120V 60Hz (45-6750/02)
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 220-240V 50Hz (45-6750/01)
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 220-240V 60Hz (45-6750/06)

[PRODUCT] Internal angle measuring device inc. asphalt Hot Mix Simulator (HMS – Hot Mix Simulator) (45-6750/14)

_Attributes_
Description
	Internal angle measuring device with Hot Mix Simulator

_Related Products_
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 110-120V 60Hz (45-6750/02)
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 220-240V 50Hz (45-6750/01)
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 220-240V 60Hz (45-6750/06)

[PRODUCT] Option for 300mm mould height (cannot be retro-fitted) (45-6750/16)

_Attributes_
Description
	Option for 300 mm mould height (cannot be retro-fitted)

_Related Products_
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 110-120V 60Hz (45-6750/02)
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 220-240V 50Hz (45-6750/01)
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 220-240V 60Hz (45-6750/06)

[PRODUCT] 2 deg. angle plate (45-6750/17)

_Attributes_
Description
	2 degree angle plate

_Related Products_
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 110-120V 60Hz (45-6750/02)
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 220-240V 50Hz (45-6750/01)
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 220-240V 60Hz (45-6750/06)

[PRODUCT] Display, Shear Force (45-6750/18)

_Attributes_
Description
	Shear Force Display

_Related Products_
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 110-120V 60Hz (45-6750/02)
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 220-240V 50Hz (45-6750/01)
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 220-240V 60Hz (45-6750/06)

[PRODUCT] Specimen Temperature Measurement (45-6750/19)

_Attributes_
Description
	Specimen Temperature Measurement

_Related Products_
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 110-120V 60Hz (45-6750/02)
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 220-240V 50Hz (45-6750/01)
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 220-240V 60Hz (45-6750/06)

[PRODUCT] Small air compressor for 45-6750 (45-6750/28)
Compressed air supply 7-10 bar, 350 Litres per minute

_Attributes_
Description
	Air compressor

_Related Products_
Main: Gyratory Compactor to  EN 12697-31, 10, ASTM D6925, SHRP M-002, AASHTO T312, inc. PC 220-240V 50Hz (45-6750/01)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[CATEGORY] Design and Testing of Bituminous Mixtures

[CATEGORY] Mixing and Temperature
The density of Marshall specimens has a direct effect on stability and flow therefore the correct moulding and compaction of laboratory specimens is essential if economical design mixes are to be produced. Efficient mixing, temperature and compaction control are closely related. Poor coating of the aggregate due to low temperatures during the mixing process will have a major effect on subsequent test results.

[PRODUCT GROUP] Mixing
A regular laboratory requirement is the mixing of samples with water and/or other constituents to provide a homogeneous mixture prior to subsequent testing. The following range of mixers provide an efficient means of mixing samples.

[PRODUCT] Bench-Mounting Mixer 4.7Litre Capacity Complete with Bowl Beater and Whisk. 220-240V 50Hz 1Ph. (23-6191/01)
The mixer has two electrically switched mixing speeds which obviates the need to switch off during speed selection. The mixing head comprises a beater which contra-rotates about a central shaft using planetary gearing. A lever-acting lifting device facilitates the insertion and removal of the bowl. This mixer is suitable for the mixing of soil samples, mortar, bituminous mixtures and associated materials where comparatively small samples are being prepared. Supplied with stainless steel bowl, beater and whisk.

_Standards_
BS 598-107, BS 1377-1, BS 1924-1

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Bench-Mounting Mixer
	
Voltage Supply
	220 - 240 V AC, 50 Hz, 1ph

_Specification_
Dimensions
	545 x 380 x 550 mm
	
Beater Speeds (rpm) low, high
	140, 285
	
Central shaft speeds (rpm) low, high
	62, 125
	
Rated power
	500 W
	
Weight
	50 kg

_Related Products_
Accessory: Isomantle Electric Heater (45-5580/01)
Spare/Consumable: Stainless Steel Bowl 4.73 Litres. (23-6191/10)

[PRODUCT] Stainless Steel Bowl 4.73 Litres. (23-6191/10)
For use with the 5 Litre Bench Mounted Mixer - 23-6191/01

_Attributes_
Description
	Stainless Steel Bowl

_Related Products_
Main: Bench-Mounting Mixer 4.7Litre Capacity Complete with Bowl Beater and Whisk. 220-240V 50Hz 1Ph. (23-6191/01)

[PRODUCT] Isomantle Electric Heater (45-5580/01)
For use with 23-6191 Bench Mounting Mixer.

_Standards_
EN 12697-35

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Isomantle Electric Heater
	
Voltage Supply
	220 - 240 V AC, 50/60 Hz, 1 ph

_Related Products_
Main: Bench-Mounting Mixer 4.7Litre Capacity Complete with Bowl Beater and Whisk. 220-240V 50Hz 1Ph. (23-6191/01)

[GROUPED PRODUCT MATRIX]
Model No.
	Voltage
	Desc
	N/A for this Product Group

[CATEGORY] Compaction
The use of automatic compaction will result in consistent and repeatable laboratory specimens. Testing houses and design consultants who use the Marshall method of mix design will benefit from automatic compaction apparatus, which releases staff for other work during the compaction process.

[PRODUCT GROUP] Manual Compaction

[PRODUCT] Compaction Hammer (45-6460)
Satisfies BS 598. The hammer has a 4535 g sliding weight with a free fall of 457 mm.

_Standards_
EN 12697-30, ASTM D6926, AASHTO T245

_Attributes_
Description
	Compaction Hammer
	
Drop, ”
	18

_Specification_
Tamping Face
	3-7/8” (98 mm) diam.
	
Hammer
	10 lb. (4.54 kg).
	
Drop
	18” (457 mm).
	
Construction
	Machined steel; cast aluminum handle.
	
Weight
	Net 16 lbs. (7.2 kg).

[PRODUCT] Compaction Pedestal BS 598 (45-6410)
Comprising a 300 mm sq x 25 mm thick steel plate complete with 4 tie rods and securing nuts. A mould clamp and hammer guide are fitted to the plate. The unit is supplied complete with a laminated hardwood block.

_Standards_
EN 12697-30

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Compaction Pedestal
	
Weight, kg
	40

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Automatic Compaction

[PRODUCT] AutoComp 100-A (45-6600/01)
* Fully automatic, simple to operate* Built-in safety features* Uniform compaction* Automatic blow counterThis ruggedly constructed automatic compactor provides a consistent and even degree of compaction. The unit incorporates a compaction pedestal comprising a laminated hardwood block secured to a concrete base by a 300 mm square x 25 mm thick steel plate. The mechanism lifts the 4535 g hammer and automatically releases it at the specified height of 457 mm. The conveniently positioned control fascia panel comprises of a mains light, start and stop buttons and a direct-reading counter used to set the required number of blows.During operation the AutoComp 100-A automatically counts down to zero. Dual rammer pick-ups have been incorporated, reducing stress on the machine's internal mechanism.Particular attention has been paid to operator safety by the inclusion of various in-built safety features.

_Standards_
EN 12697-10, EN 12697-30

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	AutoComp 100-A
	
Power Supply
	220 - 240 V AC, 50 Hz, 1 ph

_Specification_
Dimensions (l x w x h)
	535 x 535 x 1880 mm
	
Compaction foot diameter
	98.52 mm
	
Sliding weight
	4535 g
	
Height of drop
	457 mm
	
Weight
	278 kg

_Related Products_
Main: Compaction Mould (45-6310)
Accessory: Digital Hotplate (78-3104/01)
Accessory: Paper Discs (45-6462)
Accessory: Sample Tray - 306 x 306 x 38 mm (81-4020)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Accessories for manual and automatic compaction

[PRODUCT] Paper Discs (45-6462)
Non-absorbent, 99 mm diameter, pack of 100.

_Standards_
EN 12697-30

_Attributes_
Description
	Paper Discs
	
Weight, oz.
	2.9

_Specification_
Weight
	Net 2.9 oz. (82 g).

_Related Products_
Main: AutoComp 100-A (45-6600/01)

[PRODUCT] Compaction Mould (45-6310)
Comprising of mould body, baseplate and combined filling/extraction collar.

_Standards_
EN 12697-30, ASTM D6926, AASHTO T245

_Attributes_
Description
	Compaction Mould
	
Dimensions, i.d x int. ht.
	4" (101.6 mm) i.d. x 3" (76.2 mm) internal h. with base

_Specification_
Construction
	Machined seamless steel forming mold;base and collar.
	
Finish
	Plated for rust resistance.
	
Dimensions
	4” (101.6 mm) i.d. x 3” (76.2 mm) internalh. with base.
	
Weight
	Net 6 lbs. (2.7 kg).

_Related Products_
Main: AutoComp 100-A (45-6600/01)

[PRODUCT] Proctor/Core Cutter Extruder Frame and Hydraulic Jack. Extrudes 100mm/4 Inch Diameter Specimens (23-4200)
Adaptor plates will be supplied; extrudes samples from BS Compaction Mould, Proctor Mould 100 mm, Core Cutter and Marshall Mould. Maximum extrusion force 20kn.

_Standards_
BS 1377-1

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Proctor /Core Cutter Extruder
	
Extrudes samples from
	BS compaction mould<br>Proctor Mould<br>100 mm core cutter<br>Marshall mould

_Related Products_
Main: 38mm Hand Operated Hydraulic Sample Extruder with Trimming Knife 38mm Split Former & Cutting Tool. (23-4090)
Main: Cbr/Core Cutter Extruder Frame and Hydraulic Jack Extrudes 150mm/6 Inch Diameter Specimens. (23-4250)
Main: Marshall Test 50 (45-6810/01)
Accessory: Steel Block (45-6463)

[PRODUCT] Compaction Mould Body (45-6310/10)
Accepts baseplate and filling/extraction collar of 45-6310 compaction mould.

_Standards_
EN 12697-30

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Compaction Mould Body

_Related Products_
Accessory: Steel Block (45-6463)

[PRODUCT] Baseplate (45-6310/11)
For compaction mould.

_Standards_
EN 12697-30

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Baseplate

_Related Products_
Accessory: Steel Block (45-6463)

[PRODUCT] Filling/Extraction Collar (45-6310/12)
For compaction mould.

_Standards_
EN 12697-30

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Filling/Extraction Collar

[PRODUCT] Steel Block (45-6463)
100 mm diameter x 50 mm height. For heating the compaction hammer foot.

_Standards_
EN 12697-30

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Steel Block

_Related Products_
Spare/Consumable: Baseplate (45-6310/11)
Spare/Consumable: Compaction Mould Body (45-6310/10)
Main: Proctor/Core Cutter Extruder Frame and Hydraulic Jack. Extrudes 100mm/4 Inch Diameter Specimens (23-4200)
Accessory: Water Bath (45-6490/01)

[PRODUCT] 30 L Heating Bath with Led Display Cover (45-6550/01)

_Standards_
BS 2000-49, EN 1426, EN 13179-2, ASTM D5, AASHTO T49, IP 49

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	30 L Heating Bath

_Related Products_
Accessory: Breaking Head (Marshall) (45-6850)
Main: Marshall Test 50 (45-6810/01)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[CATEGORY] Marshall Stability and Flow
The accurate measurement of stability and flow of specimens tested in a load frame is important if consistent and representative results are to be achieved. The load frames and ancillary items listed have been designed to enable technicians to test specimens quickly and easily with confident recording of results.

[PRODUCT GROUP] Load frames

[PRODUCT] Marshall Test 50 (45-6810/01)
* Geared screwjack and motor drive* Precise speed* Internal limit switch for both directions of travel* Easy to use controlsThis bench-mounting mechanical load frame is ruggedly constructed to encompass the strain and loads involved with the test. The unit is compact in size and can be quickly installed on a bench top, requiring only a power point. It has been designed for simple operation, is easy to clean and requires minimum maintenance.

_Standards_
EN 12697-34

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA** Load frame, 50 kN capacity. Supplied without Breaking Head. For 220 - 240 V AC, 50 Hz, 1 ph.

_Attributes_
Marshall stability and flow
	Yes
	
Power Supply
	220 - 240 V AC, 50 Hz, 1 ph

_Related Products_
Accessory: 250 Asphalt Probe (47-0202/10)
Accessory: 30 L Heating Bath with Led Display Cover (45-6550/01)
Accessory: 50kN Load Measuring Ring (78-0860)
Accessory: 50kN S-type Load Cell (27-1559)
Accessory: Breaking Head (Marshall) (45-6850)
Main: Digital Asphalt Thermometer (47-0202)
Main: ECU Electronic Control and Readout Unit (27-1200/09)
Accessory: Flow Meter BS/EN (45-6880)
Main: Proctor/Core Cutter Extruder Frame and Hydraulic Jack. Extrudes 100mm/4 Inch Diameter Specimens (23-4200)

[PRODUCT] MultiPlex 50 Load Frame (25-3700/01)
Compact bench mounting load frame designed for performing laboratory CBR, unconfined compression, quick undrained triaxial and Marshall Stability tests. Has a variable speed of 0.5 to 50mm per minute and features rapid approach of platen. 

_Standards_
EN 12697-34, BS 598, BS 1377, BS 1924, ASTM D1883, EN 12697-23, EN 12697-24, EN 13286-47, AASHTO T193, ASTM D2850, ASTM D4767, AASHTO T296, AASHTO T297

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	MultiPlex 50 Load Frame
	
CBR Penetration
	Yes
	
Unconfined Compression
	Yes
	
Voltage Supply
	220-240 V 50/60 Hz
	
Consolidated Undrained
	-
	
Consolidated Drained
	-
	
Power Supply
	220 - 240 V AC, 50 - 60 Hz, 1 ph
	
Marshall stability and flow
	Yes

_Specification_
Dimensions (l x w x h)
	550 x 400 x 1470 mm
	
Max vertical clearance
	800 mm
	
Horizontal clearance
	265 mm
	
Platen diameter
	133 mm
	
Platen travel
	100 mm
	
Platen speed range
	0.5 to 50 mm/min
	
Rapid approach speed
	40 mm/min
	
Weight kg
	100

_Related Products_
Accessory: 50kN Load Measuring Ring (78-0860)
Accessory: 50kN S-type Load Cell (27-1559)
Accessory: Bracket and Adaptor. Dual Purpose Mounting Bracket for CBR Penetration Gauges EL24-9184/EL24-9186 (24-9188)
Accessory: Cbr Penetration Piston (Adjustable). (24-9183)
Accessory: CBR Penetration Transducer 50mm Travel Fitted with 5 Pin Din Plug. (27-1705)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/06)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/01)
Accessory: Clamped Boss Load Ring - 10.0 kN (78-0460)
Accessory: Clamped Boss Load Ring - 2.0 kN (78-0060)
Accessory: Clamped Boss Load Ring - 28.0 kN (78-0760)
Accessory: Clamped Boss Load Ring - 3.0 kN (78-0160)
Accessory: Clamped Boss Load Ring - 4.5 kN (78-0260)
Main: Digital Tritest 50 (25-3518/01)
Accessory: Penetration Dial Gauge BS (24-9186)
Accessory: Penetration Piston (24-9182)
Accessory: Penetration/Swell Dial Gauge ASTM. (24-9184)

[GROUPED PRODUCT MATRIX]
Model No.
	Marshall
	CBR
	UC
	UU
	N/A for this Product Group

[PRODUCT GROUP] Accessories for the Marshall test

[PRODUCT] Breaking Head (Marshall) (45-6850)
Complete with gauge disc. Supplied without flow meter.

_Standards_
EN 12697-34

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Breaking Head
	
Weight, kg
	9

_Related Products_
Accessory: 250 Asphalt Probe (47-0202/10)
Accessory: 30 L Heating Bath with Led Display Cover (45-6550/01)
Accessory: 50kN S-type Load Cell (27-1559)
Main: Digital Asphalt Thermometer (47-0202)
Main: ECU Electronic Control and Readout Unit (27-1200/09)
Main: Marshall Test 50 (45-6810/01)

[PRODUCT] Flow Meter BS/EN (45-6880)
Dial gauge graduated 0.01 mm with 25 mm travel. Supplied with stem brake unit and flow meter pedestal.

_Standards_
EN 12697-34

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Flow Meter BS/EN
	
Weight, kg
	0.61

_Related Products_
Main: Marshall Test 50 (45-6810/01)

[PRODUCT] Flow Meter (45-6890)
Dial gauge graduated 0.001 inches with 1 inch travel. Supplied with stem brake unit and flow meter pedestal.

_Standards_
EN 12697-34

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Flow Meter
	
Weight, kg
	0.61

[PRODUCT] 50kN Load Measuring Ring (78-0860)
Calibrated in compression.

_Standards_
EN 12697-34

_Attributes_
Description
	Load ring - 50 kN
	
Value of CBR %
	Above 40%
	
Overall Height, mm
	248
	
Force Capacity, kN
	50
	
Load device type
	Load ring

_Specification_
Capacity: kN, kgf, lbf
	50.0, 5000, 11,200
	
Typical Design sensitivity: N/div, kgf/div, lbf/div
	45.5, 4.54, 10.18
	
Overall height mm
	248
	
Approx weight kg
	7.9
	
Capacity
	50 kN
	
Value of CBR
	Above 40%
	
Capacity - lbf
	11,200
	
Capacity - kN
	50
	
Capacity - kgf
	5,000
	
Typical Design Sensitivity - lbf/div
	10.18
	
Typical Design Sensitivity - kN/div
	45.5
	
Typical Design Sensitivity - Kgf/div
	4.54
	
Overall Height
	9.76” (248 mm)
	
Approx Weight
	17.4 lbs.(7.9 kg)

_Related Products_
Main: CBR Loading Press, Hand-Operated (24-9345)
Main: CBR-Test 50 Machine 50 kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/02)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/01)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/06)
Accessory: Clamped Boss Load Ring - 10.0 kN (78-0460)
Accessory: Clamped Boss Load Ring - 2.0 kN (78-0060)
Accessory: Clamped Boss Load Ring - 28.0 kN (78-0760)
Accessory: Clamped Boss Load Ring - 3.0 kN (78-0160)
Accessory: Clamped Boss Load Ring - 4.5 kN (78-0260)
Accessory: Digital Proving Ring, 11,200 lbs (50.0 kN) (78-0864)
Main: Digital Tritest 50 (25-3518/01)
Main: Digital Tritest 50 Load Frame 110-120vAC (25-3518/02)
Main: Marshall Test 50 (45-6810/01)
Main: MultiPlex 50 Load Frame (25-3700/01)
Spare/Consumable: Spare Dial Indicator for Load Rings (78-5461)
Main: Versa-Loader (25-3525/02)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Electronic Instrumentation

[PRODUCT] DSU Electronic Readout and Control System 110 V AC 60 Hz (27-1300/02)
· Download the full brochure here [/Page/catalogue-download/NTRmZS9UaGUgTkVXIERTVSBVU0EucGRm] · Download the full DS7.2 geotechnical software brochure here [/Page/catalogue-download/NTRmZS9OZXcgRFM3IFNvZnR3YXJlIFVTQTY5LnBkZg==] · 4 channel automatic control and data-logging unit · Automatic, dual-frame control · Performs CBR, Marshall, Unconfined Compression, Direct and Residual Shear, One-Dimensional Consolidation, Unconfined Undrained, Consolidated Drained and Unconsolidated Drained tests · LAN connection - software can be running anywhere on your server · Never lose data from power fails - 2 gigabytes of non-volatile memory The Data System Unit (DSU) is a versatile instrument designed to accomodate the general logging requirements of geotechnical and materials testing engineers. Its intelligent interface allows the user to work with a range of different sensors.

_Further Information_
Become a member of the ELE International web site, add this new product to a wishlist to receive a quote! Click here [/Login] This product is now available in the USA and Canada!

_Attributes_
Description
	DSU
	
Voltage Supply
	100-120 V 60 Hz

_Related Products_
Accessory: Cable, Safety/ID (27-1300/11)
Main: DSU Electronic Readout and Control System 220 - 240 V AC 50/60 Hz (27-1300/01)
Accessory: Dual Frame Comms Cable (27-1300/10)
Accessory: PC Cable (27-1300/12)

[PRODUCT] DSU Electronic Readout and Control System 220 - 240 V AC 50/60 Hz (27-1300/01)
· Download the full brochure here [/../../../Page/the-new-dsu] · 4 channel automatic control and data-logging unit · Automatic, dual-frame control · Performs CBR, Marshall, Unconfined Compression, Direct and Residual Shear, One-Dimensional Consolidation, Unconfined Undrained, Consolidated Drained and Unconsolidated Drained tests · LAN connection - software can be running anywhere on your server · Never lose data from power fails - 2 gigabytes of non-volatile memory · Extended warranty The Data System Unit (DSU) is a versatile instrument designed to accomodate the general logging requirements of geotechnical and materials testing engineers. Its intelligent interface allows the user to work with a range of different sensors.

_Further Information_
Become a member of the ELE International web site, add this new product to a wishlist to receive a quote! Click here [/../../../Login] Please note that this product is not yet available in the USA, we will let you know as soon as it is ready!

_Attributes_
Voltage Supply
	220-240 V 50/60 Hz
	
Description
	DSU

_Related Products_
Accessory: Cable, Safety/ID (27-1300/11)
Main: DSU Electronic Readout and Control System 110 V AC 60 Hz (27-1300/02)
Accessory: Dual Frame Comms Cable (27-1300/10)
Accessory: PC Cable (27-1300/12)

[PRODUCT] 50kN S-type Load Cell (27-1559)
Maximum working capacity of 50 kN and excitation 10 V ac/dc with an output of 2.7 mV/V nominal. Aluminium alloy and stainless steel construction with IP65 environmental protection.

_Standards_
EN 12697-34

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	S-type load cell - 50 kN
	
Value of CBR %
	ALL
	
Environmental Protection
	IP65
	
Force Capacity, kN
	50

_Related Products_
Accessory: Breaking Head (Marshall) (45-6850)
Main: CBR-Test 50 Machine 50 kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/02)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/01)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/06)
Main: Marshall Test 50 (45-6810/01)
Main: MultiPlex 50 Load Frame (25-3700/01)

[PRODUCT] Flow Transducer (45-6820)
Pre-calibrated, for use with 45-6850 Breaking Head.

_Standards_
EN 12697-34

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Flow Transducer

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	Voltage
	N/A for this Product Group

[CATEGORY] Core Drilling

[PRODUCT GROUP] Compact Core Drill Machine
This compact and portable core drilling machine is designed to cut cores up to 150 mm diameter from concrete, asphalt and similar hard construction material.

[PRODUCT] Compact Core Drill (47-5175)
This compact and portable core drilling machine is designed to cut cores up to 150 mm diameter from concrete, asphalt and similar hard construction material.The machine comprises a vertical support column which carries the drill head/motor assembly.An integral water swivel is built into the drill head providing a 12 mm connection to an external water supply via 12 mm flexible hose (not supplied). The motor assembly comprises a 4 hp, 2-stroke petrol engine. Speeds of 800 rpm or 1200 rpm may be selected. A ball screw mechanism enables close control over drilling pressure and rapid return when drilling is completed.The complete assembly is supplied on a rigid metal base frame with levelling facility and is suitable for vertically down drilling applications only.

_Standards_
EN 12697-32, EN 13280-4, BS 598-104

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA** Special Note: Requires a continuous clean water supply via a 12 mm flexible hose (not supplied).

_Attributes_
Description
	Compact Core Drill

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Core Barrels
Suitable for use with the Universal and Compact Core Drilling Machines, this range of core barrels comprise a thin-wall tube 450 mm long with a series of cutting segments formed from diamond abrasive set in a specially formulated hard matrix. The cutting face has been carefully designed to remove material rapidly and obtain the highest possible drilling rates. The solid back end includes a threaded fitting to connect to the waterswivel assembly of the core drill.

[PRODUCT] Core Barrel 100 mm (47-5565)

_Standards_
EN 12697-32, EN 13280-4, BS 598-104

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Length, mm
	100

[PRODUCT] Core Barrel 150 mm (47-5605)

_Standards_
EN 12697-32, EN 13280-4, BS 598-104

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Length, mm
	150

[GROUPED PRODUCT MATRIX]
Model No.
	Length, mm
	N/A for this Product Group

[CATEGORY] Pavement

[PRODUCT GROUP] Skid Resistance Testing
The Pendulum Skid Resistance Tester was originally designed in the 40s in the USA, and further developed in the 1960s at the TRL (Transport Research Laboratory) for the testing of road surfaces. The device measures the frictional resistance between a rubber slider mounted on the end of a pendulum arm and the surface to be tested. This provides road engineers with a method of checking the resistance of wet and dry surfaces to slipping and skidding, both in the lab and insitu. It operates by a pendulum rotating about a spindle which is attached to a vertical pillar. At the end of the tubular arm a head of known mass is fitted with a rubber slider. The pendulum is released from a horizontal position so that it strikes the sample surface at a constant speed. The distance travelled by the head after hitting the sample is determined by the friction of the sample surface. 
http://localhost//cms-files/56d9/56d9b1ce806cc.jpg

[PRODUCT] Pendulum Skid Resistance Tester (42-6000)
The Pendulum Skid Resistance Tester was originally designed in the 1940s in the USA, and further developed in the 1960s at the TRL (Transport Research Laboratory) for the testing of road surfaces. The device measures the frictional resistance between a rubber slider mounted on the end of a pendulum arm and the surface to be tested. This provides road engineers with a method of checking the resistance of wet and dry surfaces to slipping and skidding, both in the lab and insitu. It operates by a pendulum rotating about a spindle which is attached to a vertical pillar. At the end of the tubular arm a head of known mass is fitted with a rubber slider. The pendulum is released from a horizontal position so that it strikes the sample surface at a constant speed. The distance travelled by the head after hitting the sample is determined by the friction of the sample surface. 

_Further Information_
Applications:  	* Assessment of surface friction and skid resistance properties  	* Testing of aggregates in the PSV (Polished Stone Value) test  	* Testing of new road surface materials 	* Testing of pedestrian pavements 	* RTA (road traffic accidents)  	* Litigation investigations Features:  	* Designed for lab and on site road surface testing  	* Factory calibrated to EN1097-8  	* Low friction arm, and lightweight pointer  	* Supplied with 'F' scale for use with small slider set for 76mm slide length (PSV test)  	* Highly repeatable 	* Supplied with carrying case 

_Attributes_
Description
	Pendulum Skid Resistance Tester

_Specification_
Dimensions (WxDxH)
	695 x 295 x 695 mm
	
Volume
	0.15m3
	
Weight
	30 kg

_Related Products_
Accessory: 1.25” Rubber Mounted PSV Slider for 42-6000 (42-6000/11)
Accessory: 3.00” Rubber Mounted CEN Slider for 42-6000 (42-6000/14)
Accessory: 3.00” Rubber Mounted Four S (96) Slider for 42-6000 (42-6000/13)
Accessory: 3.00” Rubber Mounted TRL (55) Slider for 42-6000 (42-6000/12)
Accessory: Base Plate for Skid Resistance Tester for lab testing (42-6200)
Accessory: First traceable calibration for 42-6000 (42-6000/15)
Accessory: Set of 3 Spreader Feet for Skid Resistance Tester for in-situ testing (42-6000/10)

[PRODUCT] Set of 3 Spreader Feet for Skid Resistance Tester for in-situ testing (42-6000/10)

_Attributes_
Description
	Set of 3 Spreader Feet for Skid Resistance Tester for in-situ testing

_Related Products_
Main: Pendulum Skid Resistance Tester (42-6000)

[PRODUCT] Base Plate for Skid Resistance Tester for lab testing (42-6200)

_Attributes_
Description
	Base Plate for Skid Resistance Tester for lab testing

_Related Products_
Main: Pendulum Skid Resistance Tester (42-6000)

[PRODUCT] 1.25” Rubber Mounted PSV Slider for 42-6000 (42-6000/11)
Slider for polished stones

_Attributes_
Description
	1.25” Rubber Mounted PSV Slider

_Related Products_
Main: Pendulum Skid Resistance Tester (42-6000)

[PRODUCT] 3.00” Rubber Mounted TRL (55) Slider for 42-6000 (42-6000/12)
Slider for car tyres on asphalt

_Attributes_
Description
	3.00” Rubber Mounted TRL (55) Slider 

_Related Products_
Main: Pendulum Skid Resistance Tester (42-6000)

[PRODUCT] 3.00” Rubber Mounted Four S (96) Slider for 42-6000 (42-6000/13)
Slider for shoes on surfaces

_Attributes_
Description
	3.00” Rubber Mounted Four S (96) Slider

_Related Products_
Main: Pendulum Skid Resistance Tester (42-6000)

[PRODUCT] 3.00” Rubber Mounted CEN Slider for 42-6000 (42-6000/14)

_Attributes_
Description
	3.00” Rubber Mounted CEN Slider

_Related Products_
Main: Pendulum Skid Resistance Tester (42-6000)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[CATEGORY] Surface Regularity

[PRODUCT GROUP] Benkelman Beam
* Lightweight construction* Compact, telescopic design* Direct reading of deflection* Anti-vibration systemDesigned for maximum operator efficiency, the Benkelman Beam is manufactured from a lightweight, durable material which telescopes into a small, compact unit for ease of storage and transport.

[PRODUCT] Benkelman Beam (47-1460)

_Standards_
AASHTO T256

_Further Information_
Complete with Dial Gauge 25 mm tavel x 0.02 mm divisions.

_Attributes_
Description
	Benkelman Beam
	
Open Length, ft.
	12

_Specification_
Dimensions: Main Body (length), Arm (telescopic) extended, Operating length fully extended
	1397 mm, 2400 mm, 3700 mm
	
Beam fulcrum ratio
	2:1
	
Weight
	15.9 kg
	
Main Body
	55 â€ (1,397 mm) long, black finish aluminum.
	
Probe Beam
	Aluminum, 8 ft. (2.4 m) long, telescopes into case for storage.
	
Probe Fulcrum
	Ball pivot bearing, gives lever ratio of 2:1.
	
Vibrator System
	Operating switch mounted on top of instrument section (requires 4 â€œDâ€ size batteries).
	
Dial Indicators
	Compensated for direct reading (not included).
	
Leveling Wheel
	Adjusts beams to proper elevation.
	
Open Length
	12 ft. (3.7 m) l.
	
Weight
	Net 29 lbs. (13.2 kg).

_Related Products_
Accessory: Vertical Dial Indicator 1" range x 0.002" divisions (47-1460/12)
Accessory: Vertical Dial Indicator 25 mm range x 0.02 mm divisions (47-1460/14)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Travelling Beam Device

[PRODUCT] Travelling Beam Device (47-3025)
The 3 metre long Travelling Beam Device is used to check for any irregularities in both concrete and bituminous road surfaces. A sensing unit comprising a wheel connected to an indicator provides a magnification of 4:1.Deviation of the surface from a straight-line is shown on a scale calibrated in increments of 2 mm up to 10 mm and 5 mm up to 25 mm. A dye-marker is fitted which may be used to identify suspect areas. Outrigger wheels provide mobility on site. The device is supplied as three sub-assemblies which are quickly assembled on site. The Travelling Beam is supplied fitted with an autographic recorder providing a permanent record of the surface profile. Records up to 1 kilometre can be recorded on the special chart paper rolls used.

_Standards_
EN 12697-32, EN 13280-4, BS 598-104

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Travelling Beam Device
	
Weight, kg
	66

_Related Products_
Accessory: Charts for Autographic Recorder (47-3130)
Spare/Consumable: Fibre-tipped Pen (47-3131)

[PRODUCT] Charts for Autographic Recorder (47-3130)

_Standards_
EN 12697-32, EN 13280-4, BS 598-104

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Charts for Autographic Recorder
	
Weight, kg
	2.3

_Related Products_
Main: Travelling Beam Device (47-3025)

[PRODUCT] Fibre-tipped Pen (47-3131)

_Standards_
EN 12697-32, EN 13280-4, BS 598-104

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Fibre-tipped Pen

_Related Products_
Main: Travelling Beam Device (47-3025)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[CATEGORY] Surface Dressing
The main purpose of a surface dressing is to prevent weathering, disintegration of the pavement and to increase the resistance to skidding in wet weather. The rate of spread and application of the chippings and binder is specified for most applications. Test methods have been developed to determine the actual rate of spread and are described in British Standards.

[PRODUCT GROUP] Rate of Spread of Coated Chippings
The equipment comprises a tray 300 mm square which, when used in conjunction with a specially calibrated spring balance, will determine the rate of spread of coated chippings in terms of kg/m2. The spring loaded balance will accept rates of spread between 4 and 16 kg/m2.Between 5 and 10 trays are positioned in the path of the spreading machine and after the machine has passed over, each tray is lifted, together with the retained chippings, by means of four chains. The chains are hooked to the spring balance and the rate of spread is read directly from the balance scale.

[PRODUCT] Calibrated Spring Balance (47-0011)

_Standards_
EN 12272-1, BS 598-108

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Calibrated Spring Balance
	
Weight, kg
	0.8

[PRODUCT] Tray and Chains (47-0012)
Comprising one 300 mm square tray and four chains.

_Standards_
EN 12272-1, BS 598-108

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Tray and Chains

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[CATEGORY] Specific Gravity

[PRODUCT GROUP] Rice Test Vibrator

[PRODUCT] Rice Test Vibrator (45-9315/01)
The Rice Test Vibrator is used with the 45-9300 6000 g Vacuum Pyknometer. Adjustable clamps hold the pyknometer securely to the base during vibration.

_Standards_
EN 12697-5, ASTM D2041, AASHTO T209

_Further Information_
For 220 – 240 V AC, 50 Hz, 1ph.

_Attributes_
Description
	Rice Test Vibrator 220 - 240 V AC 50 Hz
	
Dimensions, h x dia, ”
	19-1/2 x 12

_Specification_
Dimensions
	495 x 30 mm (height x base diameter)
	
Motor
	1/20 hp, 1.6 amp
	
Weight
	5.5 kg
	
Motor
	1/20 h.p.; 3000 vpm; 1.6 amp.
	
Dimensions
	19-1/2â€ (495 mm) h.; 12 â€ (30 mm) base diameter.
	
Weight
	Net 14.3 lbs. (6.5 kg).

_Related Products_
Accessory: Attachment Required for 6000 g (45-9315/10)
Main: Rice Test Vibrator 115vAC, 50/60 Hz (45-9315/02)
Accessory: Timer Clock (81-0518)

[PRODUCT] Attachment Required for 6000 g (45-9315/10)
Accessory

_Standards_
EN 12697-5

_Attributes_
Description
	Attachment required for Rice Test Vibrator

_Related Products_
Main: Rice Test Vibrator (45-9315/01)
Main: Rice Test Vibrator 115vAC, 50/60 Hz (45-9315/02)

[PRODUCT] Timer Clock (81-0518)
Accessory

_Standards_
EN 12697-5

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Timer Clock
	
Main body length, arm, operating length mm
	13 x 64 x 58

_Related Products_
Accessory: ASTM Initial Set Needle (38-2620)
Accessory: ASTM Vicat Mould (38-2660)
Main: Blaine Air Permeability Apparatus (38-1000)
Main: Buoyancy Balance 6Kg X 0.1G. Supplied with Support Frame Water Tank & Suspension Hook. (42-1000/01)
Spare/Consumable: Consistency Plunger (38-2010/10)
Accessory: EN Initial and Final Set Needle (38-2110)
Main: Heat of Hydration Apparatus (38-4600/01)
Main: Heat of Hydration Apparatus (38-4600/06)
Main: Rice Test Vibrator (45-9315/01)
Main: Standard Penetrometer (46-5290)
Accessory: Vibrating Hammer (47-0455/01)
Main: Vicat Frame (38-2010)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Vacuum Pyknometer

[PRODUCT] Vacuum Pyknometer, 6000 g (45-9300)
The Vacuum Pyknometer is a large capacity unit used in the rice test for determining the maximum specific gravity of bituminous paving mixtures. The Pyknometer has a transparent top for observation and a lightweight polycarbonate construction. The Pyknometer has a total volume of 10 litres and will conveniently accept samples of 6000 grams to minimise segregation effects.

_Standards_
EN 12697-5, ASTM D2041, AASHTO T209, AASHTO T283

_Attributes_
Description
	Vacuum Pyknometer (6,000 gram)

_Specification_
Capacity
	Approximately 10 liters; 6,000 g (13 .2 lbs.) sample weight.
	
Construction
	Lightweight polycarbonate with transparent upper half.
	
Gauge
	2” (50.8 mm) diam., 30” x 0.5” Hg.
	
Aspirator
	Plastic; 3/8” pipe thread (included).
	
Connections
	Water inlet valve; quick disconnect for vacuum gauge and hose.
	
Dimensions
	10-3/4” (273 mm) o.d. x 16” (406 mm) h.
	
Weight
	Net 8 lbs. (3.6 kg).

_Related Products_
Accessory: 1/4" O.D Plastic Tubing (45-9301/14)
Accessory: Drierite Desiccant (45-9315/14)
Accessory: Filtering Kit (45-9301)
Main: Vacuum Pyknometer (2,000 gram) (45-9310)
Main: Vacuum Pyknometer Apparatus (45-9305/01)

[PRODUCT] Vacuum Pyknometer Apparatus (45-9305/01)
* Large capacity design minimises segregation effects* Lightweight polycarbonate construction* Transparent top for visual observationsThe Vacuum Pyknometer is a large capacity unit used in the Rice Test for determining the maximum specific gravity of bituminous paving mixtures.The Pyknometer has a total volume of approximately 10 litres and will conveniently accept samples of 6000 grams to minimise segregation effects. The unit is constructed of lightweight polycarbonate, with the upper half being transparent for visual observation of the effects of the vacuum.The Vacuum Pyknometer Apparatus consists of a 6000 g pyknometer, vacuum pump with control valves/gauges, water trap and connection tubing.

_Standards_
EN 12697-5

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA** Supplied complete with 6000 g pyknometer, vacuum pump with control valves/gauges, water trap and connection tubing. For 220 - 240 V AC, 50 Hz, 1ph.

_Attributes_
Description
	Vacuum Pyknometer Apparatus
	
Power Supply
	220 - 240 V AC, 50 Hz, 1 ph

_Specification_
Dimensions
	273 x 406 mm (outside diameter x height)
	
Capacity
	Approx. 10 litres, 6000 g sample weight
	
Connections
	Water inlet valve; quick disconnect for vacuum gauge and hose
	
Weight
	3.6 kg

_Related Products_
Main: Vacuum Pyknometer, 6000 g (45-9300)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[CATEGORY] Temperature and Density
Delivery and compaction temperatures are probably the most common measurements taken during the placing of bituminous mixtures.

[PRODUCT GROUP] Digital Asphalt Thermometer
Supplied without probes the LCD display has large 12.5 mm characters and is powered by a standard PP3 battery or equivalent.

[PRODUCT] Digital Asphalt Thermometer (47-0202)
Comprises a hand-held digital thermometer with an operating range of -99 to +1372 °C with a switchable resolution between 0.1 and 1.0 °C. Operates on a 9V battery and utilises K-type thermocouple sensors.

_Standards_
BS 2000-49, EN 1426, EN 13179-2, ASTM D5, AASHTO T49, IP 49

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Digital Asphalt Thermometer
	
Temperature Range °C
	-50 to 1,000 °C
	
Resolution °C
	Switchable 0.1 or 1.0

_Specification_
Range
	–50 to 1000ºC
	
Resolution
	Switchable 0.1 or 1.0°C
	
Weight
	300 g

_Related Products_
Accessory: 250 Asphalt Probe (47-0202/10)
Accessory: Breaking Head (Marshall) (45-6850)
Main: Marshall Test 50 (45-6810/01)
Accessory: Vibrating Hammer (47-0455/01)

[PRODUCT] 250 Asphalt Probe (47-0202/10)
Has a heavy-duty and reinforced needle probe. It is built with a t-shaped polyethylene handle and has a maximum tip temperature of 250°c and a 300 mm long probe.

_Standards_
BS 2000-49, EN 1426, EN 13179-2, ASTM D5, AASHTO T49, IP 49

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Asphalt Probe
	
Maximum Temperature, ºC
	250 °C
	
Probe length mm
	300
	
Tip Diameter (needle point) mm
	6

_Specification_
Max Reading
	250°C
	
Length of probe
	300 mm
	
Tip diameter (needle point)
	6 mm

_Related Products_
Accessory: Breaking Head (Marshall) (45-6850)
Main: Digital Asphalt Thermometer (47-0202)
Main: Marshall Test 50 (45-6810/01)
Accessory: Vibrating Hammer (47-0455/01)

[PRODUCT] 535 Asphalt Probe (47-0202/11)
Has a heavy-duty and reinforced needle probe. It is built with a t-shaped polyethylene handle and has a maximum tip temperature of 250°c and a 500 mm long probe.

_Standards_
BS 2000-49, EN 1426, EN 13179-2, ASTM D5, AASHTO T49, IP 49

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Asphalt Probe
	
Maximum Temperature, ºC
	250 °C
	
Probe length mm
	500
	
Tip Diameter (needle point) mm
	6

_Specification_
Max Reading
	250°C
	
Length of probe
	500 mm
	
Tip diameter (needle point)
	100 mm

[PRODUCT] Surface Probe (47-0202/14)
130 mm long Ribbon-Type surface probe with a maximum tip temperature of 500 °C.

_Standards_
BS 2000-49, EN 1426, EN 13179-2, ASTM D5, AASHTO T49, IP 49

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Surface Probe
	
Maximum Temperature, ºC
	500 °C
	
Probe length mm
	100
	
Tip Diameter (needle point) mm
	4

_Specification_
Max Reading
	500°C
	
Length of probe
	6 mm
	
Tip diameter (needle point)
	4 mm

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	Temp Range
	Max. Temp
	Probe length
	N/A for this Product Group

[PRODUCT GROUP] Percentage Refusal Density (PRD)
Percentage Refusal Density (PRD) is defined as the ratio of the initial dried bulk density of the sample to the final density (refusal density) expressed as a percentage.

[PRODUCT] 225 Litre Drying Oven (78-1250/01)

_Standards_
EN 12697-32, EN 13280-4, BS 598-104, BS 1377

_Attributes_
Description
	Drying Oven
	
Capacity, litres
	225
	
No. of shelves supplied
	3
	
No. of shelf positions
	4
	
Temperature Fluctuation
	+/- 0.75 °C
	
Internal Dimensions (length x width x height) mm
	440 x 920 x 600 mm
	
Temperature Range °C
	0 - 200 °C
	
Voltage Supply
	220-240 V 50/60 Hz

_Specification_
Capacity
	225 litres
	
External Dimensions (l x w x h)
	540 x 1040 x 940
	
Internal Dimensions (l x w x h)
	440 x 920 x 600
	
Fluctuation
	± 0.75°C
	
Rated power heater elements
	2000 W
	
Shelves supplied
	3
	
Shelf positions
	4
	
Weight
	80 kg

_Related Products_
Main: 100 Litre Drying Oven (78-1225/01)
Main: 150 Litre Drying Oven (78-1235/01)
Main: 425 Litre Drying Oven (78-0135/01)
Main: 50 Litre Drying Oven (78-1215/01)

[PRODUCT] Cradle (34-8105)

_Standards_
EN 12697-32, EN 13280-4, BS 598-104

_Attributes_
Description
	Cradle
	
Weight, lbs
	1.24

_Related Products_
Main: Buoyancy Balance (34-8100/09)
Main: ELE Buoyancy Balance (34-8100/02)
Accessory: Vibrating Hammer (47-0455/01)

[PRODUCT] PRD Split Mould and Baseplate (47-0450)

_Standards_
EN 12697-32, EN 13280-4, BS 598-104

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	PRD Split Mould and Baseplate
	
Weight, kg
	10.7

_Related Products_
Accessory: 300 mm Shank (47-0480)
Accessory: Vibrating Hammer (47-0455/01)

[PRODUCT] Vibrating Hammer (47-0455/01)
Accessory - suitable for compacting asphalt samples.

_Standards_
EN 12697-32, EN 13280-4, BS 598-104

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Vibrating Hammer
	
Power Supply
	220 - 240 V AC, 50 - 60 Hz, 1ph

_Related Products_
Accessory: 250 Asphalt Probe (47-0202/10)
Accessory: 300 mm Shank (47-0480)
Accessory: Cradle (34-8105)
Main: Digital Asphalt Thermometer (47-0202)
Accessory: Engineer's Steel Rule (81-0805)
Accessory: Filter Paper - Medium (82-7901)
Main: Melting Pot 4 Litre Capacity. 50 to 300 Deg. C. Temperature Range. (34-6122/01)
Accessory: Paraffin Wax (82-7031)
Main: PRD Split Mould and Baseplate (47-0450)
Accessory: Spatula 200 mm (81-0140)
Accessory: Timer Clock (81-0518)
Accessory: Vernier Caliper (LCD) Range 0 to 200mm X 0.01mm (81-0590)

[PRODUCT] 300 mm Shank (47-0480)
Complete with tamping feet - 102 mm and 146 mm dia.

_Standards_
EN 12697-32, EN 13280-4, BS 598-104

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	300 mm Shank

_Related Products_
Main: PRD Split Mould and Baseplate (47-0450)
Accessory: Vibrating Hammer (47-0455/01)

[PRODUCT] Buoyancy Balance (34-8100/09)

_Standards_
EN 12697-32, EN 13280-4, BS 598-104

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Buoyancy Balance
	
Power Supply
	110 - 240 V AC, 50 - 60 Hz, 1 ph

_Related Products_
Accessory: Cradle (34-8105)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group