[DEPARTMENT] Environmental

[CATEGORY] Physical Survey

[PRODUCT GROUP] Aerial Survey

[PRODUCT] Pocket stereoscope (500-010)
Complete with case

_Further Information_
x2 magnification with plastic frame

_Attributes_
Description
	Pocket stereoscope
	
Magnification
	x 2

[PRODUCT] Basic mirror stereoscope (500-012)
Complete with case

_Attributes_
Description
	Basic mirror stereoscope
	
Magnification
	x 1.5

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	Magnification
	N/A for this Product Group

[PRODUCT GROUP] Surveying Equipment

[PRODUCT] Binoculars, 10x50 (500-190)
Centre-wheel focusing and multicoated optics. Particularly suited to twilight and night observations. Supplied complete with carrying case.

_Attributes_
Description
	Binoculars

[PRODUCT] Pocket altimeter (500-112)
With combination holder, as specified.

_Attributes_
Description
	Pocket altimeter

[PRODUCT] Electronic digital theodolite (500-175)
Supplied complete with instruction manual, protective cover, carrying case and tripod.

_Attributes_
Description
	Digital theodolite

[PRODUCT] Automatic Level (500-170)
Supplied complete with instruction manual, protective cover, carrying case and wooden tripod.

_Attributes_
Description
	Automatic Level

_Related Products_
Accessory: Levelling staff, 4m (500-144)
Accessory: Levelling staff, 5m (500-145)

[PRODUCT] Levelling staff, 4m (500-144)
Aluminium 4 section telescopic.

_Attributes_
Description
	Levelling staff 4m

_Related Products_
Main: Automatic Level (500-170)
Accessory: Levelling staff, 5m (500-145)

[PRODUCT] Levelling staff, 5m (500-145)
Aluminium 5 section telescopic.

_Attributes_
Description
	Levelling staff 5m

_Related Products_
Main: Automatic Level (500-170)
Accessory: Levelling staff, 4m (500-144)

[PRODUCT] Ranging rod (500-146)
jointed, 2 metre length.

_Attributes_
Description
	Ranging rod

[PRODUCT] Land chain (500-154)
30 m, black enamelled.

_Attributes_
Description
	Land chain

_Related Products_
Accessory: Land chain arrows (500-156)

[PRODUCT] Land chain arrows (500-156)
In bundles of 10.

_Attributes_
Description
	Land chain arrows

_Related Products_
Main: Land chain (500-154)

[PRODUCT] Clinometer (500-106)
A hand-held precision instrument for determining heights, slopes and vertical angles. The direct sighting device has the peak scale reading visible through the eye piece. Percentage and degree scales permit quick calculation of object heights using a known base line distance. Used by foresters, geologists and surveyors throughout the world.

_Attributes_
Description
	Clinometer

[PRODUCT] Sighting Compass (500-108)
With inclinometer. A folding pocket instrument with sighting mirror in the lid. Used for defining map locations and measuring geological equipment.

_Attributes_
Description
	Sighting Compass

[PRODUCT] Land measurer (500-118)
For rough terrain.

_Attributes_
Description
	Land measurer

[PRODUCT] Double prismatic square (500-126)
In leather case with plumb bob. As described.

_Attributes_
Description
	Double prismatic square

[PRODUCT] Abney level (500-132)
With separate magnifier, carrying case and sling.

_Attributes_
Description
	Abney level

[PRODUCT] Planimeter (500-140)
Complete in fitted case.

_Further Information_
320 x 50 x 140 mm

_Attributes_
Description
	Planimeter

[PRODUCT] Nylon-coated steel tape (500-162)
50 m on open frame winder.

_Attributes_
Description
	Steel tape

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[CATEGORY] Soils
ELE INTERNATIONAL ARE EXCLUSIVE UK DISTRIBUTORS OF SOILMOISTURE EQUIPMENT CORP.See our range of Soilmoisture products in the sub-categories below

[CATEGORY] Soil Sampling

[PRODUCT GROUP] Augers
A range of durable augers are based on a threaded joint system. Items in this section may be interchanged and extended to any depth required. For increased versatility and convenience it may be preferred to have sectional augers. When joined with a bayonet and sleeve connection, the resulting unit has a working length of 1.25 metres. If required the augers may be further extended by either 0.5 or 1 metre increments.

[PRODUCT] Edelman Auger 50mm Dia (510-078)
One piece model, length 1.25 metres. This is suitable for most soft soil types.

_Attributes_
Description
	Edelman Auger 50mm Dia

_Related Products_
Main: Edelman Auger 70mm Dia (510-080)

[PRODUCT] Edelman Auger 70mm Dia (510-080)
One piece model, length 1.25 metres. This is suitable for most soft soil types.

_Attributes_
Description
	Edelman Auger 70mm Dia

_Related Products_
Main: Edelman Auger 50mm Dia (510-078)

[PRODUCT] Riverside Auger 70mm Dia  (510-086)
One piece model, length 1.25 metres. This auger is used in hard stiff soils above and below ground water level. It is also satisfactory in most fine gravel soils.

_Attributes_
Description
	Riverside Auger 70mm Dia

[PRODUCT] Spiral Auger 40mm. (510-119)
One piece head and rod, approximately 600 mm long with bayonet connection for use with 510-109.

_Attributes_
Description
	Spiral Auger 40mm

[PRODUCT] Auger 70mm for Stony Ground. (510-118)
For stony ground, one piece head and rod, approximately 600 mm long with bayonet connection for use with 510-109.

_Attributes_
Description
	Auger 70mm for Stony Ground

[PRODUCT] Auger for Stony Ground 70mm Dia. One Piece Model (510-092)
One piece model, length 1.25 metres. This is used when the Riverside auger is inadequate to deal with the larger sizes of grael and stones.

_Attributes_
Description
	Auger for Stony Ground 70mm Dia

[PRODUCT] Edelman 70mm Clay Auger (510-112)
One piece head and rod, approximately 600 mm long with bayonet connection for use with 510-109.

_Attributes_
Description
	Edelman 70mm Clay Auger

_Related Products_
Main: Edelman 100mm Clay Auger. (510-113)

[PRODUCT] Edelman 100mm Clay Auger. (510-113)
One piece head and rod, approximately 600 mm long with bayonet connection for use with 510-109.

_Attributes_
Description
	Edelman 100mm Clay Auger

_Related Products_
Main: Edelman 70mm Clay Auger (510-112)

[PRODUCT] Edelman 70mm Sand Auger. (510-117)
One piece head and rod, approximately 600 mm long with bayonet connection for use with 510-109.

_Attributes_
Description
	Edelman 70mm Sand Auger

[PRODUCT] Handle and Down-Tube Assembly. (510-109)
600 mm long bayonet connection with coupling sleeve.

_Attributes_
Description
	Handle and Down-Tube Assembly

[PRODUCT] Extension Rod 0.5 Metre. (510-111)
With coupling sleeve.

_Attributes_
Description
	Extension Rod 0.5 Metre

_Related Products_
Main: Extension Rod 1 Metre (510-110)

[PRODUCT] Extension Rod 1 Metre (510-110)
With coupling sleeve.

_Attributes_
Description
	Extension Rod 1 Metre

_Related Products_
Main: Extension Rod 0.5 Metre. (510-111)

[PRODUCT] Gouge Auger 30 mm dia. (510-100)
One piece Model, operating length 1 metre.

_Attributes_
Description
	Gouge Auger 30 mm dia

[PRODUCT] Root Auger 80mm dia.  (510-104)
One piece model, sample length 150 mm.

_Attributes_
Description
	Root Auger 80mm dia

[PRODUCT] Grass Plot Sampler Small (510-106)
For collecting samples from the top 50 mm of the turf.

_Further Information_
Diam 23mm, op length 5cm, Total Length 60 cm

_Attributes_
Description
	Grass Plot Sampler

[PRODUCT] Edelman 40mm Combination Auger. (510-114)
One piece head and rod, approximately 600 mm long with bayonet connection for use with 510-109.

_Attributes_
Description
	Edelman 40mm Combination Auger

_Related Products_
Main: Edelman 100mm Combination Auger. (510-116)
Main: Edelman 70mm Combination Auger. (510-115)

[PRODUCT] Edelman 70mm Combination Auger. (510-115)
One piece head and rod, approximately 600 mm long with bayonet connection for use with 510-109.

_Attributes_
Description
	Edelman 70mm Combination Auger

_Related Products_
Main: Edelman 100mm Combination Auger. (510-116)
Main: Edelman 40mm Combination Auger. (510-114)

[PRODUCT] Edelman 100mm Combination Auger. (510-116)
One piece head and rod, approximately 600 mm long with bayonet connection for use with 510-109.

_Attributes_
Description
	Edelman 100mm Combination Auger

_Related Products_
Main: Edelman 40mm Combination Auger. (510-114)
Main: Edelman 70mm Combination Auger. (510-115)

[PRODUCT] Hand Auger Set 5M. (510-124)
Complete in an aluminium transport case with padlock.

_Further Information_
1080 x 230 x 140 mm.

_Attributes_
Description
	Hand Auger Set 5M

_Related Products_
Main: Hand Auger Set 7m. (510-128)

[PRODUCT] Hand Auger Set 7m. (510-128)
For augering all types of soil above and below the water table to a depth of 7 metres complete in aluminium transport case.

_Further Information_
1120 x 390 x 320 mm.

_Attributes_
Description
	Hand Auger Set 7m

_Related Products_
Main: Hand Auger Set 5M. (510-124)

[PRODUCT] Peat Auger Set. (510-120)
For sampling to a depth of 10 metres, complete in an aluminium transport case.

_Further Information_
1080 x 230 x 140 mm.

_Attributes_
Description
	Peat Auger Set

[PRODUCT] Sampling Kit with Water Retentivity Rings  (510-144)
This kit contains the necessary items to sample above and below the water table and comprises the handle and beating head, Edelman auger, a riverside auger, a closed ring auger and spare cutting shoe, a hammering head and guide cylinder for the rings, a nylon headed hammer, 3 extension rods 500 mm long, 24 numbered sample rings with end caps in an aluminium case, a bent spatula, brush and a carrying bag for all the equipment.

_Further Information_
Above and Below The Water Table

_Attributes_
Description
	Sampling Kit with Water Retentivity Rings

[PRODUCT] 24 Sample Rings 50mm Dia In Aluminium Case. (510-146)
In an aluminium case, 50 mm inside diamter, 53 mm outside diameter, 51 mm long. Includes 48 plastic end covers.

_Attributes_
Description
	Sample Rings 50 mm Dia

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Soil water samplers
Samples water from saturated and unsaturated soils. Easy installation and sample retrieval. Requires no maintenance. Ideal for nitrate monitoring. This range of 48mm diameter soil water samplers can be installed either above or below the water table. They are designed to collect soil water which can then be extracted from the device and taken to the laboratory for analysis. The sampler is installed into a hole made with a screw or bucket auger. A negative pressure of up to 85 centibars is applied to the tube using a hand pump. Water enters the sampler through the porous ceramic cup at the end of the sampler. Water samples can then be collected as rerquired using a syringe. The rate of water accumulation depends on the soil type and moisture content. Nitrate leaching from fertilizer applications can be monitored simply and effectively using this method.

[PRODUCT] Soil Water Sampler, 30 cm X 48 mm Dia. (450-060)
Ceramic Tip Stopper Assembly Neoprene Tubing and Pinch Clamp

_Attributes_
Description
	Soil Water Sampler - 30 cm x 48 mm

_Related Products_
Spare/Consumable: Nylon Tube 7.5 Metres (450-060/10)
Main: Soil Water Sampler, 60 cm X 48 mm Dia. (450-062)
Main: Soil Water Sampler, 90 cm X 48 mm Dia. (450-064)
Accessory: Universal Extraction Kit (450-066)

[PRODUCT] Soil Water Sampler, 60 cm X 48 mm Dia. (450-062)
Ceramic Tip Stopper Assembly Neoprene Tubing and Pinch Clamp

_Attributes_
Description
	Soil Water Sampler - 60 cm x 48 mm

_Related Products_
Spare/Consumable: Nylon Tube 7.5 Metres (450-060/10)
Main: Soil Water Sampler, 30 cm X 48 mm Dia. (450-060)
Main: Soil Water Sampler, 90 cm X 48 mm Dia. (450-064)
Accessory: Universal Extraction Kit (450-066)

[PRODUCT] Soil Water Sampler, 90 cm X 48 mm Dia. (450-064)
Ceramic Tip Stopper Assembly Neoprene Tubing and Pinch Clip

_Attributes_
Description
	Soil Water Sampler - 90 cm x 48 mm

_Related Products_
Spare/Consumable: Nylon Tube 7.5 Metres (450-060/10)
Main: Soil Water Sampler, 30 cm X 48 mm Dia. (450-060)
Main: Soil Water Sampler, 60 cm X 48 mm Dia. (450-062)
Accessory: Universal Extraction Kit (450-066)

[PRODUCT] Universal Extraction Kit (450-066)
Includes Vacuum Pump 50Ml Syringe and 2 Metres Nylon Tubing

_Attributes_
Description
	Universal Extraction Kit

_Related Products_
Spare/Consumable: Nylon Tube 7.5 Metres (450-060/10)
Main: Soil Water Sampler, 30 cm X 48 mm Dia. (450-060)
Main: Soil Water Sampler, 60 cm X 48 mm Dia. (450-062)
Main: Soil Water Sampler, 90 cm X 48 mm Dia. (450-064)

[PRODUCT] Nylon Tube 7.5 Metres (450-060/10)
Spares for 450-066

_Attributes_
Description
	Nylon Tube

_Related Products_
Main: Soil Water Sampler, 30 cm X 48 mm Dia. (450-060)
Main: Soil Water Sampler, 60 cm X 48 mm Dia. (450-062)
Main: Soil Water Sampler, 90 cm X 48 mm Dia. (450-064)
Accessory: Universal Extraction Kit (450-066)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[CATEGORY] Soil Analysis

[PRODUCT GROUP] Soil test kits
No weighing required. Safe and accurate to use. Consistency of test results. No storage or shipping hazards. Our range of soil test kits enables people without access to normal laboratory facilities to obtain accurate information about the nutrient status of a soil sample. The tests are based on a system which uses reagents compressed into stable tablet form. The tests are conducted without the intricacies of weighing out chemicals or dispensing liquid reagents. Applications include soil classification, identification of nutrient deficiencies, routine soil analysis, field and educational uses.

[PRODUCT] Complete Soil Analysis Test Kit. Photometer Ph and Conductivity Meters and Reagents for 50 Tests (513-024)
A complete soils analysis kit:  	* pH 	* lime requirement 	* nitrate nitrogen 	* phosphate 	* potassium 	* conductivity 	* calcium 	* magnesium 	* aluminium 	* ammonia 	* copper 	* chloride 	* iron 	* manganese 	* sulphate 

_Further Information_
Reagents 50 Tests of each parameter. Includes soil scoop, de-ion pack, Pocket TDS Meter, SoilTest 10 Instrument and Pokcet pH Meter. The kit is ideal where highly accurate measurement of soil ph is required or where the measurement of conductivity for salt content is an important factor in agricultural management. The ph and conductivity meters included in the kit are each supplied in a soft carrying pouch.

_Attributes_
pH Test
	Yes
	
Lime Requirement Test
	Yes
	
Nitrate Nitrogen Test
	Yes
	
Phosphate Phosphorous Test
	Yes
	
Potassium Test
	Yes
	
Calcium Test
	Yes
	
Magnesium Test
	Yes
	
Conductivity Test
	Yes
	
Complete Test
	Yes
	
Description
	Complete Soil Testing Kit with Photometer, pH & Conductivity Meters

[PRODUCT] Soil pH and Lime Requirement Test Kit (513-012)
Soil pH & Lime Requirement Kit, includes 50 pH and lime requirement tests using a comparison block.

_Further Information_
Includes a soil coop, de-ion pack and pH block.

_Attributes_
pH Test
	Yes
	
Lime Requirement Test
	Yes

[PRODUCT] Soil Analysis Test Kit for Major Nutrients (513-016)
This soil fertility kit tests for:  	* pH 	* lime requirement 	* nitrate nitrogen 	* phosphate 	* potassium

_Further Information_
Includes soil scoop, de-ion pack, pH block and N/Mg/P Soiltester block.

_Attributes_
pH Test
	Yes
	
Lime Requirement Test
	Yes
	
Nitrate Nitrogen Test
	Yes
	
Phosphate Phosphorous Test
	Yes
	
Potassium Test
	Yes
	
Description
	Major Nutrients Soil Testing Kit

[PRODUCT] Combination Soil Analysis Test Kit (513-018)
This test kit includes reagents for 50 tests of each:  	* pH 	* lime requirement 	* nitrate nitrogen 	* phosphate 	* potassium 	* conductivity 	* calcium 	* magnesium

_Further Information_
Includes soil scoop, de-ion pack, pH block, Pocket TDS Meter and N/Mg/P Soiltester block.

_Attributes_
pH Test
	Yes
	
Lime Requirement Test
	Yes
	
Nitrate Nitrogen Test
	Yes
	
Phosphate Phosphorous Test
	Yes
	
Potassium Test
	Yes
	
Calcium Test
	Yes
	
Magnesium Test
	Yes
	
Conductivity Test
	Yes
	
Description
	Soil Analysis Test Kit with Reagents for 50 Tests

[PRODUCT] Soil Management Test Kit (513-019)
For 50 tests of each of the principal nutrients:  	* nitrate nitrogen 	* phophate 	* potassium 	* magnesium 	* pH 	* lime requirement

_Further Information_
Includes soil scoop, de-ion pack, Pocket TDS Meter, SoilTest 10 Instrument and Pocket pH Meter.

_Attributes_
pH Test
	Yes
	
Lime Requirement Test
	Yes
	
Nitrate Nitrogen Test
	Yes
	
Phosphate Phosphorous Test
	Yes
	
Potassium Test
	Yes
	
Calcium Test
	Yes
	
Magnesium Test
	Yes
	
Conductivity Test
	Yes
	
Description
	Nutrient Analysis Soils Testing Kit with Digital Photometer

[GROUPED PRODUCT MATRIX]
Model No.
	pH Test
	Lime
	Nitrate
	Phosphate
	Potassium
	Calcium
	Magnesium
	Conductivity
	Complete
	N/A for this Product Group

[CATEGORY] Soil Water

[PRODUCT GROUP] Permeability

[PRODUCT] Double Ring Infiltrometer Kit. (514-440)
Comprising 3 infiltrometers; inner ring 280 mm, outer ring 530 mm diamter; inner ring 300 mm, outer ring 550 mm diameter; inner ring 320 mm, outer ring 570 mm diameter; driving plate with handle for inner and outer rings, 3 adjustable measuring bridges, 3 floats with measuring rods, nylon headed hammer, stopwatch.

_Attributes_
Description
	Double Ring Infiltrometer Kit

_Related Products_
Accessory: Driving Plate (514-446)

[PRODUCT] Double Ring Infiltrometer  (514-444)
With measuring bridge and float.

_Attributes_
Description
	Double Ring Infiltrometer

[PRODUCT] Driving Plate (514-446)
With handle for placing

_Attributes_
Description
	Driving Plate

_Related Products_
Main: Double Ring Infiltrometer (25-0660)
Main: Double Ring Infiltrometer Kit. (514-440)

[PRODUCT] Driven Wellpoint Piezometer Tip. (514-380)
Comprising a porous plastic element. 19 mm diameter x 300 mm long, in a perforated steel tube with hardened steel driving point. Terminates in a 3/4 inch BSP pocket.

_Attributes_
Description
	Driven Wellpoint Piezometer Tip

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Soil Moisture

[PRODUCT] Soil Moisture Meter. (514-126)
Battery operated, 9 V battery supplied.

_Attributes_
Description
	Soil Moisture Meter

[PRODUCT] Soil Moisture Block 0.9 m Lead (514-128)
0.9 Meter Long Lead

_Attributes_
Description
	Soil Moisture Block
	
Lead Length
	0.9 m

_Related Products_
Accessory: Soil Moisture Block 2.7 m Lead (514-130)
Accessory: Soil Moisture Block 4.5 m Lead (514-132)

[PRODUCT] Soil Moisture Block 2.7 m Lead (514-130)
2.7 Metre Long Lead

_Attributes_
Description
	Soil Moisture Block
	
Lead Length
	2.7 m

_Related Products_
Accessory: Soil Moisture Block 0.9 m Lead (514-128)
Accessory: Soil Moisture Block 4.5 m Lead (514-132)

[PRODUCT] Soil Moisture Block 4.5 m Lead (514-132)
4.5 Metre Long Lead

_Attributes_
Description
	Soil Moisture Block
	
Lead Length
	4.5 m

_Related Products_
Accessory: Soil Moisture Block 0.9 m Lead (514-128)
Accessory: Soil Moisture Block 2.7 m Lead (514-130)

[GROUPED PRODUCT MATRIX]
Model No.
	Lead
	Desc
	N/A for this Product Group

[PRODUCT GROUP] TDR

[PRODUCT] Trase Soil Moisture Analyser (514-160/01)
With Graphic Display 150mm Wave Guide Set Power Pack & Charger

_Attributes_
Description
	Trase Soil Moisture Analyser

_Related Products_
Accessory: Alignment Block (514-169)
Spare/Consumable: Wave Guide 150mm (514-160/10)
Accessory: Wave Guides 300mm (514-162)
Accessory: Wave Guides 600mm  (514-164)
Accessory: Wave Guides 700mm  (514-165)

[PRODUCT] Wave Guide 150mm (514-160/10)
150mm

_Further Information_
Set of 2 for Trase

_Attributes_
Description
	Wave Guide 150 mm

_Related Products_
Main: Trase Soil Moisture Analyser (514-160/01)

[PRODUCT] Wave Guides 300mm (514-162)
300mm

_Further Information_
Set of 2 for Trase

_Attributes_
Description
	Wave Guide 300 mm

_Related Products_
Main: Trase Soil Moisture Analyser (514-160/01)
Accessory: Wave Guides 600mm  (514-164)
Accessory: Wave Guides 700mm  (514-165)

[PRODUCT] Wave Guides 600mm  (514-164)
600mm

_Further Information_
Set of 2 for Trase

_Attributes_
Description
	Wave Guide 600 mm

_Related Products_
Main: Trase Soil Moisture Analyser (514-160/01)
Accessory: Wave Guides 300mm (514-162)

[PRODUCT] Wave Guides 700mm  (514-165)
700mm

_Further Information_
Set of 2 for Trase

_Attributes_
Description
	Wave Guide 700 mm

_Related Products_
Main: Trase Soil Moisture Analyser (514-160/01)
Accessory: Wave Guides 300mm (514-162)

[PRODUCT] Alignment Block (514-169)
For inserting wave guides into soils.

_Attributes_
Description
	Alignment Block

_Related Products_
Main: Trase Soil Moisture Analyser (514-160/01)

[PRODUCT] Minitrase Kit with Bluetooth and Android (514-190/01)

_Attributes_
Description
	Minitrase Kit

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Tensiometers
Tensiometers are used to measure soil tension, which is directly related to the amount of soil moisture available to plants. Capillarity is established between the waterfilled tensiometers and the soil water via a ceramic cup or tip. As soil water tension increases, water is drawn by suction from the tensiometer and the negative pressure created, which is representative of soil tension, may be read from a vacuum gauge.

[PRODUCT] Quickdraw soil moisture probe 305 mm (514-010)
305 mm long

_Further Information_
Supplied with coring tool and carrying case.

_Attributes_
Description
	Soil moisture probe
	
Tensiometer Type
	Quickdraw
	
Length, mm
	305 mm
	
Weight, kg
	1

_Related Products_
Main: Quickdraw soil moisture probe 460 mm (514-012)
Spare/Consumable: Replacement Dial Gauge. (514-010/12)

[PRODUCT] Quickdraw soil moisture probe 460 mm (514-012)
460 mm long

_Further Information_
Supplied with coring tool and carrying case.

_Attributes_
Description
	Soil moisture probe
	
Tensiometer Type
	Quickdraw
	
Length, mm
	460 mm
	
Weight, kg
	1

_Related Products_
Main: Quickdraw soil moisture probe 305 mm (514-010)
Spare/Consumable: Replacement Dial Gauge. (514-010/12)

[PRODUCT] Replacement Dial Gauge. (514-010/12)

_Further Information_

_Attributes_
Description
	Dial Gauge

_Related Products_
Main: Quickdraw soil moisture probe 305 mm (514-010)
Main: Quickdraw soil moisture probe 460 mm (514-012)

[PRODUCT] Dial-Type Gauge Tensiometer 300 mm (514-020)
300 mm Long

_Further Information_
Requires Part 514-034

_Attributes_
Description
	Gauge Tensiometer
	
Tensiometer Type
	Dial-Type
	
Length, mm
	300 mm

_Related Products_
Main: Dial-Type Gauge Tensiometer 600 mm (514-022)
Main: Dial-Type Gauge Tensiometer 900 mm (514-024)
Accessory: Insertion Tool (514-030)
Accessory: Service Kit (514-034)

[PRODUCT] Dial-Type Gauge Tensiometer 600 mm (514-022)
600 mm Long

_Further Information_
Requires Part 514-034

_Attributes_
Description
	Gauge Tensiometer
	
Tensiometer Type
	Dial-Type
	
Length, mm
	600 mm

_Related Products_
Main: Dial-Type Gauge Tensiometer 300 mm (514-020)
Main: Dial-Type Gauge Tensiometer 900 mm (514-024)
Accessory: Insertion Tool (514-030)
Accessory: Service Kit (514-034)

[PRODUCT] Dial-Type Gauge Tensiometer 900 mm (514-024)
900 mm Long

_Further Information_
Requires Part 514-034

_Attributes_
Description
	Gauge Tensiometer
	
Tensiometer Type
	Dial-Type
	
Length, mm
	900 mm

_Related Products_
Main: Dial-Type Gauge Tensiometer 300 mm (514-020)
Main: Dial-Type Gauge Tensiometer 600 mm (514-022)
Accessory: Insertion Tool (514-030)
Accessory: Service Kit (514-034)

[PRODUCT] JET Fill Tensiometer 150 mm (514-035)
150mm Long

_Further Information_
Requires Part No 514-034

_Attributes_
Description
	Tensiometer
	
Tensiometer Type
	Jet Fill
	
Length, mm
	150 mm

_Related Products_
Accessory: Insertion Tool (514-030)
Main: Jet Fill Tensiometer 1220 mm (514-041)
Main: JET Fill Tensiometer 300 mm (514-036)
Main: Jet Fill Tensiometer 460 mm (514-037)
Main: Jet Fill Tensiometer 600 mm (514-038)
Main: Jet Fill Tensiometer 900 mm (514-040)
Accessory: Service Kit (514-034)
Accessory: Tensiometer Extension Tube (514-042)

[PRODUCT] JET Fill Tensiometer 300 mm (514-036)
300mm Long

_Further Information_
Requires Part No 514-034

_Attributes_
Description
	Tensiometer
	
Tensiometer Type
	Jet Fill
	
Length, mm
	300 mm

_Related Products_
Accessory: Insertion Tool (514-030)
Main: Jet Fill Tensiometer 1220 mm (514-041)
Main: JET Fill Tensiometer 150 mm (514-035)
Main: Jet Fill Tensiometer 460 mm (514-037)
Main: Jet Fill Tensiometer 600 mm (514-038)
Main: Jet Fill Tensiometer 900 mm (514-040)
Accessory: Service Kit (514-034)
Accessory: Tensiometer Extension Tube (514-042)

[PRODUCT] Jet Fill Tensiometer 460 mm (514-037)
460mm Long

_Further Information_
Requires Part No 514-034

_Attributes_
Description
	Tensiometer
	
Tensiometer Type
	Jet Fill
	
Length, mm
	460 mm

_Related Products_
Accessory: Insertion Tool (514-030)
Main: Jet Fill Tensiometer 1220 mm (514-041)
Main: JET Fill Tensiometer 150 mm (514-035)
Main: JET Fill Tensiometer 300 mm (514-036)
Main: Jet Fill Tensiometer 600 mm (514-038)
Main: Jet Fill Tensiometer 900 mm (514-040)
Accessory: Service Kit (514-034)
Accessory: Tensiometer Extension Tube (514-042)

[PRODUCT] Jet Fill Tensiometer 600 mm (514-038)
600mm Long

_Further Information_
Requires Part No 514-034

_Attributes_
Description
	Tensiometer
	
Tensiometer Type
	Jet Fill
	
Length, mm
	600 mm

_Related Products_
Accessory: Insertion Tool (514-030)
Main: JET Fill Tensiometer 150 mm (514-035)
Main: JET Fill Tensiometer 300 mm (514-036)
Main: Jet Fill Tensiometer 460 mm (514-037)
Accessory: Service Kit (514-034)
Accessory: Tensiometer Extension Tube (514-042)

[PRODUCT] Jet Fill Tensiometer 900 mm (514-040)
900mm Long

_Further Information_
Requires Part No 514-034

_Attributes_
Description
	Tensiometer
	
Tensiometer Type
	Jet Fill
	
Length, mm
	900 mm

_Related Products_
Accessory: Insertion Tool (514-030)
Main: JET Fill Tensiometer 150 mm (514-035)
Main: JET Fill Tensiometer 300 mm (514-036)
Main: Jet Fill Tensiometer 460 mm (514-037)
Accessory: Service Kit (514-034)
Accessory: Tensiometer Extension Tube (514-042)

[PRODUCT] Jet Fill Tensiometer 1220 mm (514-041)
1220mm Long

_Further Information_
Requires Part No 514-034

_Attributes_
Description
	Tensiometer
	
Tensiometer Type
	Jet Fill
	
Length, mm
	1220 mm

_Related Products_
Accessory: Insertion Tool (514-030)
Main: JET Fill Tensiometer 150 mm (514-035)
Main: JET Fill Tensiometer 300 mm (514-036)
Main: Jet Fill Tensiometer 460 mm (514-037)
Accessory: Service Kit (514-034)
Accessory: Tensiometer Extension Tube (514-042)

[PRODUCT] Insertion Tool (514-030)
To provide clearance hole and maintain hole diameter for tensiometers.

_Further Information_
1370 mm long.

_Attributes_
Description
	Insertion Tool

_Related Products_
Main: Dial-Type Gauge Tensiometer 300 mm (514-020)
Main: Dial-Type Gauge Tensiometer 600 mm (514-022)
Main: Dial-Type Gauge Tensiometer 900 mm (514-024)
Main: Jet Fill Tensiometer 1220 mm (514-041)
Main: JET Fill Tensiometer 150 mm (514-035)
Main: JET Fill Tensiometer 300 mm (514-036)
Main: Jet Fill Tensiometer 460 mm (514-037)
Main: Jet Fill Tensiometer 600 mm (514-038)
Main: Jet Fill Tensiometer 900 mm (514-040)

[PRODUCT] Service Kit (514-034)
Includes vacuum hand pump, anti-algae fluid and filling bottle.

_Attributes_
Description
	Service Kit

_Related Products_
Main: Dial-Type Gauge Tensiometer 300 mm (514-020)
Main: Dial-Type Gauge Tensiometer 600 mm (514-022)
Main: Dial-Type Gauge Tensiometer 900 mm (514-024)
Main: Jet Fill Tensiometer 1220 mm (514-041)
Main: JET Fill Tensiometer 150 mm (514-035)
Main: JET Fill Tensiometer 300 mm (514-036)
Main: Jet Fill Tensiometer 460 mm (514-037)
Main: Jet Fill Tensiometer 600 mm (514-038)
Main: Jet Fill Tensiometer 900 mm (514-040)

[PRODUCT] Tensiometer Extension Tube (514-042)
1524mm Long

_Attributes_
Description
	Tensiometer Extension Tube
	
Length, mm
	1524 mm

_Related Products_
Main: Jet Fill Tensiometer 1220 mm (514-041)
Main: JET Fill Tensiometer 150 mm (514-035)
Main: JET Fill Tensiometer 300 mm (514-036)
Main: Jet Fill Tensiometer 460 mm (514-037)
Main: Jet Fill Tensiometer 600 mm (514-038)
Main: Jet Fill Tensiometer 900 mm (514-040)

[GROUPED PRODUCT MATRIX]
Model No.
	T. Type
	Length, mm
	Desc
	N/A for this Product Group

[CATEGORY] Soil Physics

[PRODUCT GROUP] Density

[PRODUCT] Sample Ring (530-175)
53mm Outside Diameter

_Further Information_
50mm Inside Dia

_Attributes_
Description
	Sample Ring

[PRODUCT] Plastic Covers (2) for 50mm Sample Rings. (530-176)
For sample rings 53 mm.

_Further Information_
Pack of 2.

_Attributes_
Description
	Plastic Covers for 50 mm Sample Rings.

[PRODUCT] Hammering Head 50mm. (530-178)
For sample rings 53 mm.

_Attributes_
Description
	Hammering Head 50 mm

[PRODUCT] Guide Cylinder for 50mm Sample Rings. (530-179)

_Attributes_
Description
	Guide Cylinder for 50 mm Sample Rings

[PRODUCT] 24 Sample Rings 50mm Dia In Aluminium Case. (510-146)
In an aluminium case, 50 mm inside diamter, 53 mm outside diameter, 51 mm long. Includes 48 plastic end covers.

_Attributes_
Description
	Sample Rings 50 mm Dia

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Penetrometer

[PRODUCT] ELE Computerised Cone Penetrometer C/W Gps Receiver 128K (516-045)
Supplied complete with rechargeable battery, case and 64K memory.

_Attributes_
Description
	Computerised Cone Penetrometer

_Related Products_
Spare/Consumable: Spare Cone and Shaft Assembly (516-045/10)

[PRODUCT] Spare Cone and Shaft Assembly (516-045/10)

_Attributes_
Description
	Spare Cone and Shaft Assembly

_Related Products_
Main: ELE Computerised Cone Penetrometer C/W Gps Receiver 128K (516-045)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Pressure plate extractors
The pressure plate apparatus is used to determine soil water retention and suctions greater than 0.4 bar. The apparatus consists of strongly built metal chambers containing one or more ceramic plates onto which uniform soil samples are placed. Having attained maximum moisture retention (field capacity) the samples within the cells are then subjected to controlled positive air pressures and water is gradually removed. By careful control of pressure, the various equilibrium conditions of pressure and soil water tension or suction, are obtained. The air pressure is provided either from a compressor, compressed air bottle, or nitrogen bottle; but must always be routed through a manifold having pressure regulators and gauges. This versatile apparatus can be used for a variety of determinations; available water capacity, water retentivity, hydraulic conductivity, and field capacity. Results have a variety of practical applications; soil classification and soil survey, the optimisation of irrigation and drainage in improving crop yields, and the calibration of soil water measuring apparatus for field use.

[PRODUCT] O-Ring Lid Seal Pack of 2 (532-100/10)

_Attributes_
Description
	O-Ring Lid Seal

_Related Products_
Main: 5-Bar Pressure Plate Extractor. (532-100)

[PRODUCT] 1-Bar Pressure Plate Cell (532-104)

_Attributes_
Description
	1-Bar Pressure Plate Cell

_Related Products_
Accessory: 15-Bar Pressure Plate Cell. (532-120/10)
Main: 15-Bar Pressure Plate Extractor. (532-120)
Accessory: 3-Bar Pressure Plate Cell (532-106)
Accessory: 5-Bar Pressure Plate Cell (532-107)
Main: 5-Bar Pressure Plate Extractor. (532-100)

[PRODUCT] 3-Bar Pressure Plate Cell (532-106)

_Attributes_
Description
	3-Bar Pressure Plate Cell

_Related Products_
Accessory: 1-Bar Pressure Plate Cell (532-104)
Accessory: 15-Bar Pressure Plate Cell. (532-120/10)
Main: 15-Bar Pressure Plate Extractor. (532-120)
Accessory: 5-Bar Pressure Plate Cell (532-107)
Main: 5-Bar Pressure Plate Extractor. (532-100)

[PRODUCT] 5-Bar Pressure Plate Cell (532-107)

_Attributes_
Description
	5-Bar Pressure Plate Cell

_Related Products_
Accessory: 1-Bar Pressure Plate Cell (532-104)
Main: 15-Bar Pressure Plate Extractor. (532-120)
Accessory: 3-Bar Pressure Plate Cell (532-106)
Main: 5-Bar Pressure Plate Extractor. (532-100)

[PRODUCT] Hose Manifold to 5 Bar Extractor. (532-111)

_Attributes_
Description
	Hose Manifold to 5 Bar Extractor

_Related Products_
Main: 5-Bar Pressure Plate Extractor. (532-100)

[PRODUCT] Hose Manifold to 15 Bar Extractor. (532-112)

_Attributes_
Description
	Hose Manifold to 15 Bar Extractor

_Related Products_
Main: 15-Bar Pressure Plate Extractor. (532-120)

[PRODUCT] Pm Compressor 220-240V 50Hz 1Ph. (532-180/01)

_Attributes_
Description
	Compressor

_Related Products_
Accessory: Connection Set for 532-180 Series. (532-182)

[PRODUCT] Connection Set for 532-180 Series. (532-182)

_Attributes_
Description
	Connection Set

_Related Products_
Main: Pm Compressor 220-240V 50Hz 1Ph. (532-180/01)

[PRODUCT] 5-Bar Pressure Plate Extractor. (532-100)
Supplied without ceramic plate cells

_Attributes_
Description
	5-Bar Pressure Plate Extractor

_Related Products_
Accessory: 1-Bar Pressure Plate Cell (532-104)
Accessory: 3-Bar Pressure Plate Cell (532-106)
Accessory: 5-Bar Pressure Plate Cell (532-107)
Main: Hose Manifold to 5 Bar Extractor. (532-111)
Spare/Consumable: O-Ring Lid Seal Pack of 2 (532-100/10)
Accessory: Soil Sample Retaining Rings Pack of 12. (532-108)

[PRODUCT] 15-Bar Pressure Plate Extractor. (532-120)
Supplied without ceramic plate cells

_Attributes_
Description
	15-Bar Pressure Plate Extractor

_Related Products_
Accessory: 1-Bar Pressure Plate Cell (532-104)
Accessory: 3-Bar Pressure Plate Cell (532-106)
Accessory: 5-Bar Pressure Plate Cell (532-107)
Main: Hose Manifold to 15 Bar Extractor. (532-112)
Accessory: Soil Sample Retaining Rings Pack of 12. (532-108)

[PRODUCT] Low Pressure Manifold (532-110)
Precise low pressure control used to regulate pressure from compressor to extractor.

_Attributes_
Description
	Low Pressure Manifold

[PRODUCT] 15-Bar Pressure Plate Cell. (532-120/10)

_Attributes_
Description
	5-Bar Pressure Plate Cell

_Related Products_
Accessory: 1-Bar Pressure Plate Cell (532-104)
Accessory: 3-Bar Pressure Plate Cell (532-106)

[PRODUCT] Soil Sample Retaining Rings Pack of 12. (532-108)

_Attributes_
Description
	Soil Sample Retaining Rings

_Related Products_
Main: 15-Bar Pressure Plate Extractor. (532-120)
Main: 5-Bar Pressure Plate Extractor. (532-100)

[PRODUCT] Low to High Pressure Manifold Compression Type (532-128)
To regulate pressure from compressor to extractor.

_Attributes_
Description
	Low to High Pressure Manifold

[PRODUCT] Combination Manifold. (532-136)
This unit is designed for precise low pressure measurement for 15 bar extractor units, or for running 5 bar and 15 bar units simultaneously from a single pressure source. The unit is based on a combination of components from 532-110 and 532-128.

_Attributes_
Description
	Combination Manifold

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[CATEGORY] Water

[CATEGORY] Water level measurement

[PRODUCT GROUP] Water level indicators
Designed to determine water levels in wells and boreholes. The tape is lowered down the hole and the device gives a clear signal when the water level is reached.

[PRODUCT] Water Level Indicator with Audio and Light Indicator 30 m (450-008)
Fitted with 30m Tape

_Further Information_
Graduated Every 10 mm.

_Attributes_
Lead Length
	30 m

_Related Products_
Main: Water Level Indicator with Audio and Light Indicator 100 m (450-011)
Main: Water Level Indicator with Audio and Light Indicator 200 m (450-013)
Main: Water Level Indicator with Audio and Light Indicator 500 m (450-017)
Main: Water Level Indicator. with Audio and Light Indicator 60 m (450-010)

[PRODUCT] Water Level Indicator. with Audio and Light Indicator 60 m (450-010)
Fitted with 60m Tape

_Further Information_
Graduated Every 10 mm.

_Attributes_
Lead Length
	60 m

_Related Products_
Main: Water Level Indicator with Audio and Light Indicator 100 m (450-011)
Main: Water Level Indicator with Audio and Light Indicator 200 m (450-013)
Main: Water Level Indicator with Audio and Light Indicator 30 m (450-008)
Main: Water Level Indicator with Audio and Light Indicator 500 m (450-017)

[PRODUCT] Water Level Indicator with Audio and Light Indicator 100 m (450-011)
Fitted with 100m Tape

_Further Information_
Graduated Every 10 mm.

_Attributes_
Lead Length
	100 m

_Related Products_
Main: Water Level Indicator with Audio and Light Indicator 200 m (450-013)
Main: Water Level Indicator with Audio and Light Indicator 30 m (450-008)
Main: Water Level Indicator with Audio and Light Indicator 500 m (450-017)
Main: Water Level Indicator. with Audio and Light Indicator 60 m (450-010)

[PRODUCT] Water Level Indicator with Audio and Light Indicator 200 m (450-013)
Fitted with 200m Tape

_Further Information_
Graduated Every 10 mm.

_Attributes_
Lead Length
	200 m

_Related Products_
Main: Water Level Indicator with Audio and Light Indicator 100 m (450-011)
Main: Water Level Indicator with Audio and Light Indicator 30 m (450-008)
Main: Water Level Indicator with Audio and Light Indicator 500 m (450-017)
Main: Water Level Indicator. with Audio and Light Indicator 60 m (450-010)

[PRODUCT] Water Level Indicator with Audio and Light Indicator 500 m (450-017)
Fitted with 500m Tape

_Further Information_
Graduated Every 10 mm.

_Attributes_
Lead Length
	500 m

_Related Products_
Main: Water Level Indicator with Audio and Light Indicator 100 m (450-011)
Main: Water Level Indicator with Audio and Light Indicator 200 m (450-013)
Main: Water Level Indicator with Audio and Light Indicator 30 m (450-008)
Main: Water Level Indicator. with Audio and Light Indicator 60 m (450-010)

[GROUPED PRODUCT MATRIX]
Model No.
	Lead
	N/A for this Product Group

[CATEGORY] Water and sediment sampling

[PRODUCT GROUP] Water samplers
Water samplers fall into 3 main categories: those which collect an heterogeneous sample from, at or just below the water surface; those which collect a sample from a specific depth in still water; and those which collect a mid-stream sample from a river, stream or irrigation channel. The ELE selection of samplers offered covers all applications mentioned.

[PRODUCT] Tube Water Sampler. (520-200)
To collect up to 250 ml complete with stainless steel measuring tape with grip and eye (20 metres).

_Attributes_
Description
	Tube Water Sampler

[PRODUCT] Water Trap Sampler. (520-215)
This sampler is designed to be used in a flowing river or stream at any desired depth to 25 metres. The design is such that the open ends through which the water flows can be simultaneously closed thus retaining the 1250 ml sample which may then be raised to the surface. The accessories include a hand winch, 25 metres of steel wire and a depth meter. The complete set is contained in a wooden transport case with padlock.

_Further Information_
Case dimensions: 700 x 350 x 260 mm

_Attributes_
Description
	Water Trap Sampler

[PRODUCT] Combination Sampling and Measuring Outfit. (521-020)
With colour scale, water sampling bottle, plankton net, bottom sampling dredge, sounding lead and calibrated line, 20 m long marked at 1 and 5 m intervals, armoured thermometer and Secchi disc (for turbidity check).

_Further Information_
Supplied with carrying case.

_Attributes_
Description
	Combination Sampling and Measuring Outfit

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[CATEGORY] Flow measurement

[PRODUCT GROUP] Flow meters
The method used for measuring the rate of a particular flow is determined by the course rate of flow and by the nature of the flow channel. The ELE range therefore encompasses equipment for measuring the faster flows encountered in rivers and streams, down to the low rates occurring during run-off from field drains.

[PRODUCT] Miniature Current Flow Meter Wading Set for Velocities 0.03 to 5 M/S. (520-265)
For velocities 0.04 to 5.0 metres/second. Consisting of current meter, revolution counter, wading rods, base and knob, 3 metres wading cable.

_Further Information_
All packed into carrying case 850 x 180 x 220 mm.

_Attributes_
Description
	Miniature Current Flow Meter
	
Velocity Range
	0.03 - 5 m/s

_Related Products_
Accessory: Pc Download Cable for Current Flow Meter. (520-261)

[PRODUCT] Large Current Flow Meter Wading Set for Velocities 0.03 to 10 M/S. (520-260)
Consisting of current meter, revolution counter, wading rods, base and knob, 3 metres wading cable. All packed into carrying case.

_Further Information_
Case dimensions: 850 x 180 x 220 mm

_Attributes_
Description
	Large Current Flow Meter
	
Velocity Range
	0.03 - 10 m/s

_Related Products_
Accessory: Pc Download Cable for Current Flow Meter. (520-261)

[PRODUCT] Pc Download Cable for Current Flow Meter. (520-261)

_Attributes_
Description
	PC Download Cable

_Related Products_
Main: Large Current Flow Meter Wading Set for Velocities 0.03 to 10 M/S. (520-260)
Main: Miniature Current Flow Meter Wading Set for Velocities 0.03 to 5 M/S. (520-265)

[GROUPED PRODUCT MATRIX]
Model No.
	Velocity Range
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Gauging weirs and flumes
Water is a precious agricultural resource. Careful monitoring is essential to ensure that it is used as effectively as possible. The comprehensive rang of equipment offered has been specifically designed to measure or estimate the mass flow in both natural, or man-made, irrigation and drainage channels.

[PRODUCT] Simple Cut-Throat Flume 100mm Throat. (520-345)
Throat width 100mm, for measuring flows in the range 0 to 15 litres/second.

_Attributes_
Description
	Cut-Throat Flume

[PRODUCT] Parshall Flume - Small. (520-360)
Having a throat width of 25 mm for flows 0.3 to 5 litres/second.

_Further Information_
Overall dimensions 710 x 360 x 270 mm.

_Attributes_
Description
	Parshall Flume - Small

[PRODUCT] Parshall Flume - Large. (520-365)
Having a throat width of 50 mm for flows 0.5 to 14 litres/second.

_Further Information_
Overall dimensions 860 x 420 x 305 mm.

_Attributes_
Description
	Parshall Flume - Large

[PRODUCT] Wsc Flume - Small. (520-375)
For flows 0.1 to 2 litres/second.

_Further Information_
Overall dimensions 500 x 250 x 175 mm.

_Attributes_
Description
	WSC Flume - Small

[PRODUCT] Wsc Flume - Large. (520-380)
For flows 1 to 7.5 litres/second.

_Further Information_
Overall dimensions 780 x 350 x 230 mm.

_Attributes_
Description
	WSC Flume - Large

[PRODUCT] Weir Plate Set with Weir Plate Carrier and Four Interchangeable Weir Plates (520-390)
1200 mm wide x 750 mm high x 5 mm thick

_Attributes_
Description
	Weir Plate Set

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[CATEGORY] Water quality testing

[PRODUCT GROUP] Comparator reagents
Where only a few chemical tests need to be done and accuracy is less important it is cost-effective to use a colour comparator. These units can be used to perform the following tests: Ammonia, Chlorine, Iron, Nitrate, Manganese and pH.

[PRODUCT] Chlorine Starter Pack Including Colour Disk and Reagents. Sufficient for 50 Tests. (432-032)

_Attributes_
Description
	Chlorine Starter Pack

_Specification_
Measurement Range
	0-4.0 mg/l

[PRODUCT] Chlorine Reagent Pack for Comparator. Sufficient for 250 tests. (432-032/10)

_Attributes_
Description
	Chlorine Reagent Refill Pack

_Specification_
Measurement Range

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Microbiological starter packs and consumables

[PRODUCT] Coliform Starter Pack. Sufficient for 200 Tests (422-010)
Sufficient for 200 tests. Comprising 200 grid membranes and absorbent pads, one pad dispenser and 38.1 grmas membrane Lauryl Sulphate broth.

_Attributes_
Description
	Coliform Starter Pack

_Related Products_
Spare/Consumable: Membrane Lauryl Sulphate Medium 38.1 Gram Pack. Sufficient for 200 Tests. (422-110)
Spare/Consumable: Pad Dispenser. (422-515)
Main: Paqualab lightweight System 25L for analysis of drinking water to EC Staandard Categories 1 & 2 (418-100)
Main: Paqualab System 25 for Analysis of Drinking Water to Ec Standard Categories 1 & 2. (418-150)
Main: Paqualab System 50 for Analysis of Drinking Water to Ec Standard Categories 1 & 2. (418-160)
Spare/Consumable: Sterile Filter Membranes and ABSorbent Pads. Pack of 200. (422-508)

[PRODUCT] Faecal Streptococci Starter Pack Sufficient for 200 Tests. (422-020)
Suitable for 200 tests. Comprising 200 grid membranes and 200 sterile plastic Petri dishes, 100 grams Slanetz and Bartley medium.

_Attributes_
Description
	Faecal Streptococci Starter Pack

[PRODUCT] Membrane Lauryl Sulphate Medium 38.1 Gram Pack. Sufficient for 200 Tests. (422-110)
38.1 grams to make approximately 500 ml medium (200 tests).

_Attributes_
Description
	Membrane Lauryl Sulphate Medium Pack

_Related Products_
Spare/Consumable: Coliform Starter Pack. Sufficient for 200 Tests (422-010)
Main: Paqualab lightweight System 25L for analysis of drinking water to EC Staandard Categories 1 & 2 (418-100)
Main: Paqualab System 25 for Analysis of Drinking Water to Ec Standard Categories 1 & 2. (418-150)
Main: Paqualab System 50 for Analysis of Drinking Water to Ec Standard Categories 1 & 2. (418-160)

[PRODUCT] Slanetz and Bartley Medium. 21G Pack. Sufficient for 200 Tests. (422-120)
100 grams to make up to approximately 200 tests.

_Attributes_
Description
	Slanetz and Bartley Medium Pack

[PRODUCT] Sterile Filter Membranes and ABSorbent Pads. Pack of 200. (422-508)
Pack of 200.

_Attributes_
Description
	Sterile Filter Membranes and Absorbent Pads x200

_Related Products_
Spare/Consumable: Coliform Starter Pack. Sufficient for 200 Tests (422-010)
Main: Paqualab lightweight System 25L for analysis of drinking water to EC Staandard Categories 1 & 2 (418-100)
Main: Paqualab System 25 for Analysis of Drinking Water to Ec Standard Categories 1 & 2. (418-150)
Main: Paqualab System 50 for Analysis of Drinking Water to Ec Standard Categories 1 & 2. (418-160)

[PRODUCT] Sterile Filter Membranes and ABSorbent Pads. Pack of 1000. (422-510)
Pack of 1000.

_Attributes_
Description
	Sterile Filter Membranes and Absorbent Pads x1000

[PRODUCT] Pad Dispenser. (422-515)

_Attributes_
Description
	Pad Dispenser

_Related Products_
Spare/Consumable: Coliform Starter Pack. Sufficient for 200 Tests (422-010)
Main: Paqualab lightweight System 25L for analysis of drinking water to EC Staandard Categories 1 & 2 (418-100)
Main: Paqualab System 25 for Analysis of Drinking Water to Ec Standard Categories 1 & 2. (418-150)
Main: Paqualab System 50 for Analysis of Drinking Water to Ec Standard Categories 1 & 2. (418-160)

[PRODUCT] Aluminium Petri Dishes Pack of 25. (422-560)
Reusable pack of 25.

_Attributes_
Description
	Aluminium Petri Dishes

_Related Products_
Main: Paqualab lightweight System 25L for analysis of drinking water to EC Staandard Categories 1 & 2 (418-100)
Main: Paqualab System 25 for Analysis of Drinking Water to Ec Standard Categories 1 & 2. (418-150)
Main: Paqualab System 50 for Analysis of Drinking Water to Ec Standard Categories 1 & 2. (418-160)

[PRODUCT] Sterile Plastic Petri Dishes. Pack of 200. (422-569)
Pack of 200.

_Attributes_
Description
	Sterile Plastic Petri Dishes x200

[PRODUCT] Sterile Plastic Petri Dishes. Pack of 700. (422-570)
Pack of 700.

_Attributes_
Description
	Sterile Plastic Petri Dishes x700

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Paqualab Portable Incubators & Filtration Unit
The ELE Paqualab incubators are fully portable which enables microbiological water analysis to be carried out in remote locations which lack normal laboratory facilities. Various power supply options are available including internal rechargeable batteries or an external 12V DC, 24V DC, 110V AC, or 240V AC supply. This flexibility means that samples can be incubated on-site, in a car or in a laboratory so producing accurate results in the shortest possible time.

[PRODUCT] Paqualab Incubator 50:- Dual Incubator Filtra- Tion Unit 50 Al Petri Dishes (420-035)
The ELE Paqualab 50 includes two incubators - the standard and universal (each with 2 pre-set temperatures, normally 37°C and 44°C), a membrane filtration unit, microbiological accessories kit, connecting cables and operating manual. All components are housed in a convenient rigid carrying case which can also accomodate a number of electronic meters from the ELE Paqualab range.

_Further Information_
The system will operate on 12 V or 24 V DC, 110 V or 240 V AC, or the internal 12 V rechargeable battery supplied.

_Attributes_
Description
	Paqualab Incubator 50

_Related Products_
Spare/Consumable: Filtration Unit Al Construction Complete with Sampling Cup. (420-450)

[PRODUCT] Paqualab Incubator 25:- Single Incubator Filtration Unit 25 Al Petri Dishes (420-030)
The ELE Paqualab 25 includes a universal incubator with 2 pre-set temperatures (normally 37°C and 44°C), a membrane filtration kit, connecting cables and operating manual. All components are housed in a convenient rigid carrying case which can also accomodate a number of electronic meters from the ELE Paqualab range.

_Further Information_
The system will operate on 12 V or 24 V DC, 110 V or 240 V AC, or the internal 12 V rechargeable battery supplied.

_Attributes_
Description
	Paqualab Incubator 25

_Related Products_
Spare/Consumable: Filtration Unit Al Construction Complete with Sampling Cup. (420-450)

[PRODUCT] Filtration Unit Al Construction Complete with Sampling Cup. (420-450)
 	* Anodised Aluminium Membrane Filtration Unit.  	* Light compact and field sterilisable.  	* Fits together for storage into a size 120 mm high x 80 mm diameter.  	* Supplied with sampling cup and nylon cord.  	* Filtration unit graduated with 50 ml and 100 ml levels.  	* Supplied with hand-operated suction pump.

_Attributes_
Description
	Filtration Unit

_Related Products_
Main: Paqualab Incubator 25:- Single Incubator Filtration Unit 25 Al Petri Dishes (420-030)
Main: Paqualab Incubator 50:- Dual Incubator Filtra- Tion Unit 50 Al Petri Dishes (420-035)
Main: Paqualab lightweight System 25L for analysis of drinking water to EC Staandard Categories 1 & 2 (418-100)
Main: Paqualab System 25 for Analysis of Drinking Water to Ec Standard Categories 1 & 2. (418-150)
Main: Paqualab System 50 for Analysis of Drinking Water to Ec Standard Categories 1 & 2. (418-160)
Spare/Consumable: Spare Parts Kit for Filtration Unit. (420-451)

[PRODUCT] Spare Parts Kit for Filtration Unit. (420-451)
For filtration unit (filter disc, gasket kit and 0-ring).

_Attributes_
Description
	Spare Parts Kit for Filtration Unit

_Related Products_
Spare/Consumable: Filtration Unit Al Construction Complete with Sampling Cup. (420-450)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Paqualab Standard Systems
The three Paqualab systems are designed so that all the necessary equipment to determine the physical, chemical and microbiological parameters can be stored in one easily carried case. Results are obtained within 16 hours. The numerical results have precision and reproducibility. The method is simple and economical enabling regular analysis to be carried out. This technique is accepted worldwide and Paqualabs are used in over 50 countries. Reusable components can be sterilised in the field. Consumables are pre-sterilised and have a long shelf life. Sample deterioration through transport and handling is eliminated.

[PRODUCT] Paqualab System 50 for Analysis of Drinking Water to Ec Standard Categories 1 & 2. (418-160)
Comprising the ELE Paqualab incubator 50, pH/temperature/mV meter, conductivity/temperature meter, turbidity meter, 0 - 50 NTU, ELE Paqualab photometer, and consumables for 200 tests on faecal or total coliforms, chlorine, ammonia, nitrates and nitrites.

_Further Information_
Overall dimensions 475 x 230 x 275 mm.

_Attributes_
Description
	Paqualab System 50

_Related Products_
Spare/Consumable: Aluminium Petri Dishes Pack of 25. (422-560)
Spare/Consumable: Coliform Starter Pack. Sufficient for 200 Tests (422-010)
Spare/Consumable: Filtration Unit Al Construction Complete with Sampling Cup. (420-450)
Spare/Consumable: Membrane Lauryl Sulphate Medium 38.1 Gram Pack. Sufficient for 200 Tests. (422-110)
Spare/Consumable: Pad Dispenser. (422-515)
Main: Paqualab lightweight System 25L for analysis of drinking water to EC Staandard Categories 1 & 2 (418-100)
Main: Paqualab System 25 for Analysis of Drinking Water to Ec Standard Categories 1 & 2. (418-150)
Spare/Consumable: Sterile Filter Membranes and ABSorbent Pads. Pack of 200. (422-508)

[PRODUCT] Paqualab System 25 for Analysis of Drinking Water to Ec Standard Categories 1 & 2. (418-150)
Including the incubator 25, pH/temperature/pH meter, conductivity/temperature meter, turbidity meter 0 - 50 NTU, ELE Paqualab photometer and consumables for 200 tests on faecal or total coliforms, chlorine, ammonia, nitrates and nitrites.

_Further Information_
Overall dimensions 335 x 230 x 275 mm

_Attributes_
Description
	Paqualab System 25

_Related Products_
Spare/Consumable: Aluminium Petri Dishes Pack of 25. (422-560)
Spare/Consumable: Coliform Starter Pack. Sufficient for 200 Tests (422-010)
Spare/Consumable: Filtration Unit Al Construction Complete with Sampling Cup. (420-450)
Spare/Consumable: Membrane Lauryl Sulphate Medium 38.1 Gram Pack. Sufficient for 200 Tests. (422-110)
Spare/Consumable: Pad Dispenser. (422-515)
Main: Paqualab lightweight System 25L for analysis of drinking water to EC Staandard Categories 1 & 2 (418-100)
Main: Paqualab System 50 for Analysis of Drinking Water to Ec Standard Categories 1 & 2. (418-160)
Spare/Consumable: Sterile Filter Membranes and ABSorbent Pads. Pack of 200. (422-508)

[PRODUCT] Paqualab lightweight System 25L for analysis of drinking water to EC Staandard Categories 1 & 2 (418-100)
Including the incubator 25L, conductivity/temperature/mV meter, turbidity tube 5 - 500 JTU, ELE Paqualab photometer and consumables for 200 tests on faecal or total coliforms, chlorine and pH.

_Further Information_
Includes a lightweight carrying case, dimensions 380 x 180 x 230 mm.

_Attributes_
Description
	Paqualab Lightweight System 25L

_Related Products_
Spare/Consumable: Aluminium Petri Dishes Pack of 25. (422-560)
Spare/Consumable: Coliform Starter Pack. Sufficient for 200 Tests (422-010)
Spare/Consumable: Filtration Unit Al Construction Complete with Sampling Cup. (420-450)
Spare/Consumable: Membrane Lauryl Sulphate Medium 38.1 Gram Pack. Sufficient for 200 Tests. (422-110)
Spare/Consumable: Pad Dispenser. (422-515)
Main: Paqualab System 25 for Analysis of Drinking Water to Ec Standard Categories 1 & 2. (418-150)
Main: Paqualab System 50 for Analysis of Drinking Water to Ec Standard Categories 1 & 2. (418-160)
Spare/Consumable: Sterile Filter Membranes and ABSorbent Pads. Pack of 200. (422-508)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Paqualab Test Meters

[PRODUCT] Digital Ph/Temp/Mv Meter. with Electodes Carrying Case and Ph Buffers. (430-020)

_Attributes_
Description
	Digital Ph/Temp/Mv Meter

[PRODUCT] Conductivity/Temp/Tds Meter with Electrode and Carrying Case (513-160)

_Attributes_
Description
	Conductivity/Temp/TDS Meter

[PRODUCT] Dissolved Oxygen / Temp Meter. with Electrode and Carrying Case (521-050)

_Attributes_
Description
	Dissolved Oxygen/Temp Meter

[PRODUCT] Turbidity Meter. Range 0-1000 Ftu. Supplied with Carrying Case Batteries and Calibration Solutions (430-260)

_Attributes_
Description
	Turbidity Meter

[PRODUCT] Paqualab Photometer Complete with Six Test Tubes Dilution Tube Operating Manual and Carrying Case. (430-550)
Comprising photometer unit as described with built-in filters, dilution tube, six glass test tubes, operating instructions and moulded plastic carrying case with space to hold up to four different reagent systems.

_Further Information_
Test reagent tablets are not supplied.

_Attributes_
Description
	Photometer

[PRODUCT] Standard Colour Comparator Kit In Carrying Case. Supplied Without Colour Disks and Reagents. (432-020)

_Attributes_
Description
	Comparator Kit

[PRODUCT] Water Test Kit. Includes Tests for Ph Chloride Total Hardness and Iron. (521-080)
For pH, chloride, hardness and iron. Supplied complete in a carrying case with reagents for 50 tests of each parameter.

_Attributes_
Description
	Water Test Kit

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Photometer Reagents
Over 40 different water tests are available. The chemical reagents required for each water test are compressed into stable tablet form eliminating the possible errors that can result when measuring out chemical solutions.

[PRODUCT] Alkalinity Reagent System Methyl or ange End Point 0-500Mg/Litre. Sufficient for 50 Tests. (433-094)
Natural and treated waters contain a variety of dissolved alkaline substances (e.g bicarbonate).

_Attributes_
Description
	Alkalinity Methyl Orange
	
Measurement Range
	0-500 mg/litre
	
Pack Size
	50

_Specification_
Measurement Range

[PRODUCT] Alkalinity Reagent Pack Methyl Orange End Point. Sufficient for 250 tests. (433-094/10)
Natural and treated waters contain a variety of dissolved alkaline substances (e.g bicarbonate).

_Attributes_
Description
	Alkalinity Methyl Orange
	
Measurement Range
	0-500 mg/litre
	
Pack Size
	250

_Specification_
Measurement Range

[PRODUCT] Alkalinity Reagent System Phenolphthalein End Point 0-500Mg/Litre. Sufficient for 50 Tests. (433-096)
Natural and treated waters contain a variety of dissolved alkaline substances (e.g bicarbonate).

_Attributes_
Description
	Alkalinity Phenolphthalein
	
Measurement Range
	0-500 mg/litre
	
Pack Size
	50

_Specification_
Measurement Range

[PRODUCT] Alkalinity Reagent Pack Phenolphthalein End Point Sufficient for 250 Tests. (433-096/10)
Natural and treated waters contain a variety of dissolved alkaline substances (e.g bicarbonate).

_Attributes_
Description
	Alkalinity Phenolphthalein
	
Measurement Range
	0-500 mg/litre
	
Pack Size
	250

_Specification_
Measurement Range

[PRODUCT] Alkalinity Reagent System 0-500Mg/Litre. Sufficient for 50 Tests. (433-098)
Natural and treated waters contain a variety of dissolved alkaline substances (e.g bicarbonate).

_Attributes_
Description
	Alkalinity
	
Measurement Range
	0-500 mg/litre
	
Pack Size
	50

_Specification_
Measurement Range
	0-500 mg/l CaCO3

[PRODUCT] Alkalinity Reagent Pack for 250 Tests (433-098/10)
Natural and treated waters contain a variety of dissolved alkaline substances (e.g bicarbonate).

_Attributes_
Description
	Alkalinity
	
Measurement Range
	0-500 mg/litre
	
Pack Size
	250

_Specification_
Measurement Range
	0-500 mg/l CaCO3

[PRODUCT] Aluminium Reagent System 0 - 0.5Mg/Litre. Sufficient for 50 Tests. (433-100)
Aluminium salts are found in natural waters. High levels can be toxic to fish. Aluminium Sulphate is used in drinking water treatment.

_Attributes_
Description
	Aluminium
	
Measurement Range
	0 - 0.5 mg/litre
	
Pack Size
	50

_Specification_
Measurement Range
	0-0.5 mg/l

[PRODUCT] Aluminium Reagent Pack Sufficient for 250 Tests. (433-100/10)
Aluminium salts are found in natural waters. High levels can be toxic to fish. Aluminium Sulphate is used in drinking water treatment.

_Attributes_
Description
	Aluminium
	
Measurement Range
	0 - 0.5 mg/litre
	
Pack Size
	250

_Specification_
Measurement Range
	0-0.5 mg/l

[PRODUCT] Ammonia Reagent System 0 - 1.0Mg/Litre. Sufficient for 50 Tests. (433-102)
Occurs when nitrogenous products break down in water. Ammonia is harmful to aquatic life, particularly fish.

_Attributes_
Description
	Ammonia
	
Measurement Range
	0 - 1.0 mg/litre
	
Pack Size
	50

_Specification_
Measurement Range
	0-1.0 mg/l N

[PRODUCT] Ammonia Reagent Pack Sufficient for 250 Tests. (433-102/10)
Occurs when nitrogenous products break down in water. Ammonia is harmful to aquatic life, particularly fish.

_Attributes_
Description
	Ammonia
	
Measurement Range
	0 - 1.0 mg/litre
	
Pack Size
	250

_Specification_
Measurement Range
	0-1.0 mg/l N

[PRODUCT] Bromine Reagent System 0 - 6.0Mg/Litre Sufficient for 50 Tests. (433-105)
A powerful disinfectant used for water treatment and swimming pool management.

_Attributes_
Description
	Bromine
	
Measurement Range
	0 - 6.0 mg/litre
	
Pack Size
	50

_Specification_
Measurement Range
	0-6.0 mg/l

[PRODUCT] Bromine Reagent Pack Sufficient for 250 tests. (433-105/10)
A powerful disinfectant used for water treatment and swimming pool management.

_Attributes_
Description
	Bromine
	
Measurement Range
	0 - 6.0 mg/litre
	
Pack Size
	250

_Specification_
Measurement Range
	0-6.0 mg/l

[PRODUCT] Calcium Hardness Reagent System 0-500Mg/Litre. Sufficient for 50 Tests. (433-108)

_Attributes_
Description
	Calcium Hardness
	
Measurement Range
	0-500 mg/litre
	
Pack Size
	50

_Specification_
Measurement Range

[PRODUCT] Chloride Reagent System 0-50,000Mg/Litre NaCl Sufficient for 50 Tests. (433-110)
Total Chlorine Test. High levels of Chlorine are used to disinfect or sterilise water distribution systems.

_Attributes_
Description
	Chloride
	
Measurement Range
	0-50,000 mg/litre
	
Pack Size
	50

_Specification_
Measurement Range

[PRODUCT] Chloride Reagent Pack. Sufficient for 250 Tests. (433-110/10)
Total Chlorine Test. High levels of Chlorine are used to disinfect or sterilise water distribution systems.

_Attributes_
Description
	Chloride
	
Measurement Range
	0-50,000Mg/Litre
	
Pack Size
	250

_Specification_
Measurement Range

[PRODUCT] Chlorine (Dpd No. 1) Free Chlorine Reagent System 0-5Mg/L. Sufficient for 50 Tests. (433-112)
Free, total and combined Chlorine test. Chlorine is used for the disinfection of drinking water and swimming pools.

_Attributes_
Description
	Chlorine DPD
	
Measurement Range
	0-5 mg/litre
	
Pack Size
	50

_Specification_
Measurement Range

[PRODUCT] Chlorine (Dpd No.1) Free Chlorine 0-5Mg/L Reagent System. Sufficient for 250 Tests. (433-112/10)
Free, total and combined Chlorine test. Chlorine is used for the disinfection of drinking water and swimming pools.

_Attributes_
Description
	Chlorine DPD
	
Measurement Range
	0-5 mg/litre
	
Pack Size
	250

_Specification_
Measurement Range

[PRODUCT] Chlorine Reagent System Free Combined and Total 0 - 5.0Mg/Litre Sufficient for 50 Tests (433-115)
Total Chlorine Test. High levels of Chlorine are used to disinfect or sterilise water distribution systems.

_Attributes_
Description
	Chlorine
	
Measurement Range
	0 - 5 mg/litre
	
Pack Size
	50

_Specification_
Measurement Range
	0-5.0 mg/l

[PRODUCT] Chlorine Reagent Pack Sufficient for 250 Tests. (433-115/10)
Total Chlorine Test. High levels of Chlorine are used to disinfect or sterilise water distribution systems.

_Attributes_
Description
	Chlorine
	
Measurement Range
	0-5 mg/litre
	
Pack Size
	250

_Specification_
Measurement Range
	0-5.0 mg/l

[PRODUCT] Chlorine Hr Reagent System Total 0-250Mg/ Litre. Sufficient for 50 Tests. (433-118)
Total Chlorine Test. High levels of Chlorine are used to disinfect or sterilise water distribution systems.

_Attributes_
Description
	Chlorine Hr
	
Measurement Range
	0-250 mg/litre
	
Pack Size
	50

_Specification_
Measurement Range
	0-250 mg/l

[PRODUCT] Chlorine Hr Reagent Pack Sufficient for 250 Tests. (433-118/10)
Total Chlorine Test. High levels of Chlorine are used to disinfect or sterilise water distribution systems.

_Attributes_
Description
	Chlorine Hr
	
Measurement Range
	0-250 mg/litre
	
Pack Size
	250

_Specification_
Measurement Range
	0-250 mg/l

[PRODUCT] Chromium Vi Reagent System 0-1.0Mg/Litre. Sufficient for 50 Tests. (433-120)

_Attributes_
Description
	Chromium Vi
	
Measurement Range
	0-1 mg/litre
	
Pack Size
	50

_Specification_
Measurement Range

[PRODUCT] Chromium III Reagent System 0-1.0mg/litre. Sufficient for 50 tests. (433-122)

_Attributes_
Description
	Chromium III
	
Measurement Range
	0-1 mg/litre
	
Pack Size
	50

_Specification_
Measurement Range

[PRODUCT] Colour Test System for Photometer. Range 10 to 500 Hazen Colour Units. (433-125)

_Attributes_
Description
	Colour Test System
	
Measurement Range
	10 to 500 Hazen Colour Units.
	
Pack Size
	50

_Specification_
Measurement Range

[PRODUCT] Copper Reagent System Total Free and Chelated 0-5.0Mg/Litre. Sufficient for 50 Tests. (433-130)
Occurs naturally in water, may cause discolouration and an astringent taste. Sometimes used as an algicide.

_Attributes_
Description
	Copper
	
Measurement Range
	0-5 mg/litre
	
Pack Size
	50

_Specification_
Measurement Range
	0-4.0 mg/l

[PRODUCT] Copper Reagent Pack Sufficient for 250 tests (433-130/10)
Occurs naturally in water, may cause discolouration and an astringent taste. Sometimes used as an algicide.

_Attributes_
Description
	Copper
	
Measurement Range
	0-5 mg/litre
	
Pack Size
	250

_Specification_
Measurement Range
	0-4.0 mg/l

[PRODUCT] Cyanuric Acid Reagent System 0-200Mg/Litre. Sufficient for 50 Tests. (433-134)
Used as a Chlorine stabiliser in swimming pool water treatment.

_Attributes_
Description
	Cyanuric Acid
	
Measurement Range
	0-200 mg/litre
	
Pack Size
	50

_Specification_
Measurement Range
	0-200 mg/l

[PRODUCT] Dissolved Oxygen Reagent Pack. Sufficient for 30 Tests. (433-136/10)

_Attributes_
Description
	Dissolved Oxygen
	
Measurement Range
	0-2 mg/litre
	
Pack Size
	30

_Specification_
Measurement Range

[PRODUCT] Fluoride Reagent System 0-1.5Mg/Litre. Sufficient for 50 Tests. (433-138)
Found naturally in some waters, but more usually introduced into drinking water to prevent tooth decay.

_Attributes_
Description
	Fluoride
	
Measurement Range
	0-1.5 mg/litre
	
Pack Size
	50

_Specification_
Measurement Range
	0-1.5 mg/l

[PRODUCT] Total Hardness Reagent System 0-500Mg/Litre. Sufficient for 50 Tests. (433-139)

_Attributes_
Description
	Total Hardness
	
Measurement Range
	0-500 mg/litre
	
Pack Size
	50

_Specification_
Measurement Range

[PRODUCT] Total Hardness Reagent Pack. Sufficient for 250 Tests. (433-139/10)

_Attributes_
Description
	Total Hardness
	
Measurement Range
	0-500 mg/litre
	
Pack Size
	250

_Specification_
Measurement Range

[PRODUCT] Hydrazine Reagent System 0-0.5Mg/Litre. Sufficient for 50 Tests. (433-141)

_Attributes_
Description
	Hydrazine
	
Measurement Range
	0-0.5 mg/litre
	
Pack Size
	50

_Specification_
Measurement Range

[PRODUCT] Hydrazine Reagent Pack, Sufficient for 150 tests (433-141/10)

_Attributes_
Description
	Hydrazine
	
Measurement Range
	0-0.5Mg/Litre
	
Pack Size
	150

_Specification_
Measurement Range

[PRODUCT] Hydrogen Peroxide Lr Reagent System 0-2.0Mg/ Litre. Sufficient for 50 Tests. (433-142)
Used in water treatment processes.

_Attributes_
Description
	Hydrogen Peroxide Lr
	
Measurement Range
	0-2 mg/litre
	
Pack Size
	50

_Specification_
Measurement Range
	0-2.0 mg/l

[PRODUCT] Hydrogen Peroxide Reagent System 0-100Mg/Litre. Sufficient for 50 Tests. (433-146)
Used in water treatment processes.

_Attributes_
Description
	Hydrogen Peroxide
	
Measurement Range
	0-100 mg/litre
	
Pack Size
	50

_Specification_
Measurement Range
	0-100 mg/l

[PRODUCT] Iron Lr Reagent Pack Sufficient for 250 Tests. (433-150/10)
Widely found in natural water. Affects the taste of water and casues staining. Insoluble iron deposits can cause small pipes to block.

_Attributes_
Description
	Iron Lr
	
Measurement Range
	0-1 mg/litre
	
Pack Size
	250

_Specification_
Measurement Range
	0-1.0 mg/l

[PRODUCT] Iron Mr Reagent System 0-5Mg/L. Sufficient for 50 Tests. (433-151)

_Attributes_
Description
	Iron Mr
	
Measurement Range
	0-5 mg/litre
	
Pack Size
	50

_Specification_
Measurement Range

[PRODUCT] Iron MR Reagent Pack. Sufficient for 250 tests. (433-151/10)

_Attributes_
Description
	Iron Mr
	
Measurement Range
	0-5 mg/litre
	
Pack Size
	250

_Specification_
Measurement Range

[PRODUCT] Iron Hr Reagent Pack. Sufficient for 250 Tests. (433-152/10)
In industry, higher levels of Iron may occur due to corrosion or as a result of industrial processes.

_Attributes_
Description
	Iron Hr
	
Measurement Range
	0-5 mg/litre
	
Pack Size
	250

_Specification_
Measurement Range
	0-10 mg/l

[PRODUCT] Magnesium Reagent System 0-100Mg/Litre. Sufficient for 50 Tests. (433-154)
Magnesium salts contribute to the hardness of water.

_Attributes_
Description
	Magnesium
	
Measurement Range
	0-100 mg/litre
	
Pack Size
	50

_Specification_
Measurement Range
	0-100 mg/l

[PRODUCT] Magnesium Reagent Pack. Sufficient for 250 Tests. (433-154/10)
Magnesium salts contribute to the hardness of water.

_Attributes_
Description
	Magnesium
	
Measurement Range
	0-100 mg/litre
	
Pack Size
	250

_Specification_
Measurement Range
	0-100 mg/l

[PRODUCT] Manganese Reagent System 0-0.03Mg/L. Sufficient for 50 Tests. (433-156)
Commonly found in many natural waters. Causes staining to laundry and plumbing fittings.

_Attributes_
Description
	Manganese
	
Measurement Range
	0-0.03 mg/litre
	
Pack Size
	50

_Specification_
Measurement Range
	0-0.03 mg/l

[PRODUCT] Manganese Reagent Pack 0-0.03Mg/L. Sufficient for 250 Tests. (433-156/10)
Commonly found in many natural waters. Causes staining to laundry and plumbing fittings.

_Attributes_
Description
	Manganese
	
Measurement Range
	0-0.03 mg/litre
	
Pack Size
	250

_Specification_
Measurement Range
	0-0.03 mg/l

[PRODUCT] Nickel Reagent Pack. Sufficient for 200 tests. (433-164/10)

_Attributes_
Description
	Nickel
	
Measurement Range
	0-10 mg/litre
	
Pack Size
	200

_Specification_
Measurement Range

[PRODUCT] Nitrate Reagent System 0-20Mg/Litre. Sufficient for 50 Tests. (433-166)
Nitrates are found in many natural and waste waters. They originate from chemical fertilisers, breakdown of vegetation and the oxidation of nitrogen compounds in effluents.

_Attributes_
Description
	Nitrate
	
Measurement Range
	0-20 mg/litre
	
Pack Size
	50

_Specification_
Measurement Range
	0-1.0 mg/l

[PRODUCT] Nitrate Reagent Pack. Sufficient for 200 Tests. (433-166/10)
Nitrates are found in many natural and waste waters. They originate from chemical fertilisers, breakdown of vegetation and the oxidation of nitrogen compounds in effluents.

_Attributes_
Description
	Nitrate
	
Measurement Range
	0-20 mg/litre
	
Pack Size
	200

_Specification_
Measurement Range
	0-1.0 mg/l

[PRODUCT] Nitrite Reagent System 0-0.5Mg/Litre. Sufficient for 50 Tests. (433-168)
Nitrites are an intermediate product in the nitrogen cycle. Nitrites are harmful to fish and aquatic organisms.

_Attributes_
Description
	Nitrite
	
Measurement Range
	0-0.5 mg/litre
	
Pack Size
	50

_Specification_
Measurement Range
	0-0.5 mg/l

[PRODUCT] Nitrite Reagent Pack Sufficient for 250 Tests. (433-168/10)
Nitrites are an intermediate product in the nitrogen cycle. Nitrites are harmful to fish and aquatic organisms.

_Attributes_
Description
	Nitrite
	
Measurement Range
	0-0.5 mg/litre
	
Pack Size
	250

_Specification_
Measurement Range
	0-0.5 mg/l

[PRODUCT] or ganophosphonate Reagent System 0-20Mg/Litre. Sufficient for 50 Tests. (433-170)

_Attributes_
Description
	Organophosphonate
	
Measurement Range
	0-20 mg/litre
	
Pack Size
	50

_Specification_
Measurement Range

[PRODUCT] Ozone Reagent Pack, Sufficient for 250 tests (433-172/10)
Ozone is used in water treatment and swimming pool water disinfection.

_Attributes_
Description
	Ozone
	
Measurement Range
	0-2 mg/litre
	
Pack Size
	250

_Specification_
Measurement Range
	0-2.0 mg/l

[PRODUCT] Ph Reagent System 6.8-8.4. Sufficient for 50 Tests. (433-180)
Uses the phenol red method to determine hydrogen ion activity.

_Attributes_
Description
	pH
	
Measurement Range
	6.8-8.4 pH
	
Pack Size
	50

_Specification_
Measurement Range
	6.8-8.4

[PRODUCT] Calcium Hardness Reagent Pack. Sufficient for 250 Tests. (433-180/10)

_Attributes_
Description
	Calcium Hardness
	
Measurement Range
	0-500 mg/litre
	
Pack Size
	250

_Specification_
Measurement Range

Measurement Range
	6.8-8.4

[PRODUCT] Phenol Reagent System 0-5Mg/Litre. Sufficient for 50 Tests. (433-182)

_Attributes_
Description
	Phenol
	
Measurement Range
	0-5 mg/litre
	
Pack Size
	50

_Specification_
Measurement Range

[PRODUCT] Phenol Reagent Pack. Sufficient for 250 Tests. (433-182/10)

_Attributes_
Description
	Phenol
	
Measurement Range
	0-5 mg/litre
	
Pack Size
	250

_Specification_
Measurement Range

[PRODUCT] Phosphate Lr Reagent System 0-4.0Mg/Litre. Sufficient for 50 Tests. (433-186)
Used extensively in food processing. Also present in many detergents and fertilisers. Not directly toxic, but phosphates are associated with the eutrophication of rivers and lakes.

_Attributes_
Description
	Phosphate Lr
	
Measurement Range
	0-4.0 mg/litre
	
Pack Size
	50

_Specification_
Measurement Range
	0-4.0 mg/l

[PRODUCT] Phosphate Lr Reagent Pack Sufficient for 250 Tests. (433-186/10)
Used extensively in food processing. Also present in many detergents and fertilisers. Not directly toxic, but phosphates are associated with the eutrophication of rivers and lakes.

_Attributes_
Description
	Phosphate Lr
	
Measurement Range
	0-4.0 mg/litre
	
Pack Size
	250

_Specification_
Measurement Range
	0-4.0 mg/l

[PRODUCT] Phosphate Reagent System 0-100Mg/Litre. Sufficient for 50 Tests. (433-188)
High levels of phosphates are used to treat water in industrial boilers so may be present in effluents.

_Attributes_
Description
	Phosphate
	
Measurement Range
	0-100 mg/litre
	
Pack Size
	50

_Specification_
Measurement Range
	0-100 mg/l

[PRODUCT] Phosphate Reagent Pack Sufficient for 250 Tests. (433-188/10)
High levels of phosphates are used to treat water in industrial boilers so may be present in effluents.

_Attributes_
Description
	Phosphate
	
Measurement Range
	0-100 mg/litre
	
Pack Size
	250

_Specification_
Measurement Range
	0-100 mg/l

[PRODUCT] Potassium Reagent System 0-12Mg/Litre. Sufficient for 50 Tests. (433-189)
An abundant natural element. High levels can be an indication of brackish waters.

_Attributes_
Description
	Potassium
	
Measurement Range
	0-12 mg/litre
	
Pack Size
	50

_Specification_
Measurement Range
	0-12 mg/l

[PRODUCT] Potassium Reagent Pack. Sufficient for 250 Tests. (433-189/10)
An abundant natural element. High levels can be an indication of brackish waters.

_Attributes_
Description
	Potassium
	
Measurement Range
	0-12 mg/litre
	
Pack Size
	250

_Specification_
Measurement Range
	0-12 mg/l

[PRODUCT] Silica Reagent System 0-4.0Mg/Litre As Si02. Sufficient for 50 Tests. (433-190)
Colloidal silica and soluble silicates are abundant in many natural waters. Causes scale problems in many industrial processes.

_Attributes_
Description
	Silica
	
Measurement Range
	0-4 mg/litre
	
Pack Size
	50

_Specification_
Measurement Range
	0-4.0 mg/l

[PRODUCT] Silica Reagent Pack Sufficient for 200 Tests. (433-190/10)
Colloidal silica and soluble silicates are abundant in many natural waters. Causes scale problems in many industrial processes.

_Attributes_
Description
	Silica
	
Measurement Range
	0-4 mg/litre
	
Pack Size
	200

_Specification_
Measurement Range
	0-4.0 mg/l

[PRODUCT] Sulphate Reagent System 0-200Mg/Litre. Sufficient for 50 Tests. (433-192)
Occurs naturally in water, but often introduced during water treatment. High levels can cause corrosion to metalwork by sulphate reducing bacteria. Damage to cement can also take place.

_Attributes_
Description
	Sulphate
	
Measurement Range
	0-200 mg/litre
	
Pack Size
	50

_Specification_
Measurement Range
	0-200 mg/l

[PRODUCT] Sulphate Reagent Pack Sufficient for 250 Tests. (433-192/10)
Occurs naturally in water, but often introduced during water treatment. High levels can cause corrosion to metalwork by sulphate reducing bacteria. Damage to cement can also take place.

_Attributes_
Description
	Sulphate
	
Measurement Range
	0-200 mg/litre
	
Pack Size
	250

_Specification_
Measurement Range
	0-200 mg/l

[PRODUCT] Sulphide Reagent System 0-0.5Mg/Litre. Sufficient for 50 Tests. (433-194)
Found in many natural waters, particularly hot springs. Present in many industrial effluents especially tanneries. Toxic to fish and aquatic organisms.

_Attributes_
Description
	Sulphide
	
Measurement Range
	0-0.5 mg/litre
	
Pack Size
	50

_Specification_
Measurement Range
	0-0.5 mg/l

[PRODUCT] Sulphide Reagent Pack Sufficient for 200 Tests. (433-194/10)
Found in many natural waters, particularly hot springs. Present in many industrial effluents especially tanneries. Toxic to fish and aquatic organisms.

_Attributes_
Description
	Sulphide
	
Measurement Range
	0-0.5 mg/litre
	
Pack Size
	200

_Specification_
Measurement Range
	0-0.5 mg/l

[PRODUCT] Sulphite Reagent System 0-500Mg/Litre. Sufficient for 50 Tests. (433-196)

_Attributes_
Description
	Sulphite
	
Measurement Range
	0-500 mg/litre
	
Pack Size
	50

_Specification_
Measurement Range

[PRODUCT] Sulphite Reagent Pack. Sufficient for 250 tests. (433-196/10)

_Attributes_
Description
	Sulphite
	
Measurement Range
	0-500 mg/litre
	
Pack Size
	250

_Specification_
Measurement Range

[PRODUCT] Zinc Reagent System 0-4.0Mg/Litre. Sufficient for 50 Tests. (433-198)
Used as a corrosion inhibitor in industrial cooling water so may be present in effluent dishcharges.

_Attributes_
Description
	Zinc
	
Measurement Range
	0-4.0 mg/litre
	
Pack Size
	50

_Specification_
Measurement Range
	0-4.0 mg/l

[GROUPED PRODUCT MATRIX]
Model No.
	Measurement Range
	Pack Size
	Desc
	N/A for this Product Group

[CATEGORY] Meteorology

[PRODUCT GROUP] Daily Raingauges

[PRODUCT] Copper Raingauge (502-010)
With 127 mm diameter rim with inner can and measuring cylinder calibrated in mm.

_Attributes_
Raingauge type
	Copper

[PRODUCT] Splayed-base daily raingauge (502-013)
British Meteorological Office MK 2 model, constructed from copper with splayed base to provide extra stability, and bevelled brass rim of 127 mm diameter. The inner copper can has a pouring lip and crass handle. Supplied with Meteorological Office pattern taper-base glass measure, graduated in mm.

_Further Information_
Dimensions 490 mm high x 216 mm base diameter.

_Attributes_
Raingauge type
	Splayed-base

[PRODUCT] De-Luxe Plastic Rain Gauge (460-010)
Made from strong UV stabilised plastic. The detachable internal collecting jar is calibrated in mm and inches of rain.

_Further Information_
Supplied with fixing bracket.

_Attributes_
Raingauge type
	Plastic

[PRODUCT] Electronic Rain Gauge. (504-012)
Consisting of collection unit, control box with 10 metres connecting cable, and 1.5 V battery.

_Further Information_
Collection unit dimensions: 100 x 50 x 113 mm.Display unit dimensions: 106 x 44 x 71 mmCollection unit dimensions: 100 x 50 x 113 mm.Display unit dimensions: 106 x 44 x 71 mmCollection unit dimensions: 100 x 50 x 113 mm.Display unit dimensions: 106 x 44 x 71 mmCollection unit dimensions: 100 x 50 x 113 mm.Display unit dimensions: 106 x 44 x 71 mmCollection unit dimensions: 100 x 50 x 113 mm.Display unit dimensions: 106 x 44 x 71 mmCollection unit dimensions: 100 x 50 x 113 mm.Display unit dimensions: 106 x 44 x 71 mmCollection unit dimensions: 100 x 50 x 113 mm.Display unit dimensions: 106 x 44 x 71 mmCollection unit dimensions: 100 x 50 x 113 mm.Display unit dimensions: 106 x 44 x 71 mmCollection unit dimensions: 100 x 50 x 113 mm.Display unit dimensions: 106 x 44 x 71 mmCollection unit dimensions: 100 x 50 x 113 mm.Display unit dimensions: 106 x 44 x 71 mmCollection unit dimensions: 100 x 50 x 113 mm.Display unit dimensions: 106 x 44 x 71 mm

_Attributes_
Raingauge type
	Electronic

[GROUPED PRODUCT MATRIX]
Model No.
	Type
	N/A for this Product Group

[PRODUCT GROUP] Wind measurement

[PRODUCT] Digital Vane Anemometer (503-060)
* Large Easy to read LCD display.* Fast, accurate readings.* Results in m/s, km/h, f/min or knots.This instrument is suitable for measuring wind speed or air flow for a variety of applications including crop spraying, ventilation surveys and crop storage checks. There is a choice of four metric and imperial measuring units together with a data hold facility.The specially designed sensor head features a low friction ball bearing design which allows free cane movement giving accurate results at both high and low velocities.

_Further Information_
Supplied complete with sensor head.

_Attributes_
Description
	Digital Vane Anemometer

[PRODUCT] Digital Hand Held Anemometer (460-050)
* Displays maximum gust.* 4 selectable measuring units.* Clear LCD display.The battery operated digital handheld anenometer is particularly suited to site investigations, environmental surveys and meteorological observations. It is lightweight, manufactured from non-corrosive materials and has replaceable cups. At least 2000 readings can be obtained from a single battery, and an error message is shown when the power is low. When the instruent is switched on the wind speed is averaged over a 15 to 18 second period after which the result is shown on the display.

_Further Information_
Complete with 2 support legs, storage bracket and spare cup.

_Attributes_
Description
	Digital Hand Held Anemometer

[PRODUCT] Anemometer Cups. Set of 3. (503-062/10)

_Attributes_
Description
	Anemometer Cups

_Related Products_
Main: Hand-Held Anemometer. (503-062)

[PRODUCT] Hand-Held Anemometer. (503-062)
A robust, easy to use instrument of durable plastic construction. Wind strength/speed is clearly and accurately displayed on 4 scales (m/s, km/h, knots and Beaufort). A secure fitting transparent cap protects the cups when not in use.

_Further Information_
Range 0 to 120 km/hr.

_Attributes_
Description
	Hand-Held Anemometer

_Related Products_
Accessory: Anemometer Cups. Set of 3. (503-062/10)

[PRODUCT] Digital Thermo-Anemometer 0-30 M/S 0-40 Deg C (503-068)
* Displays temperature or air flow.*Lightweight handheld instrument.* Wide range of applications.This battery powered instrument enables accurate readings of air temperature and wind velocity to be obtained. Air velocity is calculated by measuring the electrical energy required to maintain ta thermistor at a constant temperature.The circuitry is temperature compensated to give a rapid response over the range 0 to 30 m/s.The small probe size makes this instrument useful for micro-climate studies, measuring air circulation in crop canopies, greenhouse management and grain storage checks.

_Further Information_
Supplied complete with probe, extension rod and carrying case.

_Attributes_
Description
	Digital Thermo-Anemometer

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Temperature measurement

[PRODUCT] Wall Thermometer Dual Range. (504-011)
General purpose, economical unit. Dual range -30 to +45°C and -20 to +110°F.

_Attributes_
Description
	Wall Thermometer Dual Range

[PRODUCT] Maximum Thermometer -20 to +55 Deg. C Mercury Filled. (504-014)
Stem divided, mounted on a strong weather-resistant plastic scale with indelible figures; two drilling holes for fixing to a wall. Records maximum temperature since last reset. Usually mounted inside a meteorological screen at about 5° to the horizontal. Range -20 to +55°C, expected accuracy, +- 0.1°C; divided to 0.5°C.

_Further Information_
Dimensions 285 x 35 x 16 mm.

_Attributes_
Description
	Maximum Thermometer -20 to +55 Deg. C Mercury Filled

[PRODUCT] Minimum Thermometer -30 to +40 Deg. C Spirit Filled. (504-016)
Mounted on plastic scale to match maximum thermometer. Specification as maximum thermometer but recording minimum temperature since last reset, in the range of -30 to +40°C.

_Attributes_
Description
	Minimum Thermometer -30 to +40 Deg. C Spirit Filled

[PRODUCT] Electronic Inside/Outside Thermometer (504-019)
* Remote temperature probe.* Digital display.* Max/min memory.This electronic thermometer can be wall-mounted to display the ambient temperature. A plug in probe with 3 metres of cable can be used to obtain the temperature in another area or from outside. The instrument has a memory to recall the maximum and minimum inside and outside since the last reset.* Remote remperature probe.* Digital display.* Max/min memory.This electronic thermometer can be wall-mounted to display the ambient temperature. A plug in probe with 3 metres of cable can be used to obtain the temperature in another area or from outside. The instrument has a memory to recall the maximum and minimum inside and outside since the last reset.

_Further Information_
Supplied complete with display unit, remote temperature probe and 3 metres of cable.

_Attributes_
Description
	Electronic Inside/Outside Thermometer

[PRODUCT] De-Luxe Inside/Outside Thermometer (504-020)
* Twin digital displays.* Independent inside/outside memory.* Remote probe.The deluxe inside/outside thermometer has a separate digital display for each temperature. There is a separate maximum and minimum memory for the inside and outside temperatures. The remote outside probe is supplied with 3 metres of cable.

_Further Information_
With twin digital displays, supplied with 3 metres of cable.

_Attributes_
Description
	De-Luxe Inside/Outside Thermometer

[PRODUCT] Day and Night Thermometer -36 to 50 Deg C (504-021)
Housed ina fully enclosed plastic case. The twin scales record the maximum and minimum temperatures since the last reset. Normally used to check variations in day and night-time temperatures. Weather resistant and suitable for both inside and out. Reset by turning a knob, no magnet required.

_Further Information_
Range -36 to +50°C x 1°C.Range -36 to +50°C x 1°C.Range -36 to +50°C x 1°C.Range -36 to +50°C x 1°C.Range -36 to +50°C x 1°C.Range -36 to +50°C x 1°C.Range -36 to +50°C x 1°C.Range -36 to +50°C x 1°C.Range -36 to +50°C x 1°C.Range -36 to +50°C x 1°C.

_Attributes_
Description
	Day and Night Thermometer -36 to 50 Deg C

[PRODUCT] Laboratory Thermometer with Low Toxicity Filling (504-023)
General purpose insertion type thermometer containing no toxic filling. This thermometer features a reinforced stirring tip and an integral bulb. Ideal for propagators, greenhouse and laboratories.

_Further Information_
Length 305 mm. Range -10 to 110°C. Supplied in plastic tube.Length 305 mm. Range -10 to 110°C. Supplied in plastic tube.Length 305 mm. Range -10 to 110°C. Supplied in plastic tube.Length 305 mm. Range -10 to 110°C. Supplied in plastic tube.Length 305 mm. Range -10 to 110°C. Supplied in plastic tube.Length 305 mm. Range -10 to 110°C. Supplied in plastic tube.Length 305 mm. Range -10 to 110°C. Supplied in plastic tube.Length 305 mm. Range -10 to 110°C. Supplied in plastic tube.Length 305 mm. Range -10 to 110°C. Supplied in plastic tube.Length 305 mm. Range -10 to 110°C. Supplied in plastic tube.

_Attributes_
Description
	Laboratory Thermometer with Low Toxicity Filling

[PRODUCT] Portable Soil Thermometer -10C to +50C. (504-024)
Range -10 to +50°C, in a rugged brass case with stem graduated at 5, 10, 15, 20, 30 cm, to enable measurement at various depths. Ideal for use in education.

_Attributes_
Description
	Portable Soil Thermometer -10C to +50C.

[PRODUCT] Sheathed Earth Thermometer 300mm (504-032)
Manufactured to British Meteorological specifications, these thermometers are lowered to a selected depth in the soil via a pointed steel tube. They are solid stem mercury-in-glass type, and are fitted into a transparent sheath made of stout glass tubing. The bottom 40 mm of the sheath is filled with paraffin wax in which the bulb is embedded. The thermometer therefore responds quite slowly to temperature changes and can be raised to the surface for reading.A flange controls the exact depth of sinking and ensures sufficient projection above ground to keep out standing water, and the tube is sealed with a copper cap.

_Further Information_
300 mm length tube. Graduated -5 to +40°C x 0.5°C. Accuracy +-0.1°C.300 mm length tube. Graduated -5 to +40°C x 0.5°C. Accuracy +-0.1°C.300 mm length tube. Graduated -5 to +40°C x 0.5°C. Accuracy +-0.1°C.300 mm length tube. Graduated -5 to +40°C x 0.5°C. Accuracy +-0.1°C.300 mm length tube. Graduated -5 to +40°C x 0.5°C. Accuracy +-0.1°C.300 mm length tube. Graduated -5 to +40°C x 0.5°C. Accuracy +-0.1°C.300 mm length tube. Graduated -5 to +40°C x 0.5°C. Accuracy +-0.1°C.300 mm length tube. Graduated -5 to +40°C x 0.5°C. Accuracy +-0.1°C.300 mm length tube. Graduated -5 to +40°C x 0.5°C. Accuracy +-0.1°C.300 mm length tube. Graduated -5 to +40°C x 0.5°C. Accuracy +-0.1°C.

_Attributes_
Description
	Sheathed Earth Thermometer 300mm

[PRODUCT] Insulated Earth Thermometer 50mm (504-038)
The insulated pattern themometer is left in the soil, with the added advantage that readings can be taken in-situ without disturbing the instrument. The lower portion is placed vertically in the earth with the bulb at the required depth, and the insulated thermometer stem and opal scale are supported on a black-enamelled mild steel angle bracket. The range is -10 to +55°C divided into 2.0°C intervals.

_Further Information_
For use up to 50 mm depth.

_Attributes_
Description
	Insulated Earth Thermometer 50mm

[PRODUCT] Insulated Earth Thermometer 100mm (504-040)
The insulated pattern themometer is left in the soil, with the added advantage that readings can be taken in-situ without disturbing the instrument. The lower portion is placed vertically in the earth with the bulb at the required depth, and the insulated thermometer stem and opal scale are supported on a black-enamelled mild steel angle bracket. The range is -10 to +55°C divided into 2.0°C intervals.

_Further Information_
For use up to 100 mm depth.

_Attributes_
Description
	Insulated Earth Thermometer 100mm

[PRODUCT] Insulated Earth Thermometer 200mm (504-042)
The insulated pattern themometer is left in the soil, with the added advantage that readings can be taken in-situ without disturbing the instrument. The lower portion is placed vertically in the earth with the bulb at the required depth, and the insulated thermometer stem and opal scale are supported on a black-enamelled mild steel angle bracket. The range is -10 to +55°C divided into 2.0°C intervals.

_Further Information_
For use up to 200 mm depth.

_Attributes_
Description
	Insulated Earth Thermometer 200mm

[PRODUCT] Insulated Earth Thermometer 300mm (504-044)
The insulated pattern themometer is left in the soil, with the added advantage that readings can be taken in-situ without disturbing the instrument. The lower portion is placed vertically in the earth with the bulb at the required depth, and the insulated thermometer stem and opal scale are supported on a black-enamelled mild steel angle bracket. The range is -10 to +55°C divided into 2.0°C intervals.

_Further Information_
For use up to 300 mm depth.

_Attributes_
Description
	Insulated Earth Thermometer 300mm

[PRODUCT] Support Bracket for Earth Thermometers. (504-046)

_Attributes_
Description
	Support Bracket for Earth Thermometers

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Light measurement

[PRODUCT] Campbell Stokes Sunshine Recorder for latitudes 0-45 N or S. Includes 1 year supply of charts. (505-062)
* Records duration of sunshine.* Accurate measurements.* Simple to use.This instrument is used to record the duration of sunshine each day. The sun's rays are focused by a precision glass sphere onto a curved card. The intense heat burns a trace on the card. As the sun moves across the sky, so does the position of the spot across the card. If the sun is obscured by cloud then no trace is made. At the end of the day, the length, less gaps, is proportional to the duration of sunshine.

_Further Information_
For latitudes 0° to 40° North or South. Complete with one year's supply of cards.For latitudes 0° to 40° North or South. Complete with one year's supply of cards.For latitudes 0° to 40° North or South. Complete with one year's supply of cards.For latitudes 0° to 40° North or South. Complete with one year's supply of cards.For latitudes 0° to 40° North or South. Complete with one year's supply of cards.For latitudes 0° to 40° North or South. Complete with one year's supply of cards.For latitudes 0° to 40° North or South. Complete with one year's supply of cards.For latitudes 0° to 40° North or South. Complete with one year's supply of cards.For latitudes 0° to 40° North or South. Complete with one year's supply of cards.

_Attributes_
Description
	Campbell Stokes Sunshine Recorder

_Related Products_
Accessory: Charts 1 Year Supply for 505-062 (505-062/10)

[PRODUCT] Accupar Ceptometer with 800mm Probe Datalogger and Rs232 Interface. Battery Powered. (505-067)

_Attributes_
Description
	Accupar Ceptometer with 800mm Probe Datalogger

[PRODUCT] Large Tube Solarimeter Plain 5M. (505-070)

_Attributes_
Description
	Large Tube Solarimeter

[PRODUCT] Solar Radiation Display and Integrator. for Use with Solar Sensors. (505-086)

_Attributes_
Description
	Solar Radiation Display and Integrator

[PRODUCT] Digital Lux Meter (505-092)
* High accuracy and wide range.* Remote sensor head.* Ideal for field work.This portable lightmeter is for monitoring illuminance and gives a digital display in Lux. This simple to use instruments has only two controls; a power button and a range switch. It is ideal for field survey work and initial investigations.

_Further Information_
Supplied complete with sensor head.

_Attributes_
Description
	Digital Lux Meter

[PRODUCT] Light Measuring Unit (Luxmeter) with Sensor. (505-106)
* Direct readout in energy units of visible light.* Range 0 - 200 K Lux in 3 ranges of sensitivity.*Use for siting of buildings, measuring light variations.General measurement for human activities.The visible light is that part of the wavelength spectrum received by the human eye. The peak sensitivity is 555 nm for the adapted eye but with "dark adaption" a peak response is 507 nm. The ranges allow for readings between 0 - 200 K Lux.The sensor has a cosine-corrected head, and the FET input circuitry of the cc measuring and display unit, preserves lineariry. The unit also incorporates dual slope integration with "auto zero" for A/D conversion.

_Further Information_
With sensor and 1.2 m cable. Supplied in carrying case with battery.

_Attributes_
Description
	Light Measuring Unit (Luxmeter)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Humidity measurement

[PRODUCT] Hygrometer / Thermometer 100mm Diameter Dial 10-100% Rh -25 to +45 Deg C. (506-122)
A precision instrument using specially treated strands of human hair to measure relative humidity. The 100 mm diameter gauge covers the range 10 to 100% RH. A separate set hand with a centre button is fitted to the case to enable the user to monitor changes. Can be wall-mounted or fitted inside a Stevenson screen.

_Attributes_
Description
	Hygrometer / Thermometer 100mm

[PRODUCT] Digital Electronic Temperature/Humidity Meter (506-124)
* Designed for wall-mounting.* Shows temperature and humidity.* Max/min internal memory.This simple to use instrument shows both temperature and relative humidity on a clear LCD display. The internal memory stores the maximum and minimum temperature since the last reset. Ideal for installing in a green house, propagator or vegetable store.

_Attributes_
Description
	Digital Electronic Temperature/Humidity Meter

[PRODUCT] Kew Pattern Masons Hygrometer Supplied with Conversion Chart. (506-104)
A high quality hygrometer with accurate, stem-divided, mercury-filled thermometers made to British Meteorological Office design. The thermometers are fitted to laminated plastic mounts with indelible dividing and figuring. The mounts themselves are fitted to a laminated plastic back-plate which will not warp and is very strong. The water reservoir is supported by a metal strip attached to the back plate, and the bulb of one thermometer is kept constantly wet by capillary action. A cotton wick runs up from the reservoir and is threaded round a circle of muslin covering the bulb.

_Further Information_
With temperature ranges -20 to +55°C, complete with simple slide rule. Dimensions 380 x 140 x 50 mm.With temperature ranges -20 to +55°C, complete with simple slide rule. Dimensions 380 x 140 x 50 mm.With temperature ranges -20 to +55°C, complete with simple slide rule. Dimensions 380 x 140 x 50 mm.With temperature ranges -20 to +55°C, complete with simple slide rule. Dimensions 380 x 140 x 50 mm.With temperature ranges -20 to +55°C, complete with simple slide rule. Dimensions 380 x 140 x 50 mm.With temperature ranges -20 to +55°C, complete with simple slide rule. Dimensions 380 x 140 x 50 mm.With temperature ranges -20 to +55°C, complete with simple slide rule. Dimensions 380 x 140 x 50 mm.With temperature ranges -20 to +55°C, complete with simple slide rule. Dimensions 380 x 140 x 50 mm.With temperature ranges -20 to +55°C, complete with simple slide rule. Dimensions 380 x 140 x 50 mm.

_Attributes_
Description
	Kew Pattern Masons Hygrometer

_Related Products_
Accessory: Threaded Muslins & Wicks. (506-104/12)

[PRODUCT] Threaded Muslins & Wicks. (506-104/12)
Pack of 50.

_Attributes_
Description
	Threaded Muslins & Wicks

_Related Products_
Main: Kew Pattern Masons Hygrometer Supplied with Conversion Chart. (506-104)

[PRODUCT] Wet & Dry Bulb Hygrometer (506-106)
* Easy to read.* Use outdoors in a screen.The wet and dry bulb hygrometer is designed for general use and consists of two undivided thermometers mounted on a printed plastic scale. Between the thermometers is a unique slide pointer which allows relative humidity to be easily read. The scale is housed in a plastic case which also holds a reservoir with anti-frost device

_Further Information_
Easy to read pattern, range -10 to +50°C Easy to read pattern, range -10 to +50°C Easy to read pattern, range -10 to +50°C Easy to read pattern, range -10 to +50°C Easy to read pattern, range -10 to +50°C Easy to read pattern, range -10 to +50°C Easy to read pattern, range -10 to +50°C Easy to read pattern, range -10 to +50°C Easy to read pattern, range -10 to +50°C

_Attributes_
Description
	Wet & Dry Bulb Hygrometer

[PRODUCT] Portable Temperature and Humidity Meter with Detachable Probe. Supplied in plastic box. (506-150)
This hand-held battery operated instrument is operated by a single keypad button. It is suitable for a wide variety of applications where fast and accurate measurements of relative humidity and temperature are required. The probe is connected to the display unit via a one metre flexi-cable which enables its measurements to be taken in areas where access is limted.

_Attributes_
Description
	Portable Temperature and Humidity Meter

[PRODUCT] Portable Humidity & Temperature Meter with Dewpoint & Wet Bulb Temp Measurement. (506-160)

_Attributes_
Description
	Portable Humidity & Temperature Meter with Dewpoint & Wet Bulb

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Evaporation measurement

[PRODUCT] Hook Gauge Evaporimeter. with Aluminium Pan. (506-250)
* Measures evaporation rate from a free water surface.* Used by meteorologists and water engineers throughout the world.* Manufactured to the American Weather Bureau pattern.Because of the recognition of the accuracy of this instrument, reliable equations have been devised, by which the readings obtained may be converted into useful figures for evaporation from lakes and reservoirs.The water level in a standard cylindrical tank (1220 mm diameter) is measured, usually every 24 hours, by adjusting the height of a hook until its point just breaks the surface.The measurement is taken inside a still-well which provides a small area of warer surface free from ripples. The still0well, made of brass, stands on three levelling screws and has an opening in the base to equalise the water levels inside and out. The hook gauge, also brass, rests on top of the well supported by three horizontal arms, and has a micrometer head to provide very fine adjustment.A useful accessory is a maximum/minimum thermometer which floats just under the water surface in the main tank. A magnet is supplied for resetting the indices

_Further Information_
Consisting of hook gauge, still-well and galvanised iron tank as specified. Supplied without floating thermometer.

_Attributes_
Description
	Hook Gauge Evaporimeter

_Related Products_
Spare/Consumable: Class A Evaporation Tank. (506-250/10)
Spare/Consumable: Hook Gauge (506-250/14)
Spare/Consumable: Still-Well (506-250/12)

[PRODUCT] Class A Evaporation Tank. (506-250/10)
1220 mm diameter x 254 mm high.

_Attributes_
Description
	Class A Evaporation Tank

_Related Products_
Main: Hook Gauge Evaporimeter. with Aluminium Pan. (506-250)

[PRODUCT] Still-Well (506-250/12)
215 x 254 x 254 mm

_Attributes_
Description
	Still-Well

_Related Products_
Main: Hook Gauge Evaporimeter. with Aluminium Pan. (506-250)

[PRODUCT] Hook Gauge (506-250/14)
165 x 115 x 115 mm

_Attributes_
Description
	Hook Gauge

_Related Products_
Main: Hook Gauge Evaporimeter. with Aluminium Pan. (506-250)

[PRODUCT] Floating Maximum/Minimum Thermometer. Hazardous. (506-252)

_Attributes_
Description
	Floating Maximum/Minimum Thermometer

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Atmospheric pressure measurement

[PRODUCT] Precision Aneroid Barometer 890 -1050 Mbar. (506-042)
* Accuracy of +- 1 millibar.* Chrome case.* Compensated movement.* Dual range, millibars or mm of mercury.This precision barometer is intended for professional use. It features a massive 60 mm diameter aneroid movement which has been calibrated +-1 millibar over the whole range. Ideal for mounting inside a Stevenson screen, or hanging in the office.

_Further Information_
930 to 1080 mb range.

_Attributes_
Description
	Precision Aneroid Barometer

[PRODUCT] Brass Clip. (506-260/11)
For attaching filter-paper discs.

_Attributes_
Description
	Brass Clip

_Related Products_
Main: Piche Evaporimeter (506-260)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Chart recording instruments

[PRODUCT] Thermo-Hygrograph -15 to +65 Deg C 0-100% Rh. with 1 Year Supply of Charts and 2 Spare Pens. (506-206)
This combination instrument records both temperature and relative humidity on the same chart.

_Further Information_
Mechanical movement, supplied with 52 weekly charts and a bottle of ink.

_Attributes_
Description
	Thermo-Hygrograph -15 to +65 Deg C 0-100% Rh

_Related Products_
Spare/Consumable: Weekly Chart for Thermo- Hygrograph -15 to +65 C. 0-100% Rh. Pack of 52. (506-206/12)

[PRODUCT] Weekly Chart for Thermo- Hygrograph -15 to +65 C. 0-100% Rh. Pack of 52. (506-206/12)
Chart for Thermo-Hygrograph 506-206.

_Attributes_
Description
	Weekly Chart for Thermo- Hygrograph -15 to +65 C. 0-100% Rh

_Related Products_
Main: Thermo-Hygrograph -15 to +65 Deg C 0-100% Rh. with 1 Year Supply of Charts and 2 Spare Pens. (506-206)

[PRODUCT] Hygrograph 0-100% RH with 1 year supply of charts and spare pen. (506-203)
The hygrograph uses hair to detect changes in humidity. The expansion or contraction of the hair is transferred into a vertical movement which is recorded on the revolving drum.

_Further Information_
Mechanical movement, supplied with 52 weekly charts and a bottle of ink.

_Attributes_
Description
	Hygrograph 0-100% RH

[PRODUCT] Barograph, 955-1055 mb with 1 year supply of charts and spare pen. (506-204)
The barograph uses a vacuum capsule to detect changes in atmospheric pressure. The expansion or contraction of the capsule is transferred into a vertical movement which is recorded on the revolving drum.

_Further Information_
Mechanical movement, supplied with 52 weekly charts and a bottle of ink.

_Attributes_
Description
	Barograph, 955-1055 mb

_Related Products_
Spare/Consumable: Weekly Chart for Barograph 955 to 1055 Mb Pack of 52. (506-204/12)

[PRODUCT] Weekly Chart for Barograph 955 to 1055 Mb Pack of 52. (506-204/12)
Chart for Barograph 506-204

_Attributes_
Description
	Weekly Chart for Barograph 955 to 1055 Mb

_Related Products_
Main: Barograph, 955-1055 mb with 1 year supply of charts and spare pen. (506-204)

[PRODUCT] Thermograph -15To+65 Degc with 1 Year Supply of Charts and Spare Pen. (506-201)
The thermograph uses a bi-metallic element to detect changes in temperature. The expansion or contraction of the element is transferred into a vertical movement which is recorded on the revolving drum.

_Further Information_
Mechanical movement, supplied with 52 weekly charts and a bottle of ink.

_Attributes_
Description
	Thermograph -15To+65 Degc

_Related Products_
Spare/Consumable: Weekly Chart for Thermo- Graph. -15 to +65 Deg. C. Pack of 52. (506-201/12)

[PRODUCT] Weekly Chart for Thermo- Graph. -15 to +65 Deg. C. Pack of 52. (506-201/12)
Charts for Thermograph 506-201.

_Attributes_
Description
	Weekly Chart for Thermo- Graph. -15 to +65 Deg. C

_Related Products_
Main: Thermograph -15To+65 Degc with 1 Year Supply of Charts and Spare Pen. (506-201)

[PRODUCT] Black Fibre Tip Pen for Chart Recording Instruments. (506-212)
Refillable.

_Attributes_
Description
	Black Fibre Tip Pen for Chart Recording Instruments

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Manual weather stations

[PRODUCT] Stevenson Screen Interior Dimensions 435 X 250 X 445mm (504-120)
The Stevenson screen is designed to hold maximum and minimum thermometers, and a wet-and-dry bulb hygrometer. It is available either in the finished form, ready for use, or more cheaply as a make-it-yourself kit. Both are suitable for use in all climates.The screen is made from top quality seasoned wood, with double-louvred sides, a double layer roof, and a floor of overlapping boards separated vertically by an airspace. The front panel is hinged at the bottom to form a door, and is retained in the horizontal position by two chains; it may be padlocked shut.

_Further Information_
Supplied without instruments or stand, painted white to reflect radiation. 540 x 580 x 480 mm.

_Attributes_
Description
	Stevenson Screen Interior

_Related Products_
Accessory: Iron Stand for stevenson screen (504-120) (504-124)

[PRODUCT] Iron Stand for stevenson screen (504-120) (504-124)
Ensures the instruments are positioned at the correct height.

_Further Information_
1280 mm high.

_Attributes_
Description
	Iron Stand for stevenson screen

_Related Products_
Main: Stevenson Screen Interior Dimensions 435 X 250 X 445mm (504-120)

[PRODUCT] Budget Weather Station Inc Max/Min Thermometer Wet/Dry Bulb Hygrometer Rain Gauge Soil Thermometer (461-050)
This package of equipment provides low cost but accurate instruments to enable daily weather readings to be taken. Instruments include a maximum and minimum thermometer, soil thermometer, wet and dry bulb thermometer and Rain-o-matic electronic raingauge.A simple DIY screen is provided to house the thermometers.

_Attributes_
Description
	Budget Weather Station

[PRODUCT] Standard Weather Station with Max/Min Thermometers Kew Pattern Hygrometer Sheathed Earth Therm. (461-052)
A complete manual weather station to enable accurate daily weather readings to be obtained. Instruments include maximum thermometer, minimum thermometer, Kew pattern masons hygrometer, a sheathed earth thermometer, a copper raingauge and a handheld anemometer. A DIY Stevenson screen is provided to house the thermometers.

_Attributes_
Description
	Standard Weather Station

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[CATEGORY] Weather and monitoring stations

[PRODUCT GROUP] Environmental weather station
The Environmental Monitoring Station (EMS) provides an automatic method of recording a wide range of meteorological and environmental data. It overcomes the problem of manual recording methods and replaces them with a simple to use data logging system which can be left unattended in remote areas and harsh environments. The data can be collected at convenient intervals using a portable computer. The software enables graphs, reports and tables of results to be produced with just a few keystrokes. The modular construction enables a system to be built to your exact requirements.

[PRODUCT] Cumulus System. (508-100)

_Attributes_
Description
	Cumulus System - without solar panel

_Related Products_
Accessory: Cumulus Tool Kit. (508-186)

[PRODUCT] Cumulus System. (508-102)

_Attributes_
Description
	Cumulus System - with solar panel

_Related Products_
Accessory: Cumulus Tool Kit. (508-186)

[PRODUCT] Cumulus Tool Kit. (508-186)

_Attributes_
Description
	Cumulus Tool Kit

_Related Products_
Main: Cumulus System. (508-102)
Main: Cumulus System. (508-100)

[PRODUCT] Combined Communication and Power Supply Cable. 10m Long. for Cumulus Aws (506-192)

_Attributes_
Description
	Combined Communication and Power Supply Cable

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[CATEGORY] Crop Science

[PRODUCT GROUP] Microbiology

[PRODUCT] Hand Lens. (535-208)
With 15 mm diameter achromatc lens mounted in metal case.

_Further Information_
Magnification x10.

_Attributes_
Description
	Hand Lens

[PRODUCT] Colony Counter 220-240V 50Hz 1Ph. (535-210/01)
* Uniform glare-free illumination.* Angled front for operator comfort.* Counter triggered by depressing petri dish.* Digital display of results.* Built in magnifier.The petri dish is placed on the viewing and every time a colony is pressed a count is registered and accompanied by an audible tone. Both the amount of pressure needed to register a count and the volume of the tone are adjustable. The built-in adjustable magnifier enables samples to be examined more easily. For use with up to 10 cm glass or plastic petri dishes.* Uniform glare-free illumination.* Angled front for operator comfort.* Counter triggered by depressing petri dish.* Digital display of results.* Built in magnifier.The petri dish is placed on the viewing and every time a colony is pressed a count is registered and accompanied by an audible tone. Both the amount of pressure needed to register a count and the volume of the tone are adjustable. The built-in adjustable magnifier enables samples to be examined more easily. For use with up to 10 cm glass or plastic petri dishes.

_Further Information_
For 220-240 V, 50 Hz, 1 ph.

_Attributes_
Description
	Colony Counter 220-240V 50Hz 1Ph

[PRODUCT] Single Tullgren Funnel 220-240V 50Hz 1Ph. (535-245/01)
* Wet or dry extraction of soil organisms.* Precision aluminium funnel construction.* Stoppered collection vessel prevents loss of creatures.This apparatus is used for both dry and wet exraction of soil organisms. A soil or leaf litter sample is placed in the removable upper part of the funnel. Heat and light from the lamp creates a temperature gradient of approximately 14°C in the soil sample. This stimulates the downward movement of soil arthropods, and similar organisms, through the gauze to a receiver attached to the base of the funnel. The position of the lamp is adjustable to enable the temperature of the soil to be raised gradually thus preventing the slower moving species from becoming trapped in hard dry cakes of soil.For wet extraction, the funnel is filled with water and the gauze is placed in postition. Nematodes and other swimming forms collect in the base of the funnel and can be drawn off at intervals (this method is suitable for collecting potato eel worm). This method can be used either with or without the use of the lamp.

_Further Information_
Complete with funnel, wire gauze, soil retaining cylinder, length of rubber tube, lamphouse with lampholder, retort stand and instructions.

_Attributes_
Description
	Single Tullgren Funnel 220-240V 50Hz 1Ph.

[PRODUCT] Spore Sampler c/w sampler, wind vane, rain shield, drum, cutting block, 1kg Gelvatol, Tape, scalpel (535-260/01)
* Continuous sampling for up to 7 days.* Built-in vacuum pump.* 7 jewel clockwork recording drum.The spore sampler uses a pump to draw air through an orifice. Fungal spores and pollen are impacted onto a strip of adhesive coated plastic strip fitted to the clockwork driven drum. The sampling head can revolve and a large fin is fitted so that air is always drawn from upwind.* Continuous sampling for up to 7 days.* Built-in vacuum pump.* 7 jewel clockwork recording drum.The spore sampler uses a pump to draw air through an orifice. Fungal spores and pollen are impacted onto a strip of adhesive coated plastic strip fitted to the clockwork driven drum. The sampling head can revolve and a large fin is fitted so that air is always drawn from upwind.

_Further Information_
220-240 V, 50 Hz, 1 ph

_Attributes_
Description
	Spore Sampler

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Plant physiology

[PRODUCT] Portable Leaf Area Meter (470-010/01)
* Enables non-destructive measurements.* Lightweight and fully portable.* No calibration required.* 32 K internal memory.* Rechargeable battery.The portable leaf area matter enables samples to be measured without detaching them from the plant. The unit is operated using only two buttons to select options from the display. Individual readings can be stored, or areas can be accumulated as a running total.The unit is supplied with an RS232 cable and IBM compatible software. This enables data to be transferred to a computer for further analysis if required.A ful lrange of parameters can be measured including leaf area, width, perimeter length, shape factor and ratio. The sensitivity of the scanner can be adjusted so that healthy or diseased parts of the leaf can be recorded. This flexibility makes the instrument ideal for the field scientist investigating the effects of pollution on plants. The leaves do not have to be removed for measurement so the same plant can be monitored over a period of time in detailed experiments.

_Further Information_
for 220-240 V, 50 Hz, 1 ph.

_Attributes_
Description
	Portable Leaf Area Meter

[PRODUCT] Digital Plant Water Potential Apparatus with Carbon Dioxide Pressure Source. (540-301)
* Battery powered.* Large digital display.* Flow regulator.The ELE digital water plant potential apparatus is lightweight and portable making it suitable for both field or laboratory use. The large digital display can be frozen to provide precise readings. The standard gaskets will fit all plants with a leaf petiole of up to 6 mm. Pressures of up to 30 atmospheres can be achieved in the chamber. A safety valve is fitted to prevent pressures rising above this level.

_Attributes_
Description
	Digital Plant Water Potential Apparatus

[PRODUCT] Plant Photosynthesis Analyser with Battery 120/240V 50/60Hz (470-020/09)
* Fully portable.* Built-in self checking system.* Data storage.* Automatic atmospheric pressure compensation.The plant photosynthesis analyser enables the scientist to investigate growing plants either in the field or laboratory. Since the plant is not damaged by the analysis it can be repeatedly tested under different conditions to observe the results.The leaf chamber is placed over the selected sample and a measured flow of air is pumped over the leaf surface. Sample data is typed into the keypad when requested. This includes leaf area details which can be estimated or measured using the Portable Leaf Area Meter. The concentrations of the carbon dioxide and water vapour in the incoming air are measured. By comparing these with the outgoing concentrations, the gas exchange rate and photosynthetic rate are calculated and shown on the display. Data is stored on removable cards and can be transferred to a computer via the built-in RS232 port.

_Further Information_
Complete with battery, charger, carrying bag, harness, air probe and spare parts. Requires a leaf chamber for use.

_Attributes_
Description
	Plant Photosynthesis Analyser

[PRODUCT] Chlorophyll Content Meter for Plants and Crops. Suppllied with Battery Rs232 Cable and Software. (470-045)

_Attributes_
Description
	Chlorophyll Content Meter

[PRODUCT] Plant Efficiency analyser with control unit & sensor, field neck support & strap, charger, (470-040)
* Lightweight, compact, portable field instrument.* No moving parts for reliable operation.* State-of-the-art microprocessor and logic control.*Fast accurate measurement and calculations.* PC link and analysis software included.When lights shines on a plant it is absorbed by the chlorophyll molecules in the leaf. The absorbed energy is then utilised in a variety of ways including photosynthesis, the process by which carbon dioxide in the atmosphere is converted by the plant to organic compounds. A proportion of the absorbed energy is re-emitted as chlorophyll fluorescence.The Plant Efficiency Analyser measures this fluorescence and calculates key parameters to provide a direct measurement of photochemical efficiency and thus indicate stress conditions at an early stage.Many factors may influence the wellbeing of plants including the temperature and light conditions, shortage of water or nutrients, contaminated soil, air pollution and acid rain. All of these have an effect on chlorophyll fluorescence making this an ideal instrument for the serious study of plant health, crop selection or plant breeding.

_Further Information_
Includes carrying bag, sensor unit, battery charger unit, serial cable, analogue lead, instruction manuals, 20 leaf clips, and data analysis software for IBM PC compatible computers supplied on 5.25" and 3.5" discs.

_Attributes_
Description
	Plant Efficiency analyser

_Related Products_
Spare/Consumable: Leaf Clips 4mm Pack of 10. (Spare for 470-040). (470-040/10)

[PRODUCT] Leaf Clips 4mm Pack of 10. (Spare for 470-040). (470-040/10)
Pack of 10.

_Attributes_
Description
	Leaf Clips 4mm Pack of 10

_Related Products_
Main: Plant Efficiency analyser with control unit & sensor, field neck support & strap, charger, (470-040)

[PRODUCT] Porometer Complete with Sensor Head Etc 220-240V 50/60Hz 1Ph Battery Charger. (540-026/01)
* Direct readout of conductance or resistance.* Simple field calibration.* Stores up to 1500 readings.* Leaf stress minimised during measurements.When the sensor head is clipped onto a leaf, a small cup is gently pressed onto the leaf surface. Water vapour diffuses out of the leaf via the stomata and this raises the humidity in the cup. The instrument times the raise in humidity between two electronically preset levels. This RH transit time is a measure of water vapour loss and is automatically converted into diffusion resistance or conductivity. Calibration should be carried out at the start of each session and when environmental conditions change significantly. A polypropylene plate with 6 groups of precisely moulded holes is used to simulate a leaf. The diffusion resistance of each group is known from the physical dimensions of the holes. The instrument is calibrated using these values, and will also give a warning if changing conditions require recalibration.

_Further Information_
Includes calibration plate, rechargeable battery, carrying case, RS232 cable, adapter, data collection software, consumables and battery charger.

_Attributes_
Description
	Porometer Complete

_Related Products_
Spare/Consumable: Porometer Spares Kit Including Electronic Components Pump Cables and Fuses (540-026/10)

[PRODUCT] Porometer Spares Kit Including Electronic Components Pump Cables and Fuses (540-026/10)
Includes electronic components, pump, cables and fuses.

_Attributes_
Description
	Porometer Spares Kit

_Related Products_
Main: Porometer Complete with Sensor Head Etc 220-240V 50/60Hz 1Ph Battery Charger. (540-026/01)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Seed technology

[PRODUCT] Laboratory seed blower 220-240V 50Hz 1ph (542-044/01)
The laboratory seed blower consists of a fan, a pressure chamber and a vertical separation pipe. It is used to classify particles according to their aerodynamic behaviour in an air stream. The seed sample is placed on a perforated metal screen. Air is then blown through the sample and up into a vertical transparent pipe. By adjusting the air velocity the sample can be divided into two fractions. This process is further aided by the two baffles positioned near the top of the tube. A timer enables the blowing period to be adjusted between 0 and 15 minutes.

_Further Information_
Includes timer, separation pipe and fan with regulator.

_Attributes_
Description
	Laboratory seed blower

[PRODUCT] ELE Jacobsen Seed Testing Bath. (542-100/01)

_Attributes_
Description
	ELE Jacobsen Seed Testing Bath

_Related Products_
Accessory: Glass Plate for Jacobsen Seed Testing Bath. (13 Plates Required for Each Bath). (542-104)
Accessory: Plastic Covers Pack of 10 for Seed Testing Bath (7 Packs Required for Each Bath). (542-106)
Accessory: Stand for Jacobsen Seed Testing Bath. (542-102)

[PRODUCT] Stand for Jacobsen Seed Testing Bath. (542-102)

_Attributes_
Description
	Stand for Jacobsen Seed Testing Bath

_Related Products_
Main: ELE Jacobsen Seed Testing Bath. (542-100/01)

[PRODUCT] Glass Plate for Jacobsen Seed Testing Bath. (13 Plates Required for Each Bath). (542-104)

_Attributes_
Description
	Glass Plate for Jacobsen Seed Testing Bath

_Related Products_
Main: ELE Jacobsen Seed Testing Bath. (542-100/01)

[PRODUCT] Plastic Covers Pack of 10 for Seed Testing Bath (7 Packs Required for Each Bath). (542-106)

_Attributes_
Description
	Plastic Covers Pack of 10 for Seed Testing Bath

_Related Products_
Main: ELE Jacobsen Seed Testing Bath. (542-100/01)

[PRODUCT] Germination Cabinet with sealed stainless steel chamber 220-240v 50hz 1ph (542-124/01)
* Electronic sensing of temperature with digital indication.* Cooling provided by a built-in refrigeration unit.* 24 hour timer on temperature and fluorescent lighting.This robust germination unit is constructed in rust resistant electrozinc-plated mild steel and finished in white stove enamel paint for a smooth, tough, easy-to-clean finish.The plastic coated wire mesh shelves are fully adjustable with 32 shelf positions at 29 mm centres.The dual temperature controller and thermistor system enable two temperatures to be set to correspond with "day" and "night" environments.An adjustable over-temperature safety cut-out protects the contents from accidental overheating.

_Further Information_
With sealed stainless steel chamber. 220-240 V, 50 Hz, 1 ph.

_Attributes_
Description
	Germination Cabinet

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Crop processing

[PRODUCT] Laboratory Winnower. 220-240V 50Hz 1Ph. (543-820/01)
This machine is suitable for pre-cleaning a large number of agricultural products including hulled rice and coffee, wheat, barley and vegetable seeds, by removing light extraneous material such as such as shrivelled seed, chaff and leaf. Heavy particles including metal and stones can also be eliminated.It consists of an aspirated column with an adjustable flow rate, expansion chamber, air-return ducts and motor driven fan. The fan can easily be removed for cleaning. The unit is bench mounted.

_Attributes_
Description
	Laboratory Winnower

[PRODUCT] Grinder for Sample Preparation of Grains. 240V 50Hz 1Ph. (543-860/01)

_Attributes_
Description
	Grinder for Sample Preparation of Grains

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Micropropagation

[PRODUCT] Laminar Flow Cabinet 220-240V 50Hz 1Ph. (548-550/01)
Contaminant-free, non-turbulent air is essential for sterile inoculation of media during techniques such as tissue culture and micropropagation. Laminar flow cabinets force sterile air over the work surface and minimise the risk of external contamination and cross-contamination between two samples.The unit offered is smartly finished in white laminate and anodised alloy. It is self-contained and requires no external ducting. The variable speed fan is exceptionally quiet and reliable. The fan draws air first through a pre-filter and then through a secondary high efficiency particulate air (HEPA) filter. The sterile air is blown onto the work surface via ducts ensuring minimum turbulence.The cabinet has a clear air flow meter and filter clog indicator and the work surface is well lit to 1000 Lux by internal lights.

_Further Information_
For 220-240 V, 50 Hz, 1 ph.

_Attributes_
Description
	Laminar Flow Cabinet

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[CATEGORY] Harvesting and Storage

[PRODUCT GROUP] Seed samplers
Once a grain crop has been harvested and put into store, tests need to be carried out periodically to measure the quality and to check for pest or disease attack. Such samples must be representative of the bulk material and so need to be taken at various depths and from different locations.

[PRODUCT] Sack Spear Sampler 12.7mm Dia X 650mm Long. (560-210)

_Attributes_
Description
	Sack Spear Sampler 12.7 mm dia

[PRODUCT] Sack Spear Sampler 19mm Dia X 650mm Long. (560-212)

_Attributes_
Description
	Sack Spear Sampler 19 mm dia

[PRODUCT] 1m Sampling Spear 1 slot double tube 32mm o/d to include carrying case (560-220)

_Attributes_
Description
	1m Sampling Spear

[PRODUCT] 2m Sampling Spear 5 Slots Double Tube 32mm Od. Supplied with Carrying Case. (560-226)

_Attributes_
Description
	2m Sampling Spear

[PRODUCT] Vacuum Grain Sampler 220-240V 50Hz 1Ph. (560-225/01)

_Attributes_
Description
	Vacuum Grain Sampler

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Sample dividers

[PRODUCT] Sample Divider 12X12.7mm (560-194)

_Attributes_
Description
	Sample Divider
	
Slot width, mm
	12 x 12.7 mm

[PRODUCT] Sample Divider 12X6.35mm (560-196)

_Attributes_
Description
	Sample Divider
	
Slot width, mm
	12 x 6.35 mm

[GROUPED PRODUCT MATRIX]
Model No.
	Slot width, mm
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Moisture meters

[PRODUCT] Protimeter Grainmaster Moisture Meter with 15 Pre-Programmed Crop Calibrations. (560-020)
* Microprocessor controlled.* Automatic temperature compensation.* Instant LCD readings for many crops.* Temperature measurement facilities.A completely portable unit suited to in-store or field use. Incorporates instant digital-readout of moisture content and automatic temperature compensation for rapid and accurate moisture determinations.The simple 4 stage operation takes less than a minute per sample:* Insert the program key for the crop to be tested.* Place grinder over sample cell and grind sample.* Compress the sample.* Press "ON" switch and read moisture content.The unit is battery powered and can be used with a wide variety of crops using interchangeable program keys for direct readings. In addition, by using the probe accessory the meter may also be used to measure the temperature of stored grain, thus enabling the principle grain quality and storage checks to be carried out with one instrument.

_Further Information_
Supplied with sip-top pouch, compressor, hand grider, quick check standard, high check standard, storage case for program keys, calibration chart and prgram keys for ground samples of wheat and barley to ISO standard. Requires one PP3 battery - not included.Supplied with sip-top pouch, compressor, hand grider, quick check standard, high check standard, storage case for program keys, calibration chart and prgram keys for ground samples of wheat and barley to ISO standard. Requires one PP3 battery - not included.Supplied with sip-top pouch, compressor, hand grider, quick check standard, high check standard, storage case for program keys, calibration chart and prgram keys for ground samples of wheat and barley to ISO standard. Requires one PP3 battery - not included.Supplied with sip-top pouch, compressor, hand grider, quick check standard, high check standard, storage case for program keys, calibration chart and prgram keys for ground samples of wheat and barley to ISO standard. Requires one PP3 battery - not included.Supplied with sip-top pouch, compressor, hand grider, quick check standard, high check standard, storage case for program keys, calibration chart and prgram keys for ground samples of wheat and barley to ISO standard. Requires one PP3 battery - not included.

_Attributes_
Description
	Protimeter Grainmaster Moisture Meter

_Related Products_
Accessory: Fast Response Temperature Probe 1m Length. for Use with 560-020. (560-022)

[PRODUCT] Fast Response Temperature Probe 1m Length. for Use with 560-020. (560-022)
1 metre long with temperature program key.

_Attributes_
Description
	Fast Response Temperature Probe

_Related Products_
Main: Protimeter Grainmaster Moisture Meter with 15 Pre-Programmed Crop Calibrations. (560-020)

[PRODUCT] Moisture Meter for Baled Hay Straw and Tobacco with 600mm Long Probe. (560-038)
* Fast measurement of baled hay or straw.* Easy to read analogue display.* Built-in battery and calibration check.This lightweight hand-held instrument can be used for the rapid moisture measurement of baled hay or straw. The strong stainless steel probe is inserted into the bale and the test button pressed. The result is shown instantly on the clear analogue display. A separate button can be used to check the calibration and battery voltage.

_Further Information_
Supplied complete with probe and operating instructions.

_Attributes_
Description
	Moisture Meter for Baled Hay Straw and Tobacco

[PRODUCT] Universal Moisture Probe 1 Metre (560-095)
* Microprocessor controlled.* User programmable.* Displays temperature and moisture content.* 1 metre long insertion probe.The universal insertion moisture meter has been designed to measure the moisture content of powders, grain and granules. It has applications throughout industry but is particularly suited for use with stored seeds and grains. It can be used both for batch testing materials as they are loaded or unloaded as well as periodic checks while in storage.The probe is inserted into the sample and the result is shown instantly on the display. No weighing, grinding or other sample preparation is required. By pressing the membrane keypad the temperature of the sample can also be measured. The instrument can be programmed by the user for use with up to six crops. The simple calibration procedure means that data for new crops can be added as required.

_Further Information_
Complete with 1 metre long insertion probe and operating instructions.

_Attributes_
Description
	Universal Moisture Probe

[PRODUCT] Grain Airflow Meter. (560-050)
An essential aid for monitoring the airflow through stored srops to ensure adequate ventilation and prevent spontaneous-heating and associated condensation in grain stored slightly warm or above optimum moisture content. The information provided by this device will help prevent mildew development in store and the associated loss of revenue or benefit from cash and feed crop. The instrument is simply placed upon the stored grain and the upward airflow can then be read off one of two scales ranging from 8-30 ft/min or 2.5-9 m/min.

_Attributes_
Description
	Grain Airflow Meter

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Seed counters

[PRODUCT] Precision Seed Counter with Container for Cereals 220-240V 50Hz 1Ph (560-105/01)
* Automatic feed rate selection.* Very accurate results with small seeds.* Filter for undersized or damaged seeds.The precision seed counter is invaluable for laboratory work, research applications, 1000 grain counting and packaging of costly seeds. A special feature of the instrument is the very wide range of seed sizes which can be processed from 0.3 to 15 mm in diameter. The built-in vibrating unit automatically determines the optimum seed counting rate, although this can be set manually if required. The seed size can also be selected so that the damaged seeds or fragments of husk are eliminated from the result.Various count modes can be selected including normal, aggregate and differential. The unit is extremely quiet in operation, has an easy to read LCD display, RS232 output and a membrane key pad.

_Further Information_
Supplied with counting head for cereals and grains.

_Attributes_
Description
	Precision Seed Counter

_Related Products_
Accessory: Large Counting Head for Large Seeds Up to 15mm Diameter (560-105/12)
Accessory: Small counting head for small seeds down to 0.3 mm diameter (560-105/10)

[PRODUCT] Small counting head for small seeds down to 0.3 mm diameter (560-105/10)

_Attributes_
Description
	Small counting head

_Related Products_
Main: Precision Seed Counter with Container for Cereals 220-240V 50Hz 1Ph (560-105/01)

[PRODUCT] Large Counting Head for Large Seeds Up to 15mm Diameter (560-105/12)

_Attributes_
Description
	Large Counting Head

_Related Products_
Main: Precision Seed Counter with Container for Cereals 220-240V 50Hz 1Ph (560-105/01)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Yield quality

[PRODUCT] Hectronic Test Weight Kit (560-115)
* Rapid and consistent results.* Compact and easy-to-use.* Accurate for all grains.This instrument will benefit growers and merchants alike, providing useful feedback for the grower and easy-to-use method of grain quality for the merchant.The kit comprises an accurately measured cylinder and hopper (chondrometer) ensuring that a precise and replicable volume of grain is measured. The sample of grain is allowed to fall into the chamber of the chondrometer under the restriction of a falling weight so that a constant packing density is achieved. The grain is weighed on battery powered scales (6 x 1.5 V AA batteries required) which are included in the kit. The weight is then converted on the chart supplied to give the bushel or hectolitre weight. The unit is simple to use, provides accurate results to +-5% and can be used with all grains including wheat, oats, barley and maize. Conforms to Insernational Standard 7971 and British Standard BS4317 part 23.

_Further Information_
Supplied with a carrying case.

_Attributes_
Description
	Hectronic Test Weight Kit

[PRODUCT] Chondrometer. (560-118)
Light and accurate laboratory chondrometer suitable for use with any gramme balance capable of weighing up to 1400 g.

_Further Information_
Supplied with calibration chart.

_Attributes_
Description
	Chondrometer

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Size grading

[PRODUCT] Set of 6 Grain Sieves. (560-142)
* Laser cut for accuracy.* Non-magnetic stainless steel mesh.* Conform to BS6219 and ISO 5223.A set of 6, laser-cut stacking grain-sieves ensuring the utmost accuracy in grading. The set comprises four sieves with slots 20 mm long x 1.0; 2.0; 2.2; and 3.5 mm wide, made from hardwearing stainless steel plate to BS6219 and ISO 5223. Also included in the set are two stainless steel insect sieves 1.7 mm mesh and 710 um mesh, to aid the control of storage pests such as weevils and mites. A lid and receiver complete the set. Sieves conforming to other standards are available on request.

_Attributes_
Description
	Set of 6 Grain Sieves

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[CATEGORY] Environmental Laboratory Equipment

[PRODUCT GROUP] General laboratory instrumentation

[PRODUCT] Binocular Stereo Zoom Microscope (550-025/01)
* 4 objective nosepiece.* High quality optics.* Mechanical stage.This binocular miroscope has a sound, ergonomic design and is manufactured to a high standard. The excellent optical performance makes the instrument suitbale for both laboratory and teaching purposes. The built-in illumination with daylight filter provides an excellent light source for a wide range of applications.

_Further Information_
For 220-240 V, 50 Hz, 1 ph.

_Attributes_
Description
	Binocular Stereo Zoom Microscope

_Related Products_
Spare/Consumable: Bulb (Bottom Illumination) 12V/20W (550-025/12)
Spare/Consumable: Bulb (Top Illumination) 12V/10W (550-025/10)

[PRODUCT] Binocular Microscope 45 Deg Inclined 360 Deg Rotating Head Wf10X Eye- Piece 4X 10X & 40X (550-035/01)

_Attributes_
Description
	Binocular Microscope 45 Deg Inclined 360 Deg Rotating Head

_Related Products_
Accessory: Objective Lense 100X/1.25 (Oil). for Use with 550-035/01. (550-035/10)

[PRODUCT] Visible Range Spectro- Photometer with 100 Plastic Cuvettes (10 X 10mm) Cell Holder & Mains Lead (485-030/01)
* Microprocessor-controlled.* Digital display 320-920 nm wavelength.* Automatic zero and calibration.This instrument combines advanced electronics with a high quality optical system operating over the range 320-920 nm.The monochrominator is a modified Czerny Turner design. It incorporatesa cam-driven 1200 lines/mm holographic diffraction grating and features automatic second order resonse supression. The complete optical system is housed in an independently enclosed unit for maximum protection.Careful design has ensured that heat transfer to the sample is minimised. This enables precise measurements to be performed on a temperature dependent basis. A low noise, high stability and solid state detector for accurate reproducible results combined with a rigid structure provides a system with fast warm-up, low drift and high reliability

_Further Information_
Supplied complete with 100 plastic 10 x 10 mm cuvettes, 10 x 10 mm cell holder and mains lead.

_Attributes_
Description
	Visible Range Spectro- Photometer

[PRODUCT] Uv/Vis Spectrophotometer with 100 Plastic Cuvettes 10X10mm Cell Holder Instructions & Mains Lead (485-031/01)

_Attributes_
Description
	Uv/Vis Spectrophotometer

_Related Products_
Spare/Consumable: Spare Xenon lamp module (485-031/10)

[PRODUCT] Spare Xenon lamp module (485-031/10)

_Attributes_
Description
	Spare Xenon lamp module

_Related Products_
Main: Uv/Vis Spectrophotometer with 100 Plastic Cuvettes 10X10mm Cell Holder Instructions & Mains Lead (485-031/01)

[PRODUCT] Digital Colorimeter. (525-242/01)
* 8 built-in filters.* Dual cuvette holder.* Large LCD display.This range of colorimeters features a number of advanced measurement functions and is designed for educational laboratory and industrial functions. The instruments are housed in rugged, chemically resistant, structual foam mouldings and have ergonomically-efficient, sloping front panels.Both models feature 8 built-in gelatin filters covering the visible spectrum fitted onto a switched wheel. The dual cuvette holder enables the sample and a reference to be processed. Measurements can be taken in % transmittance, absorbance or concentration.

_Further Information_
A general purpose laboratory or portableunit which operates from mains supply or an external 12 V supply.It is supplied complete with 9 built-in filters, 100 displosable cuvettes, recorder output, mains lead and manual.

_Attributes_
Description
	Digital Colorimeter

_Related Products_
Accessory: Microsample Cuvettes 10Ml (Pack of 100). (525-246)

[PRODUCT] Microsample Cuvettes 10Ml (Pack of 100). (525-246)
Pack of 100.

_Attributes_
Description
	Microsample Cuvettes 10Ml

_Related Products_
Main: Digital Colorimeter. (525-242/01)

[PRODUCT] Bulb (Top Illumination) 12V/10W (550-025/10)

_Attributes_
Description
	Bulb (Top Illumination) 12V/10W

_Related Products_
Main: Binocular Stereo Zoom Microscope (550-025/01)

[PRODUCT] Bulb (Bottom Illumination) 12V/20W (550-025/12)

_Attributes_
Description
	Bulb (Bottom Illumination) 12V/20W

_Related Products_
Main: Binocular Stereo Zoom Microscope (550-025/01)

[PRODUCT] Objective Lense 100X/1.25 (Oil). for Use with 550-035/01. (550-035/10)

_Attributes_
Description
	Objective Lense 100X/1.25

_Related Products_
Main: Binocular Microscope 45 Deg Inclined 360 Deg Rotating Head Wf10X Eye- Piece 4X 10X & 40X (550-035/01)

[PRODUCT] Laboratory Conductivity Meter with Conductivity Cell Swing Arm Electrode Holder and Manual. (525-180/01)
* 5 measurement ranges.* Automatic temperature compensation.* Recorder output.This easy-to-use instuemtnmeasures conductivity over 5 ranges. Readings are automatically temperature compensated with a choice of either 20 or 25°C as a reference temperature. A zero control on the 20 micro Siemen range enables the elimination of cable capacities so ensuring accurate results.The unit has been designed for use with the range of conductivity cells specified, all of which are temperature compensated. However, other cells can be used in conjunction with the temperature compensation probe.

_Further Information_
Supplied complete with probe holder and conductivity level (K=1) and full operating instructions.

_Attributes_
Description
	Laboratory Conductivity Meter

_Related Products_
Spare/Consumable: Conductivity Cell K=1. (525-180/10)

[PRODUCT] Conductivity Cell K=1. (525-180/10)

_Attributes_
Description
	Conductivity Cell

_Related Products_
Main: Laboratory Conductivity Meter with Conductivity Cell Swing Arm Electrode Holder and Manual. (525-180/01)

[PRODUCT] Laboratory Ph Meter with Ph Electrode Swing Arm Temp Probe Manual and Buffer Capsules. (525-210/01)

_Attributes_
Description
	Laboratory Ph Meter

_Related Products_
Spare/Consumable: Spare Ph Probe for Lab Ph and Ion Meters. (525-210/10)

[PRODUCT] Spare Ph Probe for Lab Ph and Ion Meters. (525-210/10)

_Attributes_
Description
	Spare Ph Probe

_Related Products_
Main: Laboratory Ph Meter with Ph Electrode Swing Arm Temp Probe Manual and Buffer Capsules. (525-210/01)

[PRODUCT] Bench Dissolved oxygen meter (525-235/01)
* Measures DO2 over ranges 0-200%, 0-25% and 0-19.9 mg/l (ppm).* Measures temperature over the range -50 to +199.9°C.* Barometric pressure compensator.This unit has been designed for use in the laboratory for the measurement of dissolved oxygen accurately and with ease. Measurements can be obtained as % or mg/l and are automatically temperature compensated. All adjustments are made using multi-turn rotary controls and the results are displayed on an LED display.

_Attributes_
Description
	Bench Dissolved oxygen meter

[PRODUCT] Laboratory Ion meter with pH electrode, swing arm, temp probe. Manual+buffer capsules. 240V 50Hz 1ph (525-220/01)

_Attributes_
Description
	Laboratory Ion meter with pH electrode

_Related Products_
Accessory: Ammonia Ion Selective Electrode (Combination Type) (488-001)
Accessory: Ammonium Ion Selective Electrode (PVC) Combination Type (488-021)
Accessory: Barium Ion Selective Electrode (Combination Type) (488-002)
Accessory: Bromide Ion Selective electrode (Combination Type) (488-003)
Accessory: Cadmium Ion Selective electrode (Combination Type) (488-004)
Accessory: Calcium Ion Selective electrode (Combination Type) (488-005)
Accessory: Chloride Ion Selective electrode (Combination Type) (488-007)
Accessory: Copper Ion Selective electrode (Combination type) (488-008)
Accessory: Cyanide Ion Selective electrode (Combination type) (488-009)
Accessory: Fluoride Ion Selective electrode (Combination type) (488-010)
Accessory: Iodide Ion Selective electrode (488-011)
Accessory: Lead Ion Selective eletrode (Combination Type) (488-012)
Accessory: Nitrate Ion Selective Electrode (Combination Type) (488-013)
Accessory: Potassium Ion Selective electrode (488-014)
Accessory: Silver Ion Selective electrode (Combination Type) (488-015)
Accessory: Sodium Ion Selective electrode (Combination Type) (488-016)
Accessory: Sulphite Ion Selective electrode (Combination Type) (488-017)
Accessory: Water Hardness Ion Selective electrode (Combination Type) (488-019)

[PRODUCT] Ammonia Ion Selective Electrode (Combination Type) (488-001)

_Attributes_
Description
	Ammonia Ion Selective Electrode

_Specification_
Detection Limit
	0.02 ppm
	
Single Junction

Double Junction

_Related Products_
Main: Laboratory Ion meter with pH electrode, swing arm, temp probe. Manual+buffer capsules. 240V 50Hz 1ph (525-220/01)

[PRODUCT] Ammonium Ion Selective Electrode (PVC) Combination Type (488-021)

_Attributes_
Description
	Ammonium Ion Selective Electrode

_Related Products_
Main: Laboratory Ion meter with pH electrode, swing arm, temp probe. Manual+buffer capsules. 240V 50Hz 1ph (525-220/01)

[PRODUCT] Barium Ion Selective Electrode (Combination Type) (488-002)

_Attributes_
Description
	Barium Ion Selective Electrod

_Specification_
Detection Limit
	10 ppm
	
Single Junction
	Yes
	
Double Junction

_Related Products_
Main: Laboratory Ion meter with pH electrode, swing arm, temp probe. Manual+buffer capsules. 240V 50Hz 1ph (525-220/01)

[PRODUCT] Bromide Ion Selective electrode (Combination Type) (488-003)

_Attributes_
Description
	Bromide Ion Selective electrode

_Specification_
Detection Limit
	0.4 ppm
	
Single Junction

Double Junction
	Yes

_Related Products_
Main: Laboratory Ion meter with pH electrode, swing arm, temp probe. Manual+buffer capsules. 240V 50Hz 1ph (525-220/01)

[PRODUCT] Cadmium Ion Selective electrode (Combination Type) (488-004)

_Attributes_
Description
	Cadmium Ion Selective electrode

_Specification_
Detection Limit
	0.2 ppm
	
Single Junction
	Yes
	
Double Junction

_Related Products_
Main: Laboratory Ion meter with pH electrode, swing arm, temp probe. Manual+buffer capsules. 240V 50Hz 1ph (525-220/01)

[PRODUCT] Calcium Ion Selective electrode (Combination Type) (488-005)

_Attributes_
Description
	Calcium Ion Selective electrode

_Specification_
Detection Limit
	0.02 ppm
	
Single Junction
	Yes
	
Double Junction

_Related Products_
Main: Laboratory Ion meter with pH electrode, swing arm, temp probe. Manual+buffer capsules. 240V 50Hz 1ph (525-220/01)

[PRODUCT] Chloride Ion Selective electrode (Combination Type) (488-007)

_Attributes_
Description
	Chloride Ion Selective electrode

_Specification_
Detection Limit
	1.8 ppm
	
Single Junction

Double Junction
	Yes

_Related Products_
Main: Laboratory Ion meter with pH electrode, swing arm, temp probe. Manual+buffer capsules. 240V 50Hz 1ph (525-220/01)

[PRODUCT] Copper Ion Selective electrode (Combination type) (488-008)

_Attributes_
Description
	Copper Ion Selective electrode

_Specification_
Detection Limit
	0.3 ppm
	
Single Junction

Double Junction
	Yes

_Related Products_
Main: Laboratory Ion meter with pH electrode, swing arm, temp probe. Manual+buffer capsules. 240V 50Hz 1ph (525-220/01)

[PRODUCT] Cyanide Ion Selective electrode (Combination type) (488-009)

_Attributes_
Description
	Cyanide Ion Selective electrode

_Specification_
Detection Limit
	0.03 ppm
	
Single Junction

Double Junction
	Yes

_Related Products_
Main: Laboratory Ion meter with pH electrode, swing arm, temp probe. Manual+buffer capsules. 240V 50Hz 1ph (525-220/01)

[PRODUCT] Fluoride Ion Selective electrode (Combination type) (488-010)

_Attributes_
Description
	Fluoride Ion Selective electrode

_Specification_
Detection Limit
	0.01 ppm
	
Single Junction
	Yes
	
Double Junction

_Related Products_
Main: Laboratory Ion meter with pH electrode, swing arm, temp probe. Manual+buffer capsules. 240V 50Hz 1ph (525-220/01)

[PRODUCT] Iodide Ion Selective electrode (488-011)

_Attributes_
Description
	Iodide Ion Selective electrode

_Specification_
Detection Limit
	0.02 ppm
	
Single Junction

Double Junction
	Yes

_Related Products_
Main: Laboratory Ion meter with pH electrode, swing arm, temp probe. Manual+buffer capsules. 240V 50Hz 1ph (525-220/01)

[PRODUCT] Lead Ion Selective eletrode (Combination Type) (488-012)

_Attributes_
Description
	Lead Ion Selective eletrode

_Specification_
Detection Limit
	1.0 ppm
	
Single Junction

Double Junction
	Yes

_Related Products_
Main: Laboratory Ion meter with pH electrode, swing arm, temp probe. Manual+buffer capsules. 240V 50Hz 1ph (525-220/01)

[PRODUCT] Nitrate Ion Selective Electrode (Combination Type) (488-013)

_Attributes_
Description
	Nitrate Ion Selective Electrode

_Specification_
Detection Limit
	0.08 ppm
	
Single Junction

Double Junction
	Yes

_Related Products_
Main: Laboratory Ion meter with pH electrode, swing arm, temp probe. Manual+buffer capsules. 240V 50Hz 1ph (525-220/01)

[PRODUCT] Potassium Ion Selective electrode (488-014)

_Attributes_
Description
	Potassium Ion Selective electrode

_Specification_
Detection Limit
	0.04 ppm
	
Single Junction

Double Junction
	Yes

_Related Products_
Main: Laboratory Ion meter with pH electrode, swing arm, temp probe. Manual+buffer capsules. 240V 50Hz 1ph (525-220/01)

[PRODUCT] Silver Ion Selective electrode (Combination Type) (488-015)

_Attributes_
Description
	Silver Ion Selective electrode

_Specification_
Detection Limit
	0.01 ppm
	
Single Junction

Double Junction
	Yes

_Related Products_
Main: Laboratory Ion meter with pH electrode, swing arm, temp probe. Manual+buffer capsules. 240V 50Hz 1ph (525-220/01)

[PRODUCT] Sodium Ion Selective electrode (Combination Type) (488-016)

_Attributes_
Description
	Sodium Ion Selective electrode

_Specification_
Detection Limit
	25 ppm
	
Single Junction

Double Junction
	Yes

_Related Products_
Main: Laboratory Ion meter with pH electrode, swing arm, temp probe. Manual+buffer capsules. 240V 50Hz 1ph (525-220/01)

[PRODUCT] Sulphite Ion Selective electrode (Combination Type) (488-017)

_Attributes_
Description
	Sulphite Ion Selective electrode

_Specification_
Detection Limit
	0.003 ppm
	
Single Junction
	Yes
	
Double Junction

_Related Products_
Main: Laboratory Ion meter with pH electrode, swing arm, temp probe. Manual+buffer capsules. 240V 50Hz 1ph (525-220/01)

[PRODUCT] Water Hardness Ion Selective electrode (Combination Type) (488-019)

_Attributes_
Description
	Water Hardness Ion Selective electrode

_Specification_
Detection Limit
	0.2 ppm
	
Single Junction
	Yes
	
Double Junction

_Related Products_
Main: Laboratory Ion meter with pH electrode, swing arm, temp probe. Manual+buffer capsules. 240V 50Hz 1ph (525-220/01)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Kjedahl apparatus

[PRODUCT] Digestion Unit 8 place, semi-auto c/w block,rack, heat shield, exhaust, (525-355/01)
Supplied with digestion block, carrying rack with heat shield, exhaust system, two-tier console, instruction manual and 8 digestion tubes, 250 ml, 300 x 42 mm.

_Further Information_
For 220-240 V, 50/60 Hz, 1 ph.

_Attributes_
Description
	Digestion Unit 8 place

_Related Products_
Spare/Consumable: Digestion Tube Macro 250Ml (525-355/10)

[PRODUCT] Digestion Unit 20 Place Semi-Auto C/W Block Rack Heat Shield Exhaust Console & 250Ml Tubes (525-356/01)
Supplied with digestion block, carrying rack with heat shield, exhaust system, two-tier console, instruction manual and 20 digestion tubes, 250 ml, 300 x 42 mm.

_Further Information_
For 220-240 V, 50/60 Hz, 1 ph.

_Attributes_
Description
	Digestion Unit 20 Place

_Related Products_
Spare/Consumable: Digestion Tube Macro 250Ml (525-355/10)

[PRODUCT] Turbosog fume scrubber 220-240V 50/60Hz 1ph (525-370/01)
* Compact and space saving.* Corrosion proof and maintenance free.* Efficient, with low operating costs.The Turbosog is specially designed for the complete removal of fumes from both Kjeldahl and other inorganic acid digestions. It shows Kjeldahl digestions to be performed outisde the fume cupboard on the open bench.The fume scrubber consists of two separate parts, the Pre-separator and the Turbosog. The Pre-separator consists of two glass bottles in line between the exhaust manifold and the Turbosog. The first bottle acts as a condensate trap collecting moisture from the digestion of both water and H2SO4. The second bottle contains a neutralizing solution which removes over 90% of the acid fumes.The Turbosog is a centrifugal suction pump which pulls the reduced fumes and air flow through an inlet pipe into a water reservoir. A magnetic valve restricts water flow to a maximum of 50 litres per hour. The water level is kept constant as the unit empties by displacement. Any residual fumes are diluted and expelled with the waste water.

_Further Information_
Supplied with Turbosog pre-separator, 2 glass bottles, 1 glass insert for washing bottle, 1 glass insert for condensation bottle, isoversinic tubing and instruction manual.Power supply 220-240 V, 50/60 Hz, 1 ph.

_Attributes_
Description
	Turbosog fume scrubber

[PRODUCT] Automatic distillation unit 220-240V 50/60Hz 1ph (525-375/01)
* Fully automatic steam generator.* Electronic control of steam pressure and water level.* Programmable, utilising miroprocessor control.This distillation unit is fully automatic with full microprocessor control. The operator has only to insert the digestion tube and the distillate receiver vessel.The control display is a back-lit LCD with 2 x 16 character lines. Information is entered via the touch sensitive keypad which has numerical characters for entering distillation program parameters, and manual function keys to activate the chemical addition pumps and for programming.There are 10 programmes with 0-8 for Kjeldahl and associated distillations and 9 for alternative distillation work. Each of the programmes have the following variables entered in sequence. All the programme steps are controlled by time with chemical addition pumps having a known flow rate of 13 ml/second.The unit is divided into 4 chambers, distillation, instrumentation, steam generation and chemical pumps, for maximum protection of the various components. All the functions of the unit are monitored and errors are displayed on the character display.This unit has a manual end point titration.

_Further Information_
For 220-240 V, 50/60 Hz, 1 ph.

_Attributes_
Description
	Automatic distillation unit

_Related Products_
Accessory: Storage tanks for automatic distillation units-set of 3 (525-376)

[PRODUCT] Automatic distillation & titration system 220-240V 50/60Hz 1ph (525-380/01)
This is a fully automatic distillation and titration system, with microprocessor control and dialogue friendly software. The complete sequence of distillation, titration and calculation can be performed without intervention. This means a fast and accurate assay can be made with minimum supervision.The system has 4 main programme modes for fully automated Kjeldahl determinations:* Weight mode- Sample weight, memory for 220 samples.- Entry in g or ml.- Data entry by keyboard or RS232C interface directly from a balance.* Sample mode- 9 selectable programmes for micro/macro Kjeldahl distillations, direct distillations and nitrate analysis.- Electronic control of distillation and titration by the microprocessor with display reading of the programme steps or error codes, with calculation of results.* Calibration mode- Automatic calibration of pH electrode.- Automatic blank analysis for each of the 9 distillation programmes.- Automatic determination of the blank value of each of the distillation programmes.- Automatic analysis of a standard with recovery calculation.* Programme mode- Data entry for each of the 9 distillation programmes.- Data entry for the titration programmes.- For each of the 9 distillation programmes there are programmable titration and burette steps. The pH endpoint titration system uses a motor-burette with an interchangeable 25 ml syringe to 0.01 ml accuracy.The software is flexible and the following types of data can be programmed into the sustem. For example:* Sample weight entry.* Fixed or automatic distillation time.* pH endpoint for automatic or fixed titration.* Volume of H2O.* Volume of NaOH.* Time of suction sample.* Result calculation.* Filling and emptying of receiver vessel.

_Further Information_
With titrator and calculator. Microprocessor controlled ready for full operation. With instruction manual. For 220-240 V, 50/60 Hz, 1 ph.

_Attributes_
Description
	Automatic distillation & titration system

[PRODUCT] Digestion Tube Macro 250Ml (525-355/10)

_Attributes_
Description
	Digestion Tube Macro 250Ml

_Related Products_
Main: Digestion Unit 20 Place Semi-Auto C/W Block Rack Heat Shield Exhaust Console & 250Ml Tubes (525-356/01)
Main: Digestion Unit 8 place, semi-auto c/w block,rack, heat shield, exhaust, (525-355/01)

[PRODUCT] Storage tanks for automatic distillation units-set of 3 (525-376)
20 litres with level switch and connector to microprocessor.

_Attributes_
Description
	Storage tanks for automatic distillation unit

_Related Products_
Main: Automatic distillation unit 220-240V 50/60Hz 1ph (525-375/01)

[PRODUCT] Spare Parts Kit for 525-380/01 for 2 Years Operation. (525-384)

_Attributes_
Description
	Spare Parts Kit for Automatic distillation & titration system

_Related Products_
Spare/Consumable: Spare Parts Kit for 525-380/01 for 2 Years Operation. (525-384)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Soxhlet apparatus

[PRODUCT] Basic 4-Place Soxhlet Extraction System Less Glassware & Connections 220-240V 50/60Hz 1Ph. (525-400/01)
The soxhlet apparatus is ued for the continuous extraction of fats and oils from solid material using an organic solvent such as petroleum ether. In a practical agricultural context the method is usually applied to the determination of "oil content" in agricultural produce such as sunflower and other oil seeds.The material to be extracted is usually placed in a porous paper thimble and continuously condensing solvent allowed to perculate through it before returning to the boiling vessel either continuously or intermittently. The solvent can then be evaporated off to leave the fat.A 4 place and 6 place system is available. Each heating unit has individual hotplates of 85 mm diameter with stepless heating control so that the temperature of each hotplate can be operated individually. The heating unit has a lacquered sheet steel casing with an enamelled top plate. The basic extraction system is supplied complete with top moulds, air bath inserts support rods, 600 x 12 mm and a connection cable.

_Attributes_
Description
	Basic 4-Place Soxhlet Extraction System

_Related Products_
Accessory: Cooling Water Feed Pipe for 525-400 Series with 4 Fastening Clamps (525-405)
Accessory: Holder with Clamp for Soxhlet Glass Parts (525-404)
Accessory: Paper Thimble Double Thickness 22 X 80mm Box of 25. (525-423)
Accessory: Set of Soxhlet Glass Parts Including 1 Flask 500Ml 1 Extractor 150Ml and Condenser (525-403)

[PRODUCT] Set of Soxhlet Glass Parts Including 1 Flask 500Ml 1 Extractor 150Ml and Condenser (525-403)
Consisting of 1 flat bottomed flask 500 ml, 1 extractor 150 ml capacity and 1 condenser.

_Attributes_
Description
	Set of Soxhlet Glass Parts

_Related Products_
Main: Basic 4-Place Soxhlet Extraction System Less Glassware & Connections 220-240V 50/60Hz 1Ph. (525-400/01)
Main: Basic 6-Place Soxhlet Extraction System Less Glassware & Connections 220-240V 50/60Hz 1Ph. (525-402/01)

[PRODUCT] Holder with Clamp for Soxhlet Glass Parts (525-404)
For Soxhlet Glass Parts

_Attributes_
Description
	Holder with Clamp for Soxhlet Glass Parts

_Related Products_
Main: Basic 4-Place Soxhlet Extraction System Less Glassware & Connections 220-240V 50/60Hz 1Ph. (525-400/01)
Main: Basic 6-Place Soxhlet Extraction System Less Glassware & Connections 220-240V 50/60Hz 1Ph. (525-402/01)

[PRODUCT] Cooling Water Feed Pipe for 525-400 Series with 4 Fastening Clamps (525-405)
Made of nickel plated brass, for intake and outflow, with 4 fastening clamps.

_Attributes_
Description
	Cooling Water Feed Pipe 4 Fastening Clamps

_Related Products_
Main: Basic 4-Place Soxhlet Extraction System Less Glassware & Connections 220-240V 50/60Hz 1Ph. (525-400/01)

[PRODUCT] Cooling Water Feed Pipe for 525-402 Series with 6 Fastening Clamps. (525-406)
Made of nickel plated brass, for intake and outflow, with 4 fastening clamps.

_Attributes_
Description
	Cooling Water Feed Pipe 6 Fastening Clamps

_Related Products_
Main: Basic 6-Place Soxhlet Extraction System Less Glassware & Connections 220-240V 50/60Hz 1Ph. (525-402/01)

[PRODUCT] Paper Thimble Single Thickness 28 X 80mm Box of 25. (525-420)
Box of 25.

_Attributes_
Description
	Paper Thimble Single Thickness

[PRODUCT] Paper Thimble Double Thickness 22 X 80mm Box of 25. (525-423)
Box of 25.

_Attributes_
Description
	Paper Thimble Double Thickness

_Related Products_
Main: Basic 4-Place Soxhlet Extraction System Less Glassware & Connections 220-240V 50/60Hz 1Ph. (525-400/01)
Main: Basic 6-Place Soxhlet Extraction System Less Glassware & Connections 220-240V 50/60Hz 1Ph. (525-402/01)

[PRODUCT] Basic 6-Place Soxhlet Extraction System Less Glassware & Connections 220-240V 50/60Hz 1Ph. (525-402/01)
The soxhlet apparatus is ued for the continuous extraction of fats and oils from solid material using an organic solvent such as petroleum ether. In a practical agricultural context the method is usually applied to the determination of "oil content" in agricultural produce such as sunflower and other oil seeds.The material to be extracted is usually placed in a porous paper thimble and continuously condensing solvent allowed to perculate through it before returning to the boiling vessel either continuously or intermittently. The solvent can then be evaporated off to leave the fat.A 4 place and 6 place system is available. Each heating unit has individual hotplates of 85 mm diameter with stepless heating control so that the temperature of each hotplate can be operated individually. The heating unit has a lacquered sheet steel casing with an enamelled top plate. The basic extraction system is supplied complete with top moulds, air bath inserts support rods, 600 x 12 mm and a connection cable.

_Attributes_
Description
	Basic 6-Place Soxhlet Extraction System

_Related Products_
Accessory: Cooling Water Feed Pipe for 525-402 Series with 6 Fastening Clamps. (525-406)
Accessory: Holder with Clamp for Soxhlet Glass Parts (525-404)
Accessory: Paper Thimble Double Thickness 22 X 80mm Box of 25. (525-423)
Accessory: Set of Soxhlet Glass Parts Including 1 Flask 500Ml 1 Extractor 150Ml and Condenser (525-403)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group