[DEPARTMENT] Soils

[CATEGORY] In-situ Sampling and Preparation
The correct sampling, description and preparation of soil and soil mixtures is necessary if subsequent tests are to be meaningful and provide representative results. Various national and international standards specify a range of procedures and equipment necessary to ensure representative sampling.

[PRODUCT GROUP] Soil Colour Charts

[PRODUCT] Soil Colour Chart Set (23-7150)
The Munsell Soil Color Charts is an affordable way to evaluate the type of soil that is present within a given area. The book is set up to allow users to make soil color evaluations in the field quickly and easily. The soil classification system that has been developed around the Munsell color system is an established and accepted process to assign a soil type. This classification system has been used in the United States for more than 55 years to aid in the management and stewardship of natural resources. Through the use of the Munsell Soil Color Charts, practitioners from a wide range of professions can share reliable and consistent information about the color of soils at a particular site with colleagues anywhere around the world. The Munsell Soil Color Charts are used by a variety of industries and professions such as universities and high schools, forestry, forensics, environmental and soil science, building and contracting, landscaping, real estate, health departments, geology and archaeology.

_Further Information_
The following pages are included in the Munsell Soil Color Charts:  	* Munsell 10R Soil Chart 	* Munsell 10YR Soil Chart 	* Munsell 2.5Y Soil Chart 	* Munsell 2.5YR Soil Chart 	* Munsell 5Y Soil Chart 	* Munsell 5YR Soil Chart 	* Munsell 7.5YR Soil 	* 10Y - 5GY Colors - Olive greens Soil Chart 	* Gley 1 & 2 (2 - Separate Charts) Soil Charts 	* Munsell 5R Individual Soil Chart 	* Munsell 7.5R Individual Soil Chart 	* "New" White Page, 7.5R, 10YR, & 2.5Y

_Attributes_
Weight, kg
	0.91
	
Description
	Soil Colour Chart Set

_Specification_
Munsell Book of Soil Color Charts

 

Durable binder contains 440 Munsell Color Standards

• Featuring ISCC-NBS color names

• Munsell alpha-numeric notation

 

Color produced on water resistant substrate

 

Features Munsell notations for each color providing:

• Value (degree of lightness)

• Hue (color)

• Chroma (degree of saturation)

 

Used with medium, fine-grained, and coarse-grained rocks

 

Pages are cleanable and can be exposed to standard environmental conditions in the field

 

Dimensions

• Binder Size 6" x 7.75" x 1"

• Page Size 4 3/8" x 7 1/4"

• Weight 3 lbs. or 1. kg

_Related Products_
Main: Sand Grading Chart (23-7130)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Sample Mixers
A regular laboratory requirement is the mixing of samples with water and/or other constituents to provide a homogeneous mixture prior to subsequent testing. The following range of mixers provide an efficient means of mixing samples.

[PRODUCT] Bench-Mounting Mixer 4.7Litre Capacity Complete with Bowl Beater and Whisk. 220-240V 50Hz 1Ph. (23-6191/01)
The mixer has two electrically switched mixing speeds which obviates the need to switch off during speed selection. The mixing head comprises a beater which contra-rotates about a central shaft using planetary gearing. A lever-acting lifting device facilitates the insertion and removal of the bowl. This mixer is suitable for the mixing of soil samples, mortar, bituminous mixtures and associated materials where comparatively small samples are being prepared. Supplied with stainless steel bowl, beater and whisk.

_Standards_
BS 598-107, BS 1377-1, BS 1924-1

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Bench-Mounting Mixer
	
Voltage Supply
	220 - 240 V AC, 50 Hz, 1ph

_Specification_
Dimensions
	545 x 380 x 550 mm
	
Beater Speeds (rpm) low, high
	140, 285
	
Central shaft speeds (rpm) low, high
	62, 125
	
Rated power
	500 W
	
Weight
	50 kg

_Related Products_
Accessory: Isomantle Electric Heater (45-5580/01)
Spare/Consumable: Stainless Steel Bowl 4.73 Litres. (23-6191/10)

[PRODUCT] Stainless Steel Bowl 4.73 Litres. (23-6191/10)
For use with the 5 Litre Bench Mounted Mixer - 23-6191/01

_Attributes_
Description
	Stainless Steel Bowl

_Related Products_
Main: Bench-Mounting Mixer 4.7Litre Capacity Complete with Bowl Beater and Whisk. 220-240V 50Hz 1Ph. (23-6191/01)

[PRODUCT] Isomantle Electric Heater (45-5580/01)
For use with 23-6191 Bench Mounting Mixer.

_Standards_
EN 12697-35

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Isomantle Electric Heater
	
Voltage Supply
	220 - 240 V AC, 50/60 Hz, 1 ph

_Related Products_
Main: Bench-Mounting Mixer 4.7Litre Capacity Complete with Bowl Beater and Whisk. 220-240V 50Hz 1Ph. (23-6191/01)

[GROUPED PRODUCT MATRIX]
Model No.
	Voltage
	Desc
	N/A for this Product Group

[CATEGORY] Hand Boring and Sampling
The items listed provide the engineer with an economic range of equipment for field survey work. Using this equipment it is possible to obtain disturbed or undisturbed samples at reasonable depths, subject to ground conditions. Most items may be inter-connected.

[PRODUCT GROUP] Soil and Gravel Auger Heads
These auger heads are suitable for boring in cohesive soils or sands and gravels. The soil augers are constructed of heavy duty steel plates forming an open tube partly interlocked at the cutting end. Gravel augers comprise a one piece steel casting with a spiral point and two plates designed to close when lifting samples from the borehole. The Dutch Auger is of similar construction to the Soil Augers and is particularly useful in very fine silt-clay sands.

[GROUPED PRODUCT MATRIX]
Model No.
	Dia.
	Cohesive
	Gravel/Sand
	Silty Sand
	Weight, kg
	
23-1501
	100 mm
	Yes
	-
	-
	1.5
	
23-1504
	150 mm
	Yes
	-
	-
	2.5
	
23-1517
	150 mm
	-
	Yes
	-
	1.2
	
23-1525
	50 mm
	-
	-
	Yes
	1.5

[PRODUCT GROUP] Extension Rods, Handles and Tools

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	
23-1541
	Extension rod
	
23-1543
	Wrench
	
23-1547
	Handle and T piece
	
23-1577
	Sample tube 38 mm
	
23-1587
	Jarring Link
	
23-1617
	Spiral Auger 40 mm dia

[PRODUCT GROUP] Riffle Boxes (Sample Dividers)
Designed for the rapid preparation of samples, the ELE range of riffle boxes are constructed of heavy gauge sheet metal, with particular attention given to reinforcement of the partitions to maintain the accuracy of the slot dimensions. The units offered are supplied in a range of sizes from 7 mm to 64 mm slots.

[GROUPED PRODUCT MATRIX]
Model No.
	No. slots
	Max part. size mm BS
	Max part. size EN
	Slot width, mm
	
23-3000
	12
	4.5
	3.5
	7
	
23-3050
	12
	8.5
	6.5
	13
	
23-3070
	12
	10.0
	7.5
	15
	
23-3100
	10
	12.5
	9.5
	19
	
23-3150
	10
	16.5
	12.5
	25
	
23-3170
	10
	20.0
	15.0
	30
	
23-3200
	8
	25.0
	19.0
	38.0
	
23-3300
	8
	33.0
	25.0
	50
	
23-3350
	8
	42.5
	32
	64

[PRODUCT GROUP] Large Sample Splitter

[PRODUCT] Large Capacity Sample Splitter. (23-3425)
The splitter is designed for the reduction of test samples which are too large in volume to be conveniently handled. The splitter handles samples up to 6 inch diameter. It has much flexibility in size of opening and adjustment is provided for chutes of 0.5 1.5 2 3 4 or 6 inch by the chute bars’ positioning. The unit is lever actuated and is of a heavy gauge, welded steel construction.

_Further Information_
Complete with 2 material pans and a bag-loading chute.

_Attributes_
Description
	Sample Splitter
	
Material Pans
	Two included; 25 -3/4” l. x 9” w. x 6-1/2” h. (654 x 22 9 x 165 mm).

_Specification_
Capacity
	1 cu. ft. (0.028 m3); for sand sizes up to 4â€ (102 mm).
	
Hopper
	Lever-actuated, clamshell design.
	
Chute Bars
	48 aluminum bars, 1/2â€ (13 mm) width.
	
Chute Area
	24 â€ (610 mm) overall width.
	
Chute Openings
	Adjustable; 1/2â€, 1â€, 1-1/2â€, 2â€, 3â€, 4â€, or 6â€.
	
Frame
	Welded, heavy-gage steel.
	
Chute Attachment
	Replaces pan to allow sample collection in bag; 28-1/4â€ l. x 7â€w. x 5-1/2â€ h. (718 x 178 x 14 0 mm).
	
Material Pans
	Two included; 25 -3/4â€ l. x 9â€ w. x 6-1/2â€ h. (654 x 22 9 x 165 mm).
	
Overall Dimensions
	29â€ l. x 19â€ w. x 39â€ h. (737 x 483 x 999 mm).
	
Weight
	Shpg. 142 lbs. (64 kg).

_Related Products_
Main: Large Capacity Sample Splitter. (23-3425)
Accessory: Sample Bag - 10” x 18” (254 x 457 mm) (23-1420)
Accessory: Sample Bag - 17” x 32” (432 x 813 mm) (23-1422)
Main: Sample Splitter (Riffle Box) - 14 chutes, 1/2” (13 mm) chute width (23-3052)
Main: Sample Splitter (Riffle Box) - 14 chutes, 3/4” (19 mm) chute width (23-3102)
Main: Sample Splitter (Riffle Box) - 16 chutes, 1” (25 mm) chute width (23-3152)
Main: Sample Splitter (Riffle Box) - 8 chutes, 2-1/2” (64 mm) chute width (23-3352)
Main: Sample Splitter (Riffle Box) - 8 chutes, 2” (51 mm) chute width (23-3302)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Sample Reduction
The reduction of particles within the soil mass is necessary for a number of tests. For most purposes crushing of individual particles must be avoided. This reduction process is best achieved using a porcelain mortar and rubber headed pestle.

[PRODUCT] Rubber Headed Pestle. (23-3500)
Specially made for gently grinding soils without breaking the individual particles. Suitable for BS 1377, 1924; ASTM D421; AASHTO T87.

_Standards_
BS 1377, BS 1924, ASTM D421, AASHTO T87

_Attributes_
Description
	Rubber Headed Pestle
	
Weight, kg
	0.12

_Related Products_
Main: Mortar and Pestle Porcelain. (23-3505)

[PRODUCT] Mortar and Pestle Porcelain. (23-3505)
Thick walled porcelain mortar; 107mm internal diameter and porcelain pestle.

_Attributes_
Description
	Mortar and Pestle

_Related Products_
Main: Heat of Hydration Apparatus (38-4600/01)
Main: Heat of Hydration Apparatus (38-4600/06)
Main: Rubber Headed Pestle. (23-3500)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[CATEGORY] Extruders and Soil Lathes
The removal of soil cores from sampling tubes must be accomplished with the minimum of disturbance, particularly when small specimens have to be prepared in order to carry out laboratory tests. Large extrusion forces used indiscriminately will compress soil resulting in false values of shear strength and consolidation.

[PRODUCT GROUP] Soil Extruders

[PRODUCT] 38mm Hand Operated Hydraulic Sample Extruder with Trimming Knife 38mm Split Former & Cutting Tool. (23-4090)
This Sample Extruder comprises a vertically mounted lever action hydraulic jack, with the body extended to form a chamber which accommodates a 38 mm diameter sample tube. Supplied complete with trimming knife, 38 mm split former and wire saw.

_Standards_
BS 1377-1

_Attributes_
Description
	Hydraulic Extruder

_Related Products_
Main: Cbr/Core Cutter Extruder Frame and Hydraulic Jack Extrudes 150mm/6 Inch Diameter Specimens. (23-4250)
Main: Proctor/Core Cutter Extruder Frame and Hydraulic Jack. Extrudes 100mm/4 Inch Diameter Specimens (23-4200)

[PRODUCT] Proctor/Core Cutter Extruder Frame and Hydraulic Jack. Extrudes 100mm/4 Inch Diameter Specimens (23-4200)
Adaptor plates will be supplied; extrudes samples from BS Compaction Mould, Proctor Mould 100 mm, Core Cutter and Marshall Mould. Maximum extrusion force 20kn.

_Standards_
BS 1377-1

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Proctor /Core Cutter Extruder
	
Extrudes samples from
	BS compaction mould<br>Proctor Mould<br>100 mm core cutter<br>Marshall mould

_Related Products_
Main: 38mm Hand Operated Hydraulic Sample Extruder with Trimming Knife 38mm Split Former & Cutting Tool. (23-4090)
Main: Cbr/Core Cutter Extruder Frame and Hydraulic Jack Extrudes 150mm/6 Inch Diameter Specimens. (23-4250)
Main: Marshall Test 50 (45-6810/01)
Accessory: Steel Block (45-6463)

[PRODUCT] Cbr/Core Cutter Extruder Frame and Hydraulic Jack Extrudes 150mm/6 Inch Diameter Specimens. (23-4250)
Comprises a frame and hydraulic jack with adaptor plate supplied. Extrudes samples from BS CBR Mould and ASTM CBR Mould.

_Standards_
BS 1377-1

_Attributes_
Description
	CBR/Extruder
	
Extrudes samples from
	BS CBR mould<br>ASTM CBR mould

_Related Products_
Main: 38mm Hand Operated Hydraulic Sample Extruder with Trimming Knife 38mm Split Former & Cutting Tool. (23-4090)
Accessory: Adaptor Plate for 23-4250 to Extrude 100mm/4 Inch Diameter and Marshall Specimens. (23-4300)
Main: Proctor/Core Cutter Extruder Frame and Hydraulic Jack. Extrudes 100mm/4 Inch Diameter Specimens (23-4200)

[PRODUCT] Adaptor Plate for 23-4250 to Extrude 100mm/4 Inch Diameter and Marshall Specimens. (23-4300)
For use with 23-4250. Comprising an adaptor plate, retaining screws and a nominal 100 mm ram plunger. Enables extrusion from all ELE 100 mm moulds and core cutters listed in the table.

_Standards_
BS 1377-1

_Further Information_
Two extruders comprising a frame and hydraulic jack supplied with adaptor plates to enable a range of sample extrusion from all ELE moulds indicated in the table.

_Attributes_
Description
	Adaptor plate
	
Weight, kg
	2.2

_Related Products_
Main: Cbr/Core Cutter Extruder Frame and Hydraulic Jack Extrudes 150mm/6 Inch Diameter Specimens. (23-4250)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	Extrudes from
	N/A for this Product Group

[PRODUCT GROUP] Soil Lathes

[PRODUCT] Hand Operated Soil Lathe for 38mm Dia Specimens Up to 100mm Long. (23-5800)
For producing 38 mm diameter specimens. The lathe platen is adjustable in height and will accept specimens up to 100 mm in length.

_Standards_
BS 1377-1

_Further Information_
 	* Lightweight frame construction for both laboratory and field use. 	* Sturdy plated steel uprights serve as guides for wire saw during final trimming procedure. 	* Adjustable upper platen trimming for various sample heights.Wire Saw and other trimming accessories not included; order separately.  

_Attributes_
Description
	Hand Operated Soil Lathe
	
38 mm Sample
	Yes
	
Maximum specimen length
	100 mm
	
Specimen Diameter mm
	38 mm

_Related Products_
Main: 1.4" and 2.8" Hand Specimen Trimmer (23-5802)
Accessory: Trimming Knife (81-0710)

[PRODUCT] 1.4" and 2.8" Hand Specimen Trimmer (23-5802)
Specimen Trimmers are designed to simplify precision trimming of soil samples for triaxial, shear, unconfined compression, and other tests requiring standard cylindrical specimens. This trimming frame is supplied complete with vane type grips for both 1.4" (35 mm) and 2.8" (70 mm) diameter specimens, and a narrow wire saw.

_Further Information_
 	* Lightweight frame construction for both laboratory and field use. 	* Sturdy plated steel uprights serve as guides for wire saw during final trimming procedure. 	* Samples are held securely during trimming through vane type grips. 	* Adjustable upper gripper platen for various sample heights. 	* Plated steel uprights and gripper assemblies for rust resistance and long life.Includes Wire Saw.

_Attributes_
Description
	Hand Specimen Trimmer
	
1.4" (35 mm)
	Yes
	
2.8" (70 mm)
	Yes

_Specification_

	
Sample Size.
	Trims samples to either 1.4" (35 mm) or 2.8" (70 mm) diam.
	
Uprights.
	Positioned to guide wire saw to control final sample diam; plated steel.
	
Sample Grips.
	Vane type; hold sample during trimming; plated steel.
	
Overall Dimensions.
	7" w. x 5" d. x 14" h. (178 x 127 x 356 mm).
	
Weight.
	Net 16 lbs. (7.3 kg).

_Related Products_
Main: Hand Operated Soil Lathe for 38mm Dia Specimens Up to 100mm Long. (23-5800)
Accessory: Trimming Knife (81-0710)

[PRODUCT] Trimming Knife (81-0710)

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Trimming Knife

_Related Products_
Main: 1.4" and 2.8" Hand Specimen Trimmer (23-5802)
Main: Hand Operated Soil Lathe for 38mm Dia Specimens Up to 100mm Long. (23-5800)

[GROUPED PRODUCT MATRIX]
Model No.
	38 mm
	Desc
	1.4" (35 mm)
	2.8" (70 mm)
	N/A for this Product Group

[CATEGORY] Moisture Content

[PRODUCT GROUP] Rapid method by Speedy Moisture Tester
* Reliable and accurate moisture measurement in the field* Direct reading in percent moisture* Rapid results in minutes* New versions with heavy duty plastic carrying case and portable electronic balanceThe new range of Speedy Moisture testers now includes an electronic balance and a heavy duty plastic case. Designed for the most demanding on-site conditions, the new waterproof and durable case offers high levels of protection. The new model comprises: Speedy Moisture tester, electronic balance, beaker, cleaning cloth, cap, washer, scoop, steel pulverising balls, and cleaning brushes. Used to weigh a sample before placing it in the Speedy Moisture Tester, the portable battery powered balance includes LCD display with a measuring range 0 - 200 g x 0 g. The % moisture content of the sample is read directly from the calibrated pressure gauge.

[GROUPED PRODUCT MATRIX]
Model No.
	Model
	Moisture range
	Gauge div.
	Sample wgt.
	
23-7452
	D2 Large
	0 to 20
	0.2
	20
	
23-7462
	G2 Large
	0 to 50
	0.5
	8
	
23-7502
	D2 Small
	0 to 20
	0.2
	6

[PRODUCT GROUP] Accessories for the Speedy Moisture Tester

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	
23-7600
	Speedy Calibration Unit
	
23-7700
	Calcium carbide powder - 500g
	
23-7702
	Calcium carbide powder - 12 x 500 g

[PRODUCT GROUP] Oven Drying Method
The standard method for determining the moisture content of soil is the Oven Drying Method, which is recommended for a Soils Laboratory.

[GROUPED PRODUCT MATRIX]
Model No.
	Voltage
	Desc
	Fluctuation
	Shelves
	Positions
	Capacity, litres
	Int. Dimensions
	Temp. Range °C
	
78-1225/01
	220-240 V 50/60Hz
	Drying Oven
	+/- 0.75 °C
	3
	4
	100
	460 x 490 x 450 mm
	40 - 250 °C
	
78-1235/01
	220-240 V 50/60 Hz
	Drying Oven
	+/- 0.75 °C
	3
	5
	150
	540 x 490 x 550 mm
	40 - 250 °C
	
78-1250/01
	220-240 V 50/60 Hz
	Drying Oven
	+/- 0.75 °C
	3
	4
	225
	440 x 920 x 600 mm
	0 - 200 °C
	
78-0135/01
	220-240 V 50/60 Hz
	Drying Oven
	+/- 0.75 °C
	4
	5
	425
	640 x 920 x 760 mm
	0 - 200 °C
	
78-1215/01
	220-240 V 50/60 Hz
	Drying Oven
	+/- 0.75 °C
	2
	3
	50
	330 x 490 x 330 mm
	40 - 250 °C

[CATEGORY] Soil Index Properties
Soil index properties are used extensively by engineers to discriminate between the different kinds of soil within a broad category, e.g clay will exhibit a wide range of engineering properties depending on its composition.

[PRODUCT GROUP] Determination of Plastic Limit
The plastic limit is defined as the lowest moisture content of a soil that will permit a sample to be rolled into threads of 3 mm diameter without the threads breaking. The test procedure has remained, in principle, the same since 1932, when Casagrande proposed to define the various limits by relating the moisture content characteristics of soil under certain conditions. The apparatus required is simple yet effective. The majority of the apparatus required for this test is standard laboratory equipment. For full details see the Laboratory equipment section of the catalogue.

[PRODUCT] Glass Plate. (24-0430)
500 mm square x 10 mm thick.

_Standards_
BS 1377, EN 1997-2

_Attributes_
Description
	Glass plate
	
BS/EN Standard
	Yes

_Related Products_
Main: Bulk Density Measure 10 Litre (34-2830)
Main: Liquid Limit Device BS with Counter. C/W Metal Grooving Tool & Test Gauge. (24-0410)
Main: Motorised Liquid Limit Device W/ Counter BS 220-240V 50Hz 1Ph. (24-0417/01)

[PRODUCT] Rod Comparator (24-0811)
3mm diameter rod comparator to BS1377.

_Standards_
BS 1924-2, EN 1997-2, ASTM D4318, BS 1377, AASHTO T90

_Attributes_
Description
	Rod comparator
	
Diameter, ”
	3

[PRODUCT] Spatula 200 mm (81-0140)

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Spatula 200 mm

_Related Products_
Accessory: Vibrating Hammer (47-0455/01)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[CATEGORY] Determination of Liquid Limit
The condition of a soil can be altered by changing the moisture content. The liquid limit is the empirically established moisture content at which a soil passes from the plastic to the liquid state. A knowledge of the liquid limit allows the engineer to correlate several engineering properties with the soil. Two main types of test are used; the Casagrande type (Cup), which has been used for many years, and the cone penetrometer method, which is now the definitive method specified in BS 1377.

[PRODUCT GROUP] Casagrande Method
Particular design features of the instrument include a positive action horizontal lead screw, which is rapidly adjustable and rigidly fixes the height of cup in relation to the base during the test procedure. The cam mechanism and cup suspension assembly have been designed to withstand constant use with minimum readjustment

[PRODUCT] Liquid Limit Device BS with Counter. C/W Metal Grooving Tool & Test Gauge. (24-0410)
With revolution counter. Complete with metal grooving tool and test gauge.

_Standards_
BS 1377, EN 1997-2

_Attributes_
Description
	Liquid limit device
	
BS/EN Standard
	Yes
	
Weight, kg
	5

_Related Products_
Accessory: Glass Plate. (24-0430)
Accessory: Grooving Tool and Gauge B.S. (24-0425)
Main: Motorised Liquid Limit Device W/ Counter BS 220-240V 50Hz 1Ph. (24-0417/01)

[PRODUCT] Motorised Liquid Limit Device W/ Counter BS 220-240V 50Hz 1Ph. (24-0417/01)
Complete with revolution counter and motor.

_Standards_
BS 1377, EN 1997-2

_Attributes_
Description
	Liquid limit device - motorised
	
BS/EN Standard
	Yes
	
Power Supply
	220 - 240 V AC, 50 Hz, 1 ph

_Related Products_
Accessory: Glass Plate. (24-0430)
Accessory: Grooving Tool and Gauge B.S. (24-0425)
Main: Liquid Limit Device BS with Counter. C/W Metal Grooving Tool & Test Gauge. (24-0410)

[PRODUCT] Grooving Tool and Gauge B.S. (24-0425)
Constructed to British Standards.

_Standards_
BS 1377, EN 1997-2

_Attributes_
Description
	Grooving tool
	
BS/EN Standard
	Yes
	
Weight, kg
	0.145

_Related Products_
Main: Liquid Limit Device BS with Counter. C/W Metal Grooving Tool & Test Gauge. (24-0410)
Main: Motorised Liquid Limit Device W/ Counter BS 220-240V 50Hz 1Ph. (24-0417/01)

[PRODUCT] Glass Plate. (24-0430)
500 mm square x 10 mm thick.

_Standards_
BS 1377, EN 1997-2

_Attributes_
Description
	Glass plate
	
BS/EN Standard
	Yes

_Related Products_
Main: Bulk Density Measure 10 Litre (34-2830)
Main: Liquid Limit Device BS with Counter. C/W Metal Grooving Tool & Test Gauge. (24-0410)
Main: Motorised Liquid Limit Device W/ Counter BS 220-240V 50Hz 1Ph. (24-0417/01)

[PRODUCT] Liquid Limit Device ASTM/ Aashto Hand-Operated W/ Revolution Counter. Supplied Less Grooving Tool. (24-0434)
Complete with revolution counter. Supplied less grooving tool.

_Standards_
ASTM D4318, AASHTO T89

_Attributes_
Description
	Liquid limit device
	
AASHTO Standard
	Yes
	
ASTM Standard
	Yes
	
Weight, kg
	3

_Related Products_
Accessory: ASTM Metal Grooving Tool. (24-0453)
Accessory: Casagrande Grooving Tool Aashto (24-0461)

[PRODUCT] ASTM Metal Grooving Tool. (24-0453)

_Standards_
ASTM D4318

_Attributes_
Description
	Grooving tool
	
ASTM Standard
	Yes
	
Weight, kg
	0.1

_Related Products_
Main: Liquid Limit Device ASTM/ Aashto Hand-Operated W/ Revolution Counter. Supplied Less Grooving Tool. (24-0434)

[PRODUCT] Casagrande Grooving Tool Aashto (24-0461)
* Rust resistant brass construction.* 1 cm gage block located at end of handle.The AASHTO Grooving Tool is used to control the width of the soil groove in the liquid limit cup, in accordance with AASHTO specifications.

_Standards_
ASTM D4318, AASHTO T89

_Further Information_
Brass construction with a gauge height of 1 cm.

_Attributes_
Description
	Grooving tool
	
AASHTO Standard
	Yes
	
Gauge height, cm
	1

_Specification_
Construction
	Brass.
	
Gauge Height
	1 cm.
	
Weight
	Net 3 oz. (85 g).

_Related Products_
Spare/Consumable: ASTM Plastic Grooving Tools (24-0451)
Main: Liquid Limit Device ASTM/ Aashto Hand-Operated W/ Revolution Counter. Supplied Less Grooving Tool. (24-0434)
Main: Motorized Liquid Limit Device (24-0441/02)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	BS/EN
	ASTM
	AASHTO
	N/A for this Product Group

[PRODUCT GROUP] Cone Penetrometer Method
*Reduces operator error*Applicable to a wide range of soils*Gives reproducible test results*Provides direct measurement of penetrationThe method is fundamentally more satisfactory than the Casagrande method as it is essentially a static test depending on the soil shear strength. The test is based on the relationship between moisture content and the penetration of a cone into the soil sample under controlled conditions.

[PRODUCT] Cone Penetrometer. Complete with Stainless Steel Test Cone. (24-0540)
Bench mounted apparatus to determine the liquid limit of soils BS1377. This method is applicable to a wide range of soils. The apparatus is fitted with a 150mm diameter dial indicator for direct reading of penetration. Supplied complete with 30deg, 30mm long test cone. Manufactured from stainless steel and includes adjustable levelling feet.

_Standards_
BS 1377, EN 1997-2

_Attributes_
Description
	Cone Penetrometer
	
Cone Relase
	Manual

_Specification_
Dial Indicator
	150 mm diameter graduated in 400 x 0.1 mm divisions, indicator point incorporates friction/gear system
	
Height Adjustment
	Rapid, using integral clampingmechanism
	
Cone release
	Manual
	
Cone
	1 x 30Âº, 35 mm test cone included
	
Base
	Cast aluminium, adjustable levelling feet
	
Weight kg
	6
	
Dial Indicator
	15 0 mm diameter graduated in 400 x 0.1 mm divisions. Indicator incorporates a friction/gear system.
	
Height
	Adjustable using rapid integral clamping mechanism.
	
Cone Release
	Manual.
	
Cone
	1 x 30Â°, 35 mm test cone included.
	
Base
	Cast aluminum with adjustable leveling feet.
	
Weight
	Net 17 lbs. (7.27 kg).

_Related Products_
Spare/Consumable: Penetration Test Cone (24-0544)
Accessory: Penetration Test Cup. (24-0548)
Main: Semi-Automatic Cone Penetrometer to BS:1377:Part 2 (24-0545/01)
Accessory: Test Gauge for Checking Condition of Cone Point. (24-0546)

[PRODUCT] Penetration Test Cone (24-0544)
Stainless steel, 35 mm long with smooth surface at an angle of 30º.

_Attributes_
Description
	Test cone
	
Cone
	1 x 30°, 35 mm cone

_Related Products_
Main: Cone Penetrometer. Complete with Stainless Steel Test Cone. (24-0540)
Main: Semi-Automatic Cone Penetrometer to BS:1377:Part 2 (24-0545/01)

[PRODUCT] Test Gauge for Checking Condition of Cone Point. (24-0546)
55 mm diameter by 40 mm deep, with the rim parallel to the flat base.

_Attributes_
Description
	Test gauge
	
Dimensions w x d x h, ”
	28x45x14 mm

_Related Products_
Main: Cone Penetrometer. Complete with Stainless Steel Test Cone. (24-0540)
Main: Semi-Automatic Cone Penetrometer to BS:1377:Part 2 (24-0545/01)

[PRODUCT] Penetration Test Cup. (24-0548)
Brass construction, 55mm dia x 4mm depth to fit BS1377

_Attributes_
Description
	Penetration test cup
	
Dimensions, diameter x length, ”
	55x40

_Related Products_
Main: Cone Penetrometer. Complete with Stainless Steel Test Cone. (24-0540)
Main: Semi-Automatic Cone Penetrometer to BS:1377:Part 2 (24-0545/01)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Semi-Automatic Cone Penetrometer

[PRODUCT] Semi-Automatic Cone Penetrometer to BS:1377:Part 2 (24-0545/01)
Bench mounted apparatus to determine the liquid limit of soils BS1377. This method is applicable to a wide range of soils. The apparatus is fitted with a 150mm diameter dial indicator for direct reading of penetration. Supplied complete with 30deg, 30mm long test cone. Manufactured from stainless steel and includes adjustable levelling feet.Incorporates Digital Automatic controller, which releases the plunger head and ensures free falling of the penetration device during the test. The time set is displayed by a bright easy to read display.

_Attributes_
Description
	Semi-Automatic Cone Penetrometer
	
Weight, kg
	8.6
	
Voltage Supply
	220-240 V 50/60 Hz
	
Cone Relase
	Semi-Automatic

_Specification_
Dial Indicator
	15 0 mm diameter graduated in 400 x 0.1 mm divisions. Indicator incorporates a friction/gear system.
	
Height
	Adjustable using rapid integral clamping mechanism.
	
Cone Release
	Semi-Automatic
	
Cone
	1 x 30°, 35 mm test cone included.
	
Base
	Cast aluminum with adjustable leveling feet.
	
Weight
	Net 19 lbs. (8.64 kg).

_Related Products_
Main: Cone Penetrometer. Complete with Stainless Steel Test Cone. (24-0540)
Spare/Consumable: Penetration Test Cone (24-0544)
Accessory: Penetration Test Cup. (24-0548)
Accessory: Test Gauge for Checking Condition of Cone Point. (24-0546)

[GROUPED PRODUCT MATRIX]
Model No.
	Voltage
	Weight, kg
	N/A for this Product Group

[CATEGORY] Determination of Shrinkage Characteristics
When the water content of a fine-grained soil is reduced below the plastic limit, shrinkage of the soil mass continues until the shrinkage limit is reached. Shrinkage can be significant in clays but less so in silts and sands. The equipment listed enables the engineer to determine a number of important parameters, including shrinkage ratio, volumetric shrinkage and linear shrinkage.

[PRODUCT GROUP] Volumetric Shrinkage
This method of test covers the determination of the shrinkage limit, shrinkage ratio, volumetric shrinkage and linear shrinkage.

[PRODUCT] Prong Plate. (24-1500)
Made of acrylic plastic fitted with three prongs, nominal 76 mm square and 2.4 mm thick.

_Standards_
BS 1377, ASTM D427, AASHTO T92

_Attributes_
Description
	Prong plate
	
Prong Plate Dimensions sq x thickness, ”
	3 x 1/8

_Specification_
Construction
	Acrylic plastic with 3 metal prongs.
	
Dimensions
	3” square x 1/8” thick (76 x 3.2 mm).
	
Weight
	Net 1 oz. (28 g).

_Related Products_
Accessory: Evaporating Dish - 150 x 45 mm (82-2000)
Main: Glass Cup. (24-1600)
Accessory: Measuring Cylinder - Glass 100 ml (82-0380)
Main: Shrinkage Dish. (24-1550)

[PRODUCT] Shrinkage Dish. (24-1550)
Nominal 42 mm diameter x 12 mm deep.

_Standards_
ASTM D427, AASHTO T92

_Attributes_
Description
	Shrinkage dish
	
Dimensions w x d x h, ”
	32x40x14 mm

_Related Products_
Accessory: Evaporating Dish - 150 x 45 mm (82-2000)
Main: Glass Cup. (24-1600)
Accessory: Measuring Cylinder - Glass 100 ml (82-0380)
Main: Prong Plate. (24-1500)

[PRODUCT] Glass Cup. (24-1600)
Nominal 70 mm diameter x 50 mm deep.

_Standards_
ASTM D427, AASHTO T92

_Attributes_
Description
	Glass cup
	
Weight, lbs
	0.388

_Related Products_
Accessory: Evaporating Dish - 100 x 40 mm (82-1970)
Accessory: Measuring Cylinder - Glass 100 ml (82-0380)
Main: Prong Plate. (24-1500)
Main: Shrinkage Dish. (24-1550)

[PRODUCT] Measuring Cylinder - Glass 100 ml (82-0380)
Soda glass, spouted, BS EN 4788.

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Measuring Cylinder - Glass
	
Capacity, ml
	100

_Related Products_
Main: Glass Cup. (24-1600)
Main: Prong Plate. (24-1500)
Main: Rotatest 1500 (45-3810/01)
Main: Rotatest 3000 (45-3815/01)
Main: Shrinkage Dish. (24-1550)

[PRODUCT] Evaporating Dish - 150 x 45 mm (82-2000)
Shallow form with spout, porcelain 150 x 45 mm nominal diameter x height.

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Diameter, mm
	150 x 45
	
Description
	Evaporating dish

_Related Products_
Main: Prong Plate. (24-1500)
Main: Shrinkage Dish. (24-1550)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Linear Shrinkage
This test covers the determination of linear shrinkage of soils and indicates the plastic properties of soils with a low clay content.

[PRODUCT] Shrinkage Mould to BS 1377 (24-1800)
To produce a specimen 140 mm long x 12.5 mm radius.

_Standards_
BS 1377

_Attributes_
Description
	Shrinkage mould
	
Weight, kg
	0.3

_Related Products_
Accessory: Vernier Caliper Range 0 to 200mm X 0.02mm. (81-0588)

[PRODUCT] Vernier Caliper Range 0 to 200mm X 0.02mm. (81-0588)
Vernier callipers 200 x 0.002mm. Graduated in mm and inches.

_Standards_
EN 933-4, BS 1377

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Vernier caliper
	
Measuring Range mm
	0 - 200 mm x 0.02 mm

_Related Products_
Main: Shrinkage Mould to BS 1377 (24-1800)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[CATEGORY] Determination of Density, Particle Density and Specific Gravity
Particle density or specific gravity is a measure of the actual particles which make up the soil mass and is defined as the ratio of the mass of the particles to the mass of the water they displace. A knowledge of the particle density is essential in relation to other soil tests. It is used when calculating porosity and voids ratio and is particularly important when compaction and consolidation properties are being investigated. The majority of apparatus used for the various tests is general laboratory equipment.

[PRODUCT GROUP] Gas Jar Method
This method is suitable for soils containing up to 10% of particles retained on a 37.5 mm BS sieve.

[PRODUCT] Gas Jar 75mm Dia X 300mm with Glass Cover and Rubber Bung. (24-2830)
1 litre capacity complete withrubber bung and glass cover.

_Standards_
BS 1377, EN 1997-2

_Attributes_
Description
	Gas jar
	
Capacity, litres
	1 litre

_Related Products_
Accessory: Mechanical End-Over-End Shaker Ce with Friction Safety Device and Control Panel 220-240V 50Hz 1Ph. (24-2854/01)

[PRODUCT] Mechanical End-Over-End Shaker Ce with Friction Safety Device and Control Panel 220-240V 50Hz 1Ph. (24-2854/01)
Fitted with friction safety device, capable of rotating two EL24-2830 Gas Jars at approximately 50 rpm to satisfy BS 1377.

_Standards_
BS 1377, EN 1997-2

_Attributes_
Description
	Mechanical end-over-end shaker
	
Power Supply
	220 - 240 V AC, 50 - 6- Hz, 1ph

_Related Products_
Main: Gas Jar 75mm Dia X 300mm with Glass Cover and Rubber Bung. (24-2830)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Particle Density: Pyknometer Methods
These methods are generally suitable for fine-grained soils. The larger pycnometers are not usually suitable for clay soils.

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	Capacity, ml
	
24-2885
	Pyknometer
	-
	
24-2890
	Density bottle
	25
	
24-2900
	Density bottle
	50
	
24-2950
	Density bottle
	100

[CATEGORY] Particle Size Distribution and Sand Equivalent Value
The analysis of soils by particle size provides a useful engineering classification system from which a considerable amount of empirical data can be obtained. Two separate and different procedures are used. Sieving is used for gravel and sand size particles and sedimentation procedures are used for the finer soils.For soil containing a range of coarse and fine particles it is usual to employ a composite test of sieving and sedimentation procedures. The Sand Equivalent Test serves as a rapid field test to show the relative proportions of clay-like or plastic fines and dusts in granular soils and fine aggregates.

[PRODUCT GROUP] Constant Temperature Bath

[PRODUCT] Constant Temperature Bath 0 to 99.9 Deg.C X 0.1 Deg.C with Led Display and False Base Support. (24-4865/01)
This compact, bench-top stirrer is used for dispersing soil samples in water for hydrometer analysis. The stirrer is supplied complete with Mixing Paddle and Dispersion Cup. Weight 4 kg.

_Further Information_
Specially designed for the sedimentation testing of soils and other fine grained material, the bath is supplied with a false bottom to assist in circulation of the bath liquid. Will accommodate six Sedimentation Cylinders.

_Attributes_
Voltage Supply
	220 - 240 V AC, 50/60 Hz, 1 ph

_Specification_
Dimensions (l x w x h)
	535 x 210 x 610 mm external
	
Capacity
	Holds up to 6 sedimentation cylinders
	
Construction
	Stainless steel with toughened glass front
	
Temperature Control
	Heater/thermostat/circulation with digital controller unit
	
Power
	1500 watts
	
Weight kg
	12

[GROUPED PRODUCT MATRIX]
Model No.
	Voltage
	N/A for this Product Group

[CATEGORY] Sedimentation by the Hydrometer Method
This method determines particle size distribution in a soil from the coarse sand size down to clay size (about 2 μm). The test does not require the weighing accuracy necessary for pipette sedimentation and is suitable for use in site laboratories.

[PRODUCT GROUP] Mechanical Analysis Stirrer

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	
24-4125/01
	High speed stirrer
	
24-4125/10
	Mixing paddle (spare)
	
24-4125/11
	Dispersion cup and baffle (spare)
	
24-4145
	Sodium Hexametaphosphate

[PRODUCT GROUP] Soil Hydrometers

[GROUPED PRODUCT MATRIX]
Model No.
	ASTM/AASHTO
	Graduation
	BS/EN DD ENV
	ASTM D422 (151H)
	
24-4620
	-
	0.0995 to 1.030 g/ml
	Yes
	-
	
24-4640
	Yes
	-5 to +60 g/litre
	-
	-
	
24-4650
	-
	0.0995 to 1.038 g/ml
	-
	Yes

[PRODUCT GROUP] Hydrometer Sedimentation Cylinder

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	
24-4700
	Hydrometer sedimentation cylinder
	
24-4800
	Nomographic chart

[CATEGORY] Sieving, wet and dry method
Particle size distribution is one of the most important physical characteristics of soil and classification of soils is based on the particle size distribution. Test methods are applicable to non-cemented soils with particles less than 125 mm and less than 10% fines.

[PRODUCT GROUP] 200mm Diameter BS Sieves

[GROUPED PRODUCT MATRIX]
Model No.
	Ap. Size
	Type
	
79-0010
	-
	Lid
	
79-0020
	-
	Receiver
	
79-0050
	45 μm
	Mesh
	
79-0060
	53 μm
	Mesh
	
79-0070
	63 μm
	Mesh
	
79-0080
	75 μm
	Mesh
	
79-0085
	80 μm
	Mesh
	
79-0090
	90 μm
	Mesh
	
79-0095
	100 μm
	Mesh
	
79-0100
	106 μm
	Mesh
	
79-0110
	125 μm
	Mesh
	
79-0120
	150 μm
	Mesh
	
79-0125
	160 μm
	Mesh
	
79-0140
	212 μm
	Mesh
	
79-0150
	250 μm
	Mesh
	
79-0160
	300 μm
	Mesh
	
79-0175
	400 μm
	Mesh
	
79-0180
	425 μm
	Mesh
	
79-0190
	500 μm
	Mesh
	
79-0200
	600 μm
	Mesh
	
79-0210
	710 μm
	Mesh
	
79-0220
	850 μm
	Mesh
	
79-0230
	1 mm
	Mesh
	
79-0240
	1.18 mm
	Mesh
	
79-0245
	1.25 mm
	Mesh
	
79-0250
	1.40 mm
	Mesh
	
79-0255
	1.60 mm
	Mesh
	
79-0260
	1.70 mm
	Mesh
	
79-0270
	2 mm
	Mesh
	
79-0280
	2.36 mm
	Mesh
	
79-0285
	2.50 mm
	Mesh
	
79-0290
	2.80 mm
	Mesh
	
79-0300
	3.35 mm
	Mesh
	
79-0310
	4 mm
	Mesh
	
79-0320
	4.75 mm
	Mesh
	
79-1500
	4 mm
	Perforated
	
79-1510
	4.75 mm
	Perforated
	
79-1515
	5 mm
	Perforated
	
79-1520
	5.60 mm
	Perforated
	
79-1525
	6.30 mm
	Perforated
	
79-1530
	6.70 mm
	Perforated
	
79-1540
	8 mm
	Perforated
	
79-1550
	9.50 mm
	Perforated
	
79-1555
	10 mm
	Perforated
	
79-1560
	11.20 mm
	Perforated
	
79-1565
	12.50 mm
	Perforated
	
79-1570
	13.20 mm
	Perforated
	
79-1575
	14 mm
	Perforated
	
79-1580
	16 mm
	Perforated
	
79-1590
	19 mm
	Perforated
	
79-1595
	20 mm
	Perforated
	
79-1600
	22.40 mm
	Perforated
	
79-1605
	25 mm
	Perforated
	
79-1610
	26.50 mm
	Perforated
	
79-1615
	28 mm
	Perforated
	
79-1630
	31.50 mm
	Perforated
	
79-1640
	37.50 mm
	Perforated
	
79-1655
	50 mm
	Perforated
	
79-1660
	53 mm
	Perforated
	
79-1670
	63 mm
	Perforated
	
79-1680
	75 mm
	Perforated

[PRODUCT GROUP] 300mm Diameter BS Sieves

[GROUPED PRODUCT MATRIX]
Model No.
	Ap. Size
	Type
	
79-2010
	-
	Lid
	
79-2020
	-
	Receiver
	
79-2070
	63 μm
	Mesh
	
79-2080
	75 μm
	Mesh
	
79-2085
	80 μm
	Mesh
	
79-2090
	90 μm
	Mesh
	
79-2095
	100 μm
	Mesh
	
79-2110
	125 μm
	Mesh
	
79-2120
	150 μm
	Mesh
	
79-2135
	200 μm
	Mesh
	
79-2140
	212 μm
	Mesh
	
79-2150
	250 μm
	Mesh
	
79-2160
	300 μm
	Mesh
	
79-2165
	315 μm
	Mesh
	
79-2180
	425 μm
	Mesh
	
79-2190
	500 μm
	Mesh
	
79-2200
	600 μm
	Mesh
	
79-2205
	630 μm
	Mesh
	
79-2220
	850 μm
	Mesh
	
79-2230
	1 mm
	Mesh
	
79-2240
	1.18 mm
	Mesh
	
79-2245
	1.25 mm
	Mesh
	
79-2255
	1.60 mm
	Mesh
	
79-2260
	1.70 mm
	Mesh
	
79-2270
	2 mm
	Mesh
	
79-2280
	2.36 mm
	Mesh
	
79-2285
	2.50 mm
	Mesh
	
79-2300
	3.35 mm
	Mesh
	
79-2320
	4.75 mm
	Mesh
	
79-2500
	4 mm
	Perforated
	
79-2510
	4.75 mm
	Perforated
	
79-2515
	5 mm
	Perforated
	
79-2525
	6.30 mm
	Perforated
	
79-2530
	6.70 mm
	Perforated
	
79-2540
	8 mm
	Perforated
	
79-2550
	9.50 mm
	Perforated
	
79-2555
	10 mm
	Perforated
	
79-2565
	12.50 mm
	Perforated
	
79-2570
	13.20 mm
	Perforated
	
79-2575
	14 mm
	Perforated
	
79-2580
	16 mm
	Perforated
	
79-2590
	19 mm
	Perforated
	
79-2595
	20 mm
	Perforated
	
79-2600
	22.40 mm
	Perforated
	
79-2605
	25 mm
	Perforated
	
79-2610
	26.50 mm
	Perforated
	
79-2615
	28 mm
	Perforated
	
79-2630
	31.50 mm
	Perforated
	
79-2640
	37.50 mm
	Perforated
	
79-2645
	40 mm
	Perforated
	
79-2655
	50 mm
	Perforated
	
79-2660
	53 mm
	Perforated
	
79-2670
	63 mm
	Perforated
	
79-2680
	75 mm
	Perforated
	
79-2684
	80 mm
	Perforated
	
79-2710
	125 mm
	Perforated

[PRODUCT GROUP] 8" Diameter ASTM Sieves

[GROUPED PRODUCT MATRIX]
Model No.
	Ap. Size
	Type
	
79-5400
	-
	Lid
	
79-5410
	-
	Receiver
	
79-5290
	45 µm
	Mesh
	
79-5270
	63 µm
	Mesh
	
79-5260
	75 µm
	Mesh
	
79-5250
	90 µm
	Mesh
	
79-5240
	106 µm
	Mesh
	
79-5230
	125 µm
	Mesh
	
79-5220
	150 µm
	Mesh
	
79-5210
	180 µm
	Mesh
	
79-5200
	121 µm
	Mesh
	
79-5190
	250 µm
	Mesh
	
79-5180
	300 µm
	Mesh
	
79-5160
	425 µm
	Mesh
	
79-5150
	500 µm
	Mesh
	
79-5140
	600 µm
	Mesh
	
79-5120
	850 µm
	Mesh
	
79-5110
	1 mm
	Mesh
	
79-5100
	1.18 mm
	Mesh
	
79-5090
	1.40 mm
	Mesh
	
79-5080
	1.70 mm
	Mesh
	
79-5070
	2 mm
	Mesh
	
79-5060
	2.36 mm
	Mesh
	
79-5050
	2.80 mm
	Mesh
	
79-5040
	3.35 mm
	Mesh
	
79-5000
	6.30 mm
	Mesh
	
79-5030
	4 mm
	Mesh
	
79-5020
	4.75 mm
	Mesh
	
79-5010
	5.60 mm
	Mesh
	
79-5490
	6.70 mm
	Mesh
	
79-5500
	8 mm
	Mesh
	
79-5510
	9.50 mm
	Mesh
	
79-5520
	11.20 mm
	Mesh
	
79-5530
	12.50 mm
	Mesh
	
79-5540
	13.20 mm
	Mesh
	
79-5550
	16 mm
	Mesh
	
79-5560
	19 mm
	Mesh
	
79-5570
	22.40 mm
	Mesh
	
79-5580
	25 mm
	Mesh
	
79-5610
	37.50 mm
	Mesh
	
79-5630
	50 mm
	Mesh
	
79-5650
	63 mm
	Mesh
	
79-5660
	75 mm
	Mesh

[PRODUCT GROUP] 12" Diameter ASTM Sieves

[GROUPED PRODUCT MATRIX]
Model No.
	Ap. Size
	Type
	
79-5800
	6.30 mm
	Mesh
	
79-5810
	5.60 mm
	Mesh
	
79-5820
	4.75 mm
	Mesh
	
79-5830
	4 mm
	Mesh
	
79-5840
	3.35 mm
	Mesh
	
79-5850
	2.80 mm
	Mesh
	
79-5860
	2.36 mm
	Mesh
	
79-5870
	2 mm
	Mesh
	
79-5880
	1.70 mm
	Mesh
	
79-5890
	1.40 mm
	Mesh
	
79-5900
	1.18 mm
	Mesh
	
79-5910
	1 mm
	Mesh
	
79-5920
	850 µm
	Mesh
	
79-5930
	710 µm
	Mesh
	
79-5940
	600 µm
	Mesh
	
79-5950
	500 µm
	Mesh
	
79-5960
	425 µm
	Mesh
	
79-5970
	355 µm
	Mesh
	
79-5980
	300 µm
	Mesh
	
79-5990
	250 µm
	Mesh
	
79-6000
	212 µm
	Mesh
	
79-6010
	180 µm
	Mesh
	
79-6020
	150 µm
	Mesh
	
79-6030
	125 µm
	Mesh
	
79-6040
	106 µm
	Mesh
	
79-6050
	90 µm
	Mesh
	
79-6060
	75 µm
	Mesh
	
79-6070
	63 µm
	Mesh
	
79-6080
	53 µm
	Mesh
	
79-6090
	45 µm
	Mesh
	
79-6100
	38 µm
	Mesh
	
79-6150
	-
	Lid
	
79-6160
	-
	Receiver
	
79-6190
	6.70 mm
	Mesh
	
79-6200
	8 mm
	Mesh
	
79-6210
	9.50 mm
	Mesh
	
79-6220
	11.20 mm
	Mesh
	
79-6230
	12.50 mm
	Mesh
	
79-6240
	13.20 mm
	Mesh
	
79-6250
	16 mm
	Mesh
	
79-6260
	19 mm
	Mesh
	
79-6270
	22.40 mm
	Mesh
	
79-6280
	25 mm
	Mesh
	
79-6290
	26.50 mm
	Mesh
	
79-6300
	31.50 mm
	Mesh
	
79-6310
	37.50 mm
	Mesh
	
79-6320
	45 mm
	Mesh
	
79-6330
	50 mm
	Mesh
	
79-6340
	53 mm
	Mesh
	
79-6350
	63 mm
	Mesh
	
79-6360
	75 mm
	Mesh
	
79-6370
	90 mm
	Mesh
	
79-6380
	100 mm
	Mesh
	
79-6400
	125 mm
	Mesh

[CATEGORY] Sand Equivalent Value
This test method assigns an empirical value to the relative amount, fineness, and character of claylike material present in the test specimen.

[PRODUCT GROUP] Sand Equivalent Value

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	
24-4919
	Sand equivalent apparatus ASTM D2419
	
24-4925
	Syphon assembly
	
24-4930
	Calcium chloride
	
24-4932
	Formaldehyde
	
24-4934
	Glycerol analar
	
24-4945/01
	Motorised sand equivalent shaker

[CATEGORY] Compaction & CBR

[CATEGORY] Compaction
Compaction tests typically enable the following criteria to be established:  	* The relationship between dry density and moisture content for a given degree of compactive effort. 	* The moisture content for the most efficient compaction; that is, at which the maximum dry density is achieved under that compactive effort. 	* The value of the maximum dry density achieved.There are several different standard laboratory compaction tests, with the most appropriate in each case being based on the nature of the project, the type of soil and the availability of equipment on site.APPLICATIONS OF COMPACTION Soil used as fill:  	* To refill an excavation or void 	* To provide made-up ground to support a structure 	* As a sub-base for a road, railway or airfield runway 	* As a structure; e.g. an earth damImprovement by compaction  	* Higher stability 	* Higher CBR Value 	* Lower compressibilty 	* Lower permeability 	* Lower frost susceptibilityEffect on mass of fill  	* Greater stability 	* Less settlement 	* Less deformation 	* Less water absorption 	* Less risk of frost heave

[PRODUCT GROUP] BS/EN compaction test 2.5kg
This test method utilises a 2.5 kg hand compaction hammer and a one litre capacity compaction mould. Often referred to as the 'Proctor' test it is suitable for soils containing particles no larger than 20 mm. The mould and hammer is manufactured from corrosion protected steel components to withstand the heavy usage involved in the test.

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	
24-9000
	Standard compaction mould
	
24-9002
	Standard compaction rammer

[PRODUCT GROUP] BS/EN compaction test 4.5kg
This test method utilises a 4.5 kg hand rammer resulting in a heavier compactive effort than the 2.5 kg test method. Compactive energy some 4.5 times greater is applied to the sample using the heavier rammer.The method is often specified where higher levels of compaction are necessary in a structure, e.g. an airfield sub-base material. Manufactured from corrosion protected steel components the 4.5 kg rammer is designed to withstand heavy usage involved in the test method.

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	
24-9004
	4.5 kg compaction rammer
	
24-9010
	300 mm straight edge

[PRODUCT GROUP] Proctor compaction

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	
24-9010
	300 mm straight edge
	
24-9060
	Proctor mould
	
24-9063
	Proctor compaction rammer

[PRODUCT GROUP] ASTM/Modified Proctor compaction

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	
24-9066
	ASTM/Modified Proctor compaction mould
	
24-9070
	ASTM/Modified Proctor rammer

[CATEGORY] Automatic Compaction of Soils
The time and effort required to prepare specimens for compaction studies and other test methods can often be costly and time-consuming. The use of an automatic, mechanical compactor will show considerable cost benefits over hand compaction methods. Two models meeting the requirements of BS/EN and ASTM are available.

[PRODUCT GROUP] Automatic Compactors
* Pre-set blow pattern ensures even compaction* Solid state controls for reliability and ease of maintenance* Automatic re-setting of counter after completion of blow patternThese machines automatically compact specimens eliminating the laborious hand compaction method. The height and weight of the rammer are adjustable to suit test requirements. An automatic blow pattern ensures optimum compaction for each layer of soil. The rammer travels across the mould and the table rotates the mould in equal steps on a base that is extremely stable. The number of blows per layer can be set at the beginning of the test.

[PRODUCT] Automatic Soil Compactor BS 220-240V 50Hz 1Ph. (24-9090/01)
Preset blow pattern ensures an even compaction, includes solid state controls for reliability and maintenance. An automatic digital counter resets to zero on the completion of a test. An adjustable rammer with a drop height of 300-450mm, an adjustable rammer weight of 2.5-4-5kg. A preset number of blows per layer can be set by thumb wheel control. A compaction rate of approximately 26 blows per minute. Accepts BS Standard Compaction and CBR moulds; also meets the requirements of BS1377. Voltage 220-240v ac 50/60hz 1ph.

_Standards_
BS 1377, EN 1997-2, EN 1924

_Attributes_
Voltage Supply
	220-240 V 50 Hz
	
BS/EN Standard
	Yes
	
Description
	Automatic Soil Compactor
	
Power Supply
	220 - 240 V AC 50 Hz 1 ph

_Specification_
Dimensions (l x w x h)
	430 x 240 x 1400 mm
	
Rammer BS/EN
	Circular faced, 50 mm dia, adjustableto 2.5 kg or 4.5 kg weight.
	
Rammer ASTM
	Circular faced, 2 in (50.8 mm) dia,adjustable to 5.5 lb (2.5 kg) or 10 lb(4.5 kg) weight.
	
Drop BS/EN
	Adjustable to 300 mm or 450 mm
	
Drop ASTM
	Adjustable to 12 in (305 mm) or 18in (457 mm)
	
Weight kg
	98

_Related Products_
Main: Automatic Soil Compactor BS 220-240V 60Hz 1Ph. (24-9090/06)
Accessory: BS Cbr Mould Body. (24-9198)
Accessory: BS Extension Collar (24-9200)
Accessory: BS Solid Base or  Top Plate (24-9204)
Accessory: BS Standard Compaction Mould 1000Cm Capacity. (24-9000)

[PRODUCT] Automatic Soil Compactor BS 220-240V 60Hz 1Ph. (24-9090/06)
Preset blow pattern ensures an even compaction, includes solid state controls for reliability and maintenance. An automatic digital counter resets to zero on the completion of a test. An adjustable rammer with a drop height of 300-450mm, an adjustable rammer weight of 2.5-4-5kg. A preset number of blows per layer can be set by thumb wheel control. A compaction rate of approximately 26 blows per minute. Accepts BS Standard Compaction and CBR moulds; also meets the requirements of BS1377. Voltage 220-240v ac 50/60hz 1ph.

_Attributes_
Voltage Supply
	220-240 V 60 Hz
	
BS/EN Standard
	Yes
	
Description
	Automatic Soil Compactor

_Specification_
Dimensions (l x w x h)
	430 x 240 x 1400 mm
	
Rammer BS/EN
	Circular faced, 50 mm dia, adjustableto 2.5 kg or 4.5 kg weight.
	
Rammer ASTM
	Circular faced, 2 in (50.8 mm) dia,adjustable to 5.5 lb (2.5 kg) or 10 lb(4.5 kg) weight.
	
Drop BS/EN
	Adjustable to 300 mm or 450 mm
	
Drop ASTM
	Adjustable to 12 in (305 mm) or 18in (457 mm)
	
Weight kg
	98

_Related Products_
Main: Automatic Soil Compactor BS 220-240V 50Hz 1Ph. (24-9090/01)
Accessory: BS Cbr Mould Body. (24-9198)
Accessory: BS Extension Collar (24-9200)
Accessory: BS Solid Base or  Top Plate (24-9204)
Accessory: BS Standard Compaction Mould 1000Cm Capacity. (24-9000)

[PRODUCT] Automatic Soils Compactor ASTM 220-240V 50Hz 1Ph. (24-9095/01)

_Standards_
ASTM D558, ASTM D559, ASTM D560, ASTM D698, ASTM D1557, AASHTO T99, AASHTO T134, AASHTO T135, AASHTO T136, AASHTO T180

_Attributes_
Description
	Automatic Soil Compactor
	
ASTM/AASHTO Standard
	Yes
	
Voltage Supply
	220-240 V 50 Hz
	
Hammer Weight, lbs
	5.5/10

_Specification_
Hammer
	Circular faced, 2.0” (50.8 mm) diam. foot; adjustable to either 5.5 lb.(2.5 kg) or 10 lb. (4.5 kg) weight.
	
Drop
	Adjustable to either 12 ” (305 mm) or 18” (45 7 mm)
	
Controls
	Digital counter system, selector switch for either standard proctor test or modified proctor/CBR testing.
	
Dimensions
	10” w. x 17” d. x 55 ” h. (25 0 x 43 0 x 1,400 mm).
	
Weight
	Net 41 9 lbs. (190 kg).

_Related Products_
Accessory: ASTM Compaction Mould 152mm. (24-9066)
Main: Automatic Soil Compactor ASTM 110-120 vAC (24-9095/02)
Main: Automatic Soils Compactor ASTM 220-240V 60Hz 1Ph. (24-9095/06)
Accessory: Calibration Kit (24-9095/12)
Spare/Consumable: Lead Cylinders (24-9095/13)
Spare/Consumable: Modified Compaction Mould (24-9098)
Accessory: Proctor Mould 1/30 Ft3. (24-9060)
Spare/Consumable: Standard Compaction Mould (24-9097)

[PRODUCT] Automatic Soil Compactor ASTM 110-120 vAC (24-9095/02)

_Standards_
ASTM D558, ASTM D559, ASTM D560, ASTM D698, ASTM D1557, AASHTO T99, AASHTO T134, AASHTO T135, AASHTO T136, AASHTO T180

_Further Information_
110-120vAC, 50/60 Hz, 1ø.

_Attributes_
Description
	Automatic Soil Compactor
	
ASTM/AASHTO Standard
	Yes
	
Voltage Supply
	110 - 120 V 60 Hz
	
Hammer Weight, lbs
	5.5/10

_Specification_
Hammer
	Circular faced, 2.0” (50.8 mm) diam. foot; adjustable to either 5.5 lb.(2.5 kg) or 10 lb. (4.5 kg) weight.
	
Drop
	Adjustable to either 12 ” (305 mm) or 18” (45 7 mm)
	
Controls
	Digital counter system, selector switch for either standard proctor test or modified proctor/CBR testing.
	
Dimensions
	10” w. x 17” d. x 55 ” h. (25 0 x 43 0 x 1,400 mm).
	
Weight
	Net 41 9 lbs. (190 kg).

_Related Products_
Accessory: ASTM Compaction Mould 152mm. (24-9066)
Main: Automatic Soils Compactor ASTM 220-240V 50Hz 1Ph. (24-9095/01)
Main: Automatic Soils Compactor ASTM 220-240V 60Hz 1Ph. (24-9095/06)
Accessory: Calibration Kit (24-9095/12)
Spare/Consumable: Lead Cylinders (24-9095/13)
Spare/Consumable: Modified Compaction Mould (24-9098)
Accessory: Proctor Mould 1/30 Ft3. (24-9060)
Spare/Consumable: Standard Compaction Mould (24-9097)

[PRODUCT] Automatic Soils Compactor ASTM 220-240V 60Hz 1Ph. (24-9095/06)

_Standards_
ASTM D558, ASTM D559, ASTM D560, ASTM D698, ASTM D1557, AASHTO T99, AASHTO T134, AASHTO T135, AASHTO T136, AASHTO T180

_Further Information_
For 110 - 120 V AC, 60 Hz, 1ph

_Attributes_
Description
	Automatic Soil Compactor
	
ASTM/AASHTO Standard
	Yes
	
Voltage Supply
	220-240 V 60 Hz

_Related Products_
Accessory: ASTM Compaction Mould 152mm. (24-9066)
Main: Automatic Soil Compactor ASTM 110-120 vAC (24-9095/02)
Main: Automatic Soils Compactor ASTM 220-240V 50Hz 1Ph. (24-9095/01)
Accessory: Proctor Mould 1/30 Ft3. (24-9060)

[GROUPED PRODUCT MATRIX]
Model No.
	Voltage
	Desc
	BS/EN
	ASTM/AASHTO
	N/A for this Product Group

[PRODUCT GROUP] Accessories for BS compaction and CBR

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	
24-9000
	Standard compaction mould
	
24-9198
	CBR mould body
	
24-9200
	CBR extension collar
	
24-9204
	BS CBR solid base

[PRODUCT GROUP] Accessories for ASTM and Proctor compaction

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	
24-9060
	Proctor mould
	
24-9066
	ASTM/Modified Proctor compaction mould

[CATEGORY] California Bearing Ratio
This test can be performed in the laboratory on prepared samples or on location. It is important to appreciate that this test, being of an empirical nature, is valid only for the application for which it was developed, i.e. the design of highway base thicknesses.A number of options are available to collect and analyse data with the ELE CBR-Test 50 or the MultiPlex 50 machines  	* Mechanical, using standard Load Rings and Penetration Dial Gauges. 	* Electronic, Load Transducers and Displacement Transducers in conjunction with the ELE Electronic Control and Readout Unit supplied with download software. 	* Electronic, using Electronic measuring devices as above in conjunction with the ELE DataSystem that provides full analysis of CBR Test data.

[PRODUCT GROUP] Load frames

[PRODUCT] Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/01)
* Single speed machine (BS/EN and ASTM)* Rapid platen adjustment* Complete with stabilising bar* Compact, bench-mounting design* Options for mechanical or electronic measurementDesigned for performing laboratory CBR tests to BS 1377, EN13286-47 and ASTM D1883, this bench mounting machine comprises a twin column frame incorporating a motorised drive system. Rapid adjustment of the platen is provided, which enables daylight to be taken up quickly and also close control of application of a seating load.

_Standards_
BS 1377, BS 1924, EN 13286-47, ASTM D1883, AASHTO T193

_Attributes_
Description
	CBR-Test 50 Machine
	
CBR Penetration
	Yes
	
Voltage Supply
	220-240 V 50 Hz
	
Power Supply
	220 V AC, 50 Hz, 1 ph

_Specification_
Dimensions (l x w x h)
	550 x 400 x 1220 mm
	
Max vertical clearance
	800 mm
	
Horizontal clearance
	255 mm
	
Platen diameter
	133 mm
	
Platen travel
	105 mm
	
Weight kg
	80

_Related Products_
Accessory: 50kN Load Measuring Ring (78-0860)
Accessory: 50kN S-type Load Cell (27-1559)
Accessory: ASTM Cbr Mould Complete with Collar & Perferated Base (24-9228)
Accessory: BS Cbr Mould Body. (24-9198)
Accessory: BS Extension Collar (24-9200)
Accessory: BS Solid Base or  Top Plate (24-9204)
Accessory: Cbr Penetration Piston (Adjustable). (24-9183)
Accessory: CBR Penetration Transducer 50mm Travel Fitted with 5 Pin Din Plug. (27-1705)
Main: CBR-Test 50 Machine 50 kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/02)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/06)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/01)
Accessory: Clamped Boss Load Ring - 10.0 kN (78-0460)
Accessory: Clamped Boss Load Ring - 2.0 kN (78-0060)
Accessory: Clamped Boss Load Ring - 28.0 kN (78-0760)
Main: MultiPlex 50 Load Frame (25-3700/01)
Accessory: Penetration Dial Gauge BS (24-9186)
Accessory: Penetration Piston (24-9182)
Accessory: Penetration/Swell Dial Gauge ASTM. (24-9184)

[PRODUCT] Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/06)
* Single speed machine (BS/EN and ASTM)* Rapid platen adjustment* Complete with stabilising bar* Compact, bench-mounting design* Options for mechanical or electronic measurementDesigned for performing laboratory CBR tests to BS 1377, EN13286-47 and ASTM D1883, this bench mounting machine comprises a twin column frame incorporating a motorised drive system. Rapid adjustment of the platen is provided, which enables daylight to be taken up quickly and also close control of application of a seating load.

_Attributes_
Description
	CBR-Test 50 Machine
	
CBR Penetration
	Yes
	
Voltage Supply
	220-240 V 60Hz

_Specification_
Dimensions (l x w x h)
	550 x 400 x 1220 mm
	
Max vertical clearance
	800 mm
	
Horizontal clearance
	255 mm
	
Platen diameter
	133 mm
	
Platen travel
	105 mm
	
Weight kg
	80

_Related Products_
Accessory: 50kN Load Measuring Ring (78-0860)
Accessory: 50kN S-type Load Cell (27-1559)
Accessory: ASTM Cbr Mould Complete with Collar & Perferated Base (24-9228)
Accessory: Bracket and Adaptor. Dual Purpose Mounting Bracket for CBR Penetration Gauges EL24-9184/EL24-9186 (24-9188)
Accessory: BS Cbr Mould Body. (24-9198)
Accessory: BS Extension Collar (24-9200)
Accessory: BS Solid Base or  Top Plate (24-9204)
Accessory: Cbr Penetration Piston (Adjustable). (24-9183)
Accessory: CBR Penetration Transducer 50mm Travel Fitted with 5 Pin Din Plug. (27-1705)
Main: CBR-Test 50 Machine 50 kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/02)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/01)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/06)
Accessory: Clamped Boss Load Ring - 10.0 kN (78-0460)
Accessory: Clamped Boss Load Ring - 2.0 kN (78-0060)
Accessory: Clamped Boss Load Ring - 28.0 kN (78-0760)
Main: MultiPlex 50 Load Frame (25-3700/01)
Accessory: Penetration Dial Gauge BS (24-9186)
Accessory: Penetration Piston (24-9182)
Accessory: Penetration/Swell Dial Gauge ASTM. (24-9184)

[PRODUCT] CBR-Test 50 Machine 50 kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/02)

_Standards_
AASHTO T99, AASHTO T134, AASHTO T135, AASHTO T136, AASHTO T180

_Further Information_
110-120vAC, 50/60 Hz, 1ø. Proving Ring, Penetration Piston assembly and penetration dial indicator not included, order separately

_Attributes_
CBR Penetration
	Yes
	
Voltage Supply
	110-120 V 60 Hz
	
Platen Travel, ”
	4.13
	
Description
	CBR-Test 50 Machine

_Specification_
Capacity
	11 ,200 lbf. (50 kN).
	
Horizontal Clearance
	10” (255 mm).
	
Vertical Clearance
	31 .5” (800 mm) maximum.
	
Platen
	5.24 ” (133 mm) diam.
	
Platen Travel
	4.13 ” (105 mm).
	
Dimensions
	15 .75” w. x 21 .65” d. x 48” h. (400 x 55 0 x 1,22 0 mm).
	
Weight
	Net 269 lbs. (122 kg).

_Related Products_
Accessory: 50kN Load Measuring Ring (78-0860)
Accessory: 50kN S-type Load Cell (27-1559)
Accessory: ASTM Cbr Mould Complete with Collar & Perferated Base (24-9228)
Accessory: BS Cbr Mould Body. (24-9198)
Accessory: BS Extension Collar (24-9200)
Accessory: BS Solid Base or  Top Plate (24-9204)
Main: CBR Loading Press, Hand-Operated (24-9345)
Accessory: Cbr Penetration Piston (Adjustable). (24-9183)
Accessory: CBR Penetration Piston Assembly (24-9179)
Accessory: CBR Penetration Transducer 50mm Travel Fitted with 5 Pin Din Plug. (27-1705)
Accessory: CBR Test Accessory Set English (24-9175)
Accessory: CBR Test Accessory Set For Use with GDU (24-9185)
Accessory: CBR Test Accessory Set Metric (24-9177)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/06)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/01)
Accessory: Clamped Boss Load Ring - 10.0 kN (78-0460)
Accessory: Clamped Boss Load Ring - 2.0 kN (78-0060)
Accessory: Clamped Boss Load Ring - 28.0 kN (78-0760)
Spare/Consumable: Dial Indicator - 1.0" Range (88-4100)
Accessory: Digital Proving Ring, 11,200 lbs (50.0 kN) (78-0864)
Accessory: Digital Proving Ring, 6,000 lbs (28.0 kN) (78-0764)
Main: Digital Tritest 50 Load Frame 110-120vAC (25-3518/02)
Accessory: Penetration Dial Gauge BS (24-9186)
Accessory: Penetration Piston (24-9182)
Accessory: Penetration/Swell Dial Gauge ASTM. (24-9184)
Main: Versa-Loader (25-3525/02)

[PRODUCT] MultiPlex 50 Load Frame (25-3700/01)
Compact bench mounting load frame designed for performing laboratory CBR, unconfined compression, quick undrained triaxial and Marshall Stability tests. Has a variable speed of 0.5 to 50mm per minute and features rapid approach of platen. 

_Standards_
EN 12697-34, BS 598, BS 1377, BS 1924, ASTM D1883, EN 12697-23, EN 12697-24, EN 13286-47, AASHTO T193, ASTM D2850, ASTM D4767, AASHTO T296, AASHTO T297

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	MultiPlex 50 Load Frame
	
CBR Penetration
	Yes
	
Unconfined Compression
	Yes
	
Voltage Supply
	220-240 V 50/60 Hz
	
Consolidated Undrained
	-
	
Consolidated Drained
	-
	
Power Supply
	220 - 240 V AC, 50 - 60 Hz, 1 ph
	
Marshall stability and flow
	Yes

_Specification_
Dimensions (l x w x h)
	550 x 400 x 1470 mm
	
Max vertical clearance
	800 mm
	
Horizontal clearance
	265 mm
	
Platen diameter
	133 mm
	
Platen travel
	100 mm
	
Platen speed range
	0.5 to 50 mm/min
	
Rapid approach speed
	40 mm/min
	
Weight kg
	100

_Related Products_
Accessory: 50kN Load Measuring Ring (78-0860)
Accessory: 50kN S-type Load Cell (27-1559)
Accessory: Bracket and Adaptor. Dual Purpose Mounting Bracket for CBR Penetration Gauges EL24-9184/EL24-9186 (24-9188)
Accessory: Cbr Penetration Piston (Adjustable). (24-9183)
Accessory: CBR Penetration Transducer 50mm Travel Fitted with 5 Pin Din Plug. (27-1705)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/06)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/01)
Accessory: Clamped Boss Load Ring - 10.0 kN (78-0460)
Accessory: Clamped Boss Load Ring - 2.0 kN (78-0060)
Accessory: Clamped Boss Load Ring - 28.0 kN (78-0760)
Accessory: Clamped Boss Load Ring - 3.0 kN (78-0160)
Accessory: Clamped Boss Load Ring - 4.5 kN (78-0260)
Main: Digital Tritest 50 (25-3518/01)
Accessory: Penetration Dial Gauge BS (24-9186)
Accessory: Penetration Piston (24-9182)
Accessory: Penetration/Swell Dial Gauge ASTM. (24-9184)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	CBR
	UC
	UU
	Voltage
	N/A for this Product Group

[PRODUCT GROUP] Penetration and measurement

[PRODUCT] Penetration Piston (24-9182)
1.935 mm2 (3 in2) area foot of case hardened steel. Designed to fit all ELE load rings.

_Attributes_
Description
	Penetration piston
	
Weight, kg
	3.7

_Related Products_
Main: CBR-Test 50 Machine 50 kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/02)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/06)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/01)
Main: MultiPlex 50 Load Frame (25-3700/01)

[PRODUCT] CBR Penetration Transducer 50mm Travel Fitted with 5 Pin Din Plug. (27-1705)
* Ideally suited for use with GDU for accurate displacement measurements* Models available for use in consolidation, shear, CBR and triaxial test applications* Supplied complete with mounting hardware for specified productsDisplacement Transducers are used in consolidation, shear, CBR and triaxial test applications for accuratevdisplacement measurements. They are supplied complete with a 5-pin DIN type connector for direct connection to the GDU.

_Attributes_
Description
	Penetration transducer
	
Mounting Bracket
	Included

_Specification_
Construction
	Fully encapsulated electronics,sealed in a stainless steel case
	
Excitation
	14 V DC
	
Connector
	5-pin DIN type
	
Mounting bracket
	Included as standard
	
Weight kg
	0.45

_Related Products_
Main: CBR-Test 50 Machine 50 kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/02)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/06)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/01)
Main: MultiPlex 50 Load Frame (25-3700/01)

[PRODUCT] Penetration/Swell Dial Gauge ASTM. (24-9184)
1 in travel x 0.0005 in divisions. Complete with rack extensions and chisel edge anvil.

_Attributes_
Description
	Penetration/swell gauge ASTM

_Related Products_
Main: CBR-Test 50 Machine 50 kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/02)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/06)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/01)
Main: Conversion Frame. (24-9341)
Main: MultiPlex 50 Load Frame (25-3700/01)

[PRODUCT] Bracket and Adaptor. Dual Purpose Mounting Bracket for CBR Penetration Gauges EL24-9184/EL24-9186 (24-9188)
Dual purpose mounting bracket for CBR penetration dial gauges. Allows gauge to be fixed to penetration piston or load ring.

_Attributes_
Description
	Bracket and adaptor

_Related Products_
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/06)
Main: Conversion Frame. (24-9341)
Main: MultiPlex 50 Load Frame (25-3700/01)

[PRODUCT] Penetration Dial Gauge BS (24-9186)
Complete with rack extensions and chisel edge anvil.25 mm travel x 0.01 mm divisions. 

_Attributes_
Description
	Penetration dial gauge - BS

_Related Products_
Main: CBR-Test 50 Machine 50 kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/02)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/06)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/01)
Main: Conversion Frame. (24-9341)
Main: MultiPlex 50 Load Frame (25-3700/01)

[PRODUCT] Cbr Penetration Piston (Adjustable). (24-9183)
As 24-9182 but with a coarse stem adjustment. This piston is particularly useful for in-situ testing.

_Attributes_
Description
	Penetration Piston - with adjustment

_Related Products_
Main: CBR-Test 50 Machine 50 kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/02)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/01)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/06)
Main: Conversion Frame. (24-9341)
Main: MultiPlex 50 Load Frame (25-3700/01)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Force measurement
A range of load rings will be required depending upon the type of material being tested. Detailed below is a selected range of load rings and transducers that are suitable for differing values of CBR.

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	CBR %
	
27-1559
	S-type load cell - 50 kN
	ALL
	
78-0060
	Load ring - 2 kN
	Up to 8%
	
78-0460
	Load ring - 10 kN
	8% to 40%
	
78-0760
	Load ring - 28 kN
	Average range of CBR
	
78-0860
	Load ring - 50 kN
	Above 40%

[PRODUCT GROUP] Automatic data acquisition

[PRODUCT] GDU 8 Channel Data Acquisition Unit 220-240 V 50/60 Hz, 1 Ph. (27-1500/01)
The GDU is a stand-alone, multi-tasking, multi-channel data logger, that is reliable and powerful, enabling it to co-ordinate test data from the range of ELE transducers required for various test methods.The ELE Geotechnical Software package (DS7.1), in conjunction with the GDU and a range of transducers, are the two central components required to create a modern turnkey soil testing system. Being fully modular it can be adapted to a wide range of soil testing laboratory configurations. * For performing CBR, Consolidation, Direct/Residual Shear and Total & Effective Stress Triaxial tests* 8 Channels expandable to 32 for performing multiple, concurrent tests for cost savings* Independent signal conditioning on each channel to maintain data accuracy* Field-upgradeable software, meaning no downtime for future software and functionality upgrades* Extended warranty.

_Attributes_
Description
	GDU 8 channel data acquisition unit
	
Transducer Supply
	10vDC.
	
Voltage Supply
	220-240 V 50/60 Hz

_Specification_
Case
	Aluminum, free standing; houses power supply, analog to digital conversion module and an 8-channel analog input module with transducer energization.
	
Sockets
	Standard 5-pin DIN type.
	
Input Range
	± 5 volts to ± 10 mV full scale.
	
Transducer Supply
	10vDC.
	
Dimensions
	12.8” w. x 14.3” d. x 6.1” h. (325 x 363 x 155 mm).
	
Weight
	Net 14.08 lbs. (6.4 kg).

_Related Products_
Accessory: 8-Channel Expansion Analog Input Module (27-1505)
Main: GDU 8 Channel Data Acquisition Unit 100-120 V 60 Hz (27-1500/02)
Accessory: USB to Serial Adapter (27-1701)

[PRODUCT] DS7.2 California Bearing Ratio (CBR) Penetration Program for Windows 7, 32/64 bit (27-1798)
This program provides the classical data for the CBR test. Load and penetration are monitored simultaneously. The program tabulates the results and provides a graphical presentation report.

_Attributes_
Description
	DS7.2 California Bearing Ratio (CBR) Penetration Program
	
GDU Compatability
	Yes
	
DSU Compatability
	Yes

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[CATEGORY] CBR Moulds and Accessories
A range of moulds and accessories designed to meet relevant Standards. The equipment is manufactured from high quality materials and with regular maintenance will give years of satisfactory performance.

[PRODUCT GROUP] ASTM/AASHTO CBR mould and accessories

[PRODUCT] ASTM Cbr Mould Complete with Collar & Perferated Base (24-9228)
With collar and perforated baseplate.

_Standards_
ASTM D1883, AASHTO T193

_Attributes_
Description
	CBR mould with collar and baseplate
	
Base Plate
	Perforated

_Specification_
Mould
	152.4 x 177.8 mm (inside diameter x height)
	
Collar
	50.8 mm height, fits both ends of mould
	
Base plate
	Perforated
	
Construction
	All steel, plated
	
Weight kg
	9

_Related Products_
Accessory: 4.5Kg Annular Surcharge Weight ASTM. (24-9243)
Accessory: 5 Lb. Annular Surcharge Weight ASTM. (24-9245)
Accessory: ASTM Cutting Collar. (24-9236)
Accessory: ASTM Spacing Disc. (24-9238)
Main: CBR-Test 50 Machine 50 kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/02)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/01)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/06)

[PRODUCT] ASTM Cutting Collar. (24-9236)
To fit ASTM CBR mould body, manufactured with a cutting edge to enable undisturbed samples to be taken in the field.

_Standards_
ASTM D1883, AASHTO T193

_Attributes_
Description
	CBR cutting collar
	
Mould Dimensions, i.d x h, ”
	6 x 1-1/2

_Specification_
Dimensions
	6â€ i.d. x 1-1/2â€ h. (152 .4 x 38 mm).
	
Construction
	Machined seamless steel tubing; recessed for mounting on CBR Mold.
	
Finish
	Plated.
	
Weight
	Net 1-1/2 lbs. (0.7 kg).

_Related Products_
Accessory: ASTM Cbr Mould Complete with Collar & Perferated Base (24-9228)

[PRODUCT] ASTM Spacing Disc. (24-9238)
150.8 mm diameter x 61.4 mm deep.

_Attributes_
Description
	CBR spacing disc
	
Finish
	Plated

_Specification_
Construction
	Steel; machined on all sides.
	
Finish
	Plated.
	
Weights
	Net 18.9 lbs. (8.6 kg).

_Related Products_
Accessory: ASTM Cbr Mould Complete with Collar & Perferated Base (24-9228)
Main: Spacer Disc 5-7/8" Diameter (24-9237)

[PRODUCT] Filter Screen 150mm Dia with 0.15mm Mesh. (24-9240)
150 mm dia, 150 μm mesh for use with ASTM mould.

_Attributes_
Description
	Filter screen
	
Mesh
	Brass; no. 100

_Specification_
Mesh
	Brass; number 100.
	
Size
	5-15 /16â€ diam. (135 mm).
	
Weight
	Net 1 oz. (28 g).

_Related Products_
Accessory: Filter Paper Equivalent to Whatman No 5 150mm Dia Box of 100. (24-9250)

[PRODUCT] 4.5Kg Annular Surcharge Weight ASTM. (24-9243)

_Attributes_
Description
	10 lb annular surcharge weight
	
Weight, kg
	4.5

_Related Products_
Accessory: ASTM Cbr Mould Complete with Collar & Perferated Base (24-9228)

[PRODUCT] 5Lb (2.27Kg) Split Surcharge Weight. (24-9244)

_Attributes_
Description
	5 lb split surcharge weight
	
Finish
	Plated

_Specification_
Construction
	Machined steel.
	
Finish
	Plated.

_Related Products_
Accessory: 5 Lb. Annular Surcharge Weight ASTM. (24-9245)
Main: 9.1Kg (20 Lb) Slotted Surcharge Weight (Cbr). (24-9248)
Main: Circular Surcharge Weight 10 lb (24-9247)
Main: Slotted Surcharge Weight 10 lb (24-9246)

[PRODUCT] 5 Lb. Annular Surcharge Weight ASTM. (24-9245)

_Attributes_
Description
	5 lb annular surcharge weight
	
Finish
	Plated

_Specification_
Construction
	Machined steel.
	
Finish
	Plated.

_Related Products_
Accessory: 5Lb (2.27Kg) Split Surcharge Weight. (24-9244)
Main: 9.1Kg (20 Lb) Slotted Surcharge Weight (Cbr). (24-9248)
Accessory: ASTM Cbr Mould Complete with Collar & Perferated Base (24-9228)
Main: Circular Surcharge Weight 10 lb (24-9247)
Main: Slotted Surcharge Weight 10 lb (24-9246)

[PRODUCT] Filter Paper Equivalent to Whatman No 5 150mm Dia Box of 100. (24-9250)
Box of 100.

_Standards_
ASTM D1883, AASHTO T193

_Attributes_
Description
	Filter papers - 150 mm diameter
	
Size (height x width x diameter) cm
	5.9

_Specification_
Grade
	Coarse.
	
Size
	15 cm diam. (5.9â€).
	
Weight
	Net 8 oz. (22 7 g).

_Related Products_
Accessory: Filter Screen 150mm Dia with 0.15mm Mesh. (24-9240)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] BS EN CBR mould and acccessories

[PRODUCT] BS Cbr Mould Body. (24-9198)

_Standards_
BS 1377, BS 1924, EN 13286-4, EN 1997-2

_Attributes_
Description
	CBR mould body
	
Base Plate
	Solid

_Specification_
Mould
	152 x 127 mm (inside diameter x height)
	
Collar
	51 mm height, fits both ends of mould
	
Base plate
	Solid, fits both ends od mould
	
Construction
	All steel, plated
	
Weight kg
	7.3

_Related Products_
Main: Automatic Soil Compactor BS 220-240V 50Hz 1Ph. (24-9090/01)
Main: Automatic Soil Compactor BS 220-240V 60Hz 1Ph. (24-9090/06)
Main: CBR-Test 50 Machine 50 kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/02)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/01)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/06)

[PRODUCT] BS Extension Collar (24-9200)

_Standards_
BS 1377, BS 1924, EN 13286-4, EN 1997-2

_Attributes_
Description
	CBR extension collar
	
Base Plate
	Solid

_Related Products_
Main: Automatic Soil Compactor BS 220-240V 50Hz 1Ph. (24-9090/01)
Main: Automatic Soil Compactor BS 220-240V 60Hz 1Ph. (24-9090/06)
Main: CBR-Test 50 Machine 50 kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/02)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/01)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/06)

[PRODUCT] BS Solid Base or  Top Plate (24-9204)

_Standards_
BS 1377, BS 1924, EN 13286-4, EN 1997-2

_Attributes_
Description
	BS CBR solid base
	
Base Plate
	Solid

_Related Products_
Accessory: 2Kg Annular Surcharge Weight (24-9214)
Main: Automatic Soil Compactor BS 220-240V 50Hz 1Ph. (24-9090/01)
Main: Automatic Soil Compactor BS 220-240V 60Hz 1Ph. (24-9090/06)
Accessory: Base Plate Tool for BS Mould (24-9210)
Accessory: BS Perforated Base Plate. (24-9202)
Accessory: Cbr Cutting Collar with Area Ratio of 21.9% to Fit BS Moulds. (24-9206)
Main: CBR-Test 50 Machine 50 kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/02)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/01)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/06)
Accessory: Filter Papers 150mm Dia Equivalent to Whatman No 1. Box of 100. (24-9220)

[PRODUCT] BS Perforated Base Plate. (24-9202)
To fit mould body

_Standards_
BS 1377, BS 1924, EN 13286-4, EN 1997-2

_Attributes_
Description
	Perforated base plate
	
Weight, kg
	1.8

_Related Products_
Accessory: BS Solid Base or  Top Plate (24-9204)

[PRODUCT] Cbr Cutting Collar with Area Ratio of 21.9% to Fit BS Moulds. (24-9206)
To fit BS/EN mould body.

_Standards_
BS 1377, BS 1924, EN 13286-4, EN 1997-2

_Attributes_
Description
	CBR cutting collar
	
Weight, kg
	1.4

_Related Products_
Accessory: BS Solid Base or  Top Plate (24-9204)

[PRODUCT] C-Spanner for BS Cbr Mould. Two Required. (24-9208)
To fit BS/EN CBR moulds and collars. Two required.

_Standards_
BS 1377, BS 1924, EN 13286-4, EN 1997-2

_Attributes_
Description
	C-spanner for CBR mould
	
Weight, kg
	1.7

[PRODUCT] Base Plate Tool for BS Mould (24-9210)
To fit into base plate to assist removal from mould body.

_Standards_
BS 1377, BS 1924, EN 13286-4, EN 1997-2

_Attributes_
Description
	Base plate tool
	
Weight, kg
	0.7

_Related Products_
Accessory: BS Solid Base or  Top Plate (24-9204)

[PRODUCT] Static Compaction Plug. (24-9212)
Steel, 150 mm dia x 51 mm thick. Complete with removable handle.

_Standards_
BS 1377, BS 1924, EN 13286-4, EN 1997-2

_Attributes_
Description
	Static compaction plug
	
Weight, kg
	7.3

[PRODUCT] 2Kg Annular Surcharge Weight (24-9214)

_Standards_
BS 1377, BS 1924, EN 13286-4, EN 1997-2

_Attributes_
Description
	2 kg annular surcharge weight
	
Weight, kg
	2

_Related Products_
Accessory: BS Solid Base or  Top Plate (24-9204)

[PRODUCT] 2Kg Split Surcharge Weight. (24-9216)

_Standards_
BS 1377, BS 1924, EN 13286-4, EN 1997-2

_Attributes_
Description
	2 kg split surcharge weight
	
Weight, kg
	2

[PRODUCT] Filter Papers 150mm Dia Equivalent to Whatman No 1. Box of 100. (24-9220)
Box of 100.

_Standards_
BS 1377, BS 1924, EN 13286-4, EN 1997-2

_Attributes_
Description
	Filter paper - 150 mm diameter

_Related Products_
Accessory: BS Solid Base or  Top Plate (24-9204)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Expansion (swell) Test Equipment

[PRODUCT] Swell Plate (24-9260)
With adjustable stem.

_Standards_
ASTM D1883, AASHTO T193

_Attributes_
Description
	Swell plate
	
Contact Head
	Adjustable; locks on stem with knurled nut.

_Specification_
Base Plate
	5-7/8” diam. (14 9.2 mm); perforated.
	
Contact Head
	Adjustable; locks on stem with knurled nut.
	
Construction
	All brass.
	
Weight
	Net 2-1/2 lbs. (1.1 kg).

[PRODUCT] Penetration/Swell Dial Gauge ASTM. (24-9184)
1 in travel x 0.0005 in divisions. Complete with rack extensions and chisel edge anvil.

_Attributes_
Description
	Penetration/swell gauge ASTM

_Related Products_
Main: CBR-Test 50 Machine 50 kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/02)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/06)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/01)
Main: Conversion Frame. (24-9341)
Main: MultiPlex 50 Load Frame (25-3700/01)

[PRODUCT] Swell Tripod (24-9262)
For mounting Swell Dial Gauge in position on CBR mould collar.

_Standards_
ASTM D1883, AASHTO T193

_Further Information_
Requires dial indicator; not included, order separately

_Attributes_
Description
	Swell tripod
	
Clamp
	Integral part of assembly; holds dial indicator.

_Specification_
Construction
	Machined, one-piece cast aluminum.
	
Contact Head
	Integral part of ssembly; holds dial indicator.
	
Construction
	2” l. (50.8 mm) included.
	
Weight
	Net 1 lb. (0.4 kg).

_Related Products_
Spare/Consumable: Dial Indicator - 1.0" Range (88-4100)
Main: Electronic Digital Indicator, 1.0"/25.4 mm range (88-4220)
Accessory: Mechanical Dial Indicator - 25 mm Range Clockwise Movement (88-4110)

[PRODUCT] Large Curing Tank C/W with Circulating Pump Heater/Thermostat Unit and Lower Rack (34-6575/01)
This curing tank is supplied complete with a submersible pump, immersion heater/thermostat unit and separate control panel. The tank includes a lower rack as standard and is designed to maintain the temperature at 20 ± 2ºC, providing that the ambient temperature does not fall below 15ºC or rise above 20ºC.

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA** Supplied as specified. For 220 - 240 V AC, 50 - 60 Hz, 1 ph.

_Attributes_
Description
	Curing/soaking tank

_Specification_
Internal Dimensions
	1040 x 1040 x 605 mm (l x w x h)
	
Capacity
	650 litres
	
Rated Power
	2000 watt
	
Weight
	60 kg

_Related Products_
Main: Jolting Table 220 - 240 V AC 60 Hz (39-1150/06)
Accessory: Maximum and Minimum Thermometer (82-5310)

[PRODUCT] Dial Gauge 25mm Travel X 0.01mm Divisions. (24-9275)
25 mm travel x 0.01 mm.

_Attributes_
Description
	Penetration/swell gauge BS

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[CATEGORY] In-situ CBR
The use of in-situ CBR apparatus on road construction contracts enables the bearing capacity of soils to be determined quickly and efficiently with minimum delay. The BS 1377, BS 1924 and ASTM D4429 standards describe in-situ test procedures.

[PRODUCT GROUP] In-situ CBR

[PRODUCT] Penetration/Swell Dial Gauge ASTM. (24-9184)
1 in travel x 0.0005 in divisions. Complete with rack extensions and chisel edge anvil.

_Attributes_
Description
	Penetration/swell gauge ASTM

_Related Products_
Main: CBR-Test 50 Machine 50 kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/02)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/06)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/01)
Main: Conversion Frame. (24-9341)
Main: MultiPlex 50 Load Frame (25-3700/01)

[PRODUCT] Bracket and Adaptor. Dual Purpose Mounting Bracket for CBR Penetration Gauges EL24-9184/EL24-9186 (24-9188)
Dual purpose mounting bracket for CBR penetration dial gauges. Allows gauge to be fixed to penetration piston or load ring.

_Attributes_
Description
	Bracket and adaptor

_Related Products_
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/06)
Main: Conversion Frame. (24-9341)
Main: MultiPlex 50 Load Frame (25-3700/01)

[PRODUCT] Penetration Dial Gauge BS (24-9186)
Complete with rack extensions and chisel edge anvil.25 mm travel x 0.01 mm divisions. 

_Attributes_
Description
	Penetration dial gauge - BS

_Related Products_
Main: CBR-Test 50 Machine 50 kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/02)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/06)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/01)
Main: Conversion Frame. (24-9341)
Main: MultiPlex 50 Load Frame (25-3700/01)

[PRODUCT] Cbr Penetration Piston (Adjustable). (24-9183)
As 24-9182 but with a coarse stem adjustment. This piston is particularly useful for in-situ testing.

_Attributes_
Description
	Penetration Piston - with adjustment

_Related Products_
Main: CBR-Test 50 Machine 50 kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/02)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/01)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/06)
Main: Conversion Frame. (24-9341)
Main: MultiPlex 50 Load Frame (25-3700/01)

[PRODUCT] 45kN (10000Lb) Capacity Mechanical Jack. (24-9290)
The body is corrosion protected and houses an enclosed worm and wheel gear. The gear ratio has been carefully selected to provide a handwheel speed that can be comfortably maintained, particularly with soils of high CBR value. A quick-release device in the screwjack allows the plunger to be rapidly adjusted prior to the test.

_Attributes_
Description
	45 kN (10000 lb) capacity mechanical jack

_Related Products_
Main: Conversion Frame. (24-9341)

[PRODUCT] Land Rover Bracket to Attach EL29-200 Jack. for Land Rovers Models 90 & 110 From 1983 Onwards. (24-9298)
Fits all models in Land Rover series 90 and 110.

_Attributes_
Description
	Land Rover bracket

[PRODUCT] Ball Seating for EL 24-9290 45 kN Jack (24-9300)
For fitting between the mechanical jack and reaction point. The ball seating is used when testing on undulating ground to ensure that the jack, load measuring ring and penetration piston are truly vertical. Non-axial loading of the load ring will give false results and will eventually damage the ring itself.

_Attributes_
Description
	Ball seating attachment

[PRODUCT] Set of Extension Rods Complete (24-9308)
Made from highquality steel with large-section thread for quick assembly.

_Attributes_
Description
	Set of extension rods

[PRODUCT] Datum Bar Assembly. (24-9312)
Comprising 2 tripod stands and a datum bar.

_Attributes_
Description
	Datum bar assembly

[PRODUCT] 10Lb (4.5Kg) Annular Surcharge Weight. (24-9320)

_Attributes_
Description
	10 lb (4.5Kg) annular surcharge weight
	
Weight, kg
	4.5

[PRODUCT] 10Lb (4.5Kg) Slotted Surcharge Weight. (24-9322)

_Attributes_
Description
	10 lb (4.5Kg) slotted surcharge weight
	
Weight, kg
	4.5

[PRODUCT] 9.1Kg (20 Lb) Slotted Surcharge Weight (Cbr). (24-9248)

_Attributes_
Description
	Slotted Surcharge Weight 20 lb
	
Finish
	Plated

_Specification_
Construction
	Machined steel.
	
Finish
	Plated.

_Related Products_
Accessory: 5 Lb. Annular Surcharge Weight ASTM. (24-9245)
Accessory: 5Lb (2.27Kg) Split Surcharge Weight. (24-9244)
Main: Circular Surcharge Weight 10 lb (24-9247)
Main: Slotted Surcharge Weight 10 lb (24-9246)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Conversion of In-situ to Laboratory CBR
The in-situ CBR jack assembly can be mounted in a simple conversion frame to measure CBR values in the laboratory. The frame is used with the jack, a suitable load ring, CBR mould and penetration piston.

[PRODUCT] Conversion Frame. (24-9341)

_Attributes_
Description
	50 kN conversion frame
	
Weight, kg
	53

_Related Products_
Accessory: 45kN (10000Lb) Capacity Mechanical Jack. (24-9290)
Accessory: Bracket and Adaptor. Dual Purpose Mounting Bracket for CBR Penetration Gauges EL24-9184/EL24-9186 (24-9188)
Accessory: Cbr Penetration Piston (Adjustable). (24-9183)
Accessory: Clamped Boss Load Ring - 28.0 kN (78-0760)
Accessory: Penetration Dial Gauge BS (24-9186)
Accessory: Penetration/Swell Dial Gauge ASTM. (24-9184)

[PRODUCT] 45kN (10000Lb) Capacity Mechanical Jack. (24-9290)
The body is corrosion protected and houses an enclosed worm and wheel gear. The gear ratio has been carefully selected to provide a handwheel speed that can be comfortably maintained, particularly with soils of high CBR value. A quick-release device in the screwjack allows the plunger to be rapidly adjusted prior to the test.

_Attributes_
Description
	45 kN (10000 lb) capacity mechanical jack

_Related Products_
Main: Conversion Frame. (24-9341)

[PRODUCT] Penetration/Swell Dial Gauge ASTM. (24-9184)
1 in travel x 0.0005 in divisions. Complete with rack extensions and chisel edge anvil.

_Attributes_
Description
	Penetration/swell gauge ASTM

_Related Products_
Main: CBR-Test 50 Machine 50 kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/02)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/06)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/01)
Main: Conversion Frame. (24-9341)
Main: MultiPlex 50 Load Frame (25-3700/01)

[PRODUCT] Bracket and Adaptor. Dual Purpose Mounting Bracket for CBR Penetration Gauges EL24-9184/EL24-9186 (24-9188)
Dual purpose mounting bracket for CBR penetration dial gauges. Allows gauge to be fixed to penetration piston or load ring.

_Attributes_
Description
	Bracket and adaptor

_Related Products_
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/06)
Main: Conversion Frame. (24-9341)
Main: MultiPlex 50 Load Frame (25-3700/01)

[PRODUCT] Penetration Dial Gauge BS (24-9186)
Complete with rack extensions and chisel edge anvil.25 mm travel x 0.01 mm divisions. 

_Attributes_
Description
	Penetration dial gauge - BS

_Related Products_
Main: CBR-Test 50 Machine 50 kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/02)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/06)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/01)
Main: Conversion Frame. (24-9341)
Main: MultiPlex 50 Load Frame (25-3700/01)

[PRODUCT] Cbr Penetration Piston (Adjustable). (24-9183)
As 24-9182 but with a coarse stem adjustment. This piston is particularly useful for in-situ testing.

_Attributes_
Description
	Penetration Piston - with adjustment

_Related Products_
Main: CBR-Test 50 Machine 50 kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/02)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/01)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/06)
Main: Conversion Frame. (24-9341)
Main: MultiPlex 50 Load Frame (25-3700/01)

[PRODUCT] Clamped Boss Load Ring - 28.0 kN (78-0760)

_Attributes_
Description
	Load ring - 28 kN
	
Load device type
	Load ring
	
Force Capacity, kN
	28
	
Value of CBR %
	Average range of CBR
	
Overall Height, mm
	248

_Specification_
Capacity: kN, kgf, lbf
	28.0, 2800, 6000
	
Typical Design sensitivity: N/div, kgf/div, lbf/div
	25.5, 2.54, 5.45
	
Overall height mm
	248
	
Approx weight kg
	5.4
	
Capacity
	28 kN
	
Value of CBR
	Average range of CBR
	
Capacity - lbf
	6,000
	
Capacity - kN
	28
	
Capacity - kgf
	2,800
	
Typical Design Sensitivity - lbf/div
	5.45
	
Typical Design Sensitivity - kN/div
	25.5
	
Typical Design Sensitivity - Kgf/div
	2.54
	
Overall Height
	9.76” (248 mm)
	
Approx Weight
	11 .9 lbs.(5.4 kg)

_Related Products_
Accessory: 50kN Load Measuring Ring (78-0860)
Main: CBR Loading Press, Hand-Operated (24-9345)
Main: CBR-Test 50 Machine 50 kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/02)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/01)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/06)
Accessory: Clamped Boss Load Ring - 10.0 kN (78-0460)
Accessory: Clamped Boss Load Ring - 2.0 kN (78-0060)
Accessory: Clamped Boss Load Ring - 3.0 kN (78-0160)
Accessory: Clamped Boss Load Ring - 4.5 kN (78-0260)
Main: Conversion Frame. (24-9341)
Accessory: Digital Proving Ring, 6,000 lbs (28.0 kN) (78-0764)
Main: Digital Tritest 50 (25-3518/01)
Main: Digital Tritest 50 Load Frame 110-120vAC (25-3518/02)
Main: MultiPlex 50 Load Frame (25-3700/01)
Spare/Consumable: Spare Dial Indicator for Load Rings (78-5461)
Main: Versa-Loader (25-3525/02)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[CATEGORY] Consolidation
It is generally understood that clays and other compressible soils can be subject to long-term consolidation under the loads imposed by foundations and above ground structures. Also that settlement may occur even if the applied pressure is wihtin the safe bearing capacity of the soil.

[CATEGORY] One-Dimensional Consolidation
The One-dimensional Consolidation test is used to determine the consolidation characteristics of soils of low permeability. Tests are carried out on specimens prepared from undisturbed samples. Data obtained from these tests, together with classification data and a knowledge of the soils loading history, enables estimates to be made of the behaviour of foundations under load.

[PRODUCT GROUP] Consolidation Apparatus

[PRODUCT] Consolidation Frame One Dimensional Consolidation Incremental Loading Device. (25-0402)
* High capacity - 8800 kPa on 50 mm diameter specimens using 11:1 beam ratio* Triple beam ratio, 9:1, 10:1, 11:1* Compact unit ensures maximum space savingThe ELE Oedometer is rigidly constructed to ensure minimum frame distortion. The frame is designed to load the specimen through a yoke assembly and one of three alternative beam ratios. The beam is fitted with a counterbalance weight and beam support jack. The cell platform will accept the complete range of ELE consolidation cells and is fitted with a central spigot to ensure accurate centring of the cell under the loading yoke. Dimensions without hanger 711 x 203 x 508 mm (l x w x h). Weight 22 kg.

_Standards_
BS 1377, EN 1997-2, ASTM D2435, ASTM D4546, AASHTO T216

_Further Information_
Supplied without dial gauge and weights.

_Attributes_
Description
	Consolidation frame
	
Loading Beam
	Cast aluminum; counterbalanced; 9:1,10:1 and 11:1 ratios.

_Specification_
Load Capacity
	48 tons/sq. ft. (5,14 8 kPa) on 2.5” (63 mm) diam. samples.
	
Loading Beam
	Cast aluminum; counterbalanced; 9:1,10:1 and 11 :1 ratios.
	
Frame
	Cast aluminum; integral beam support jack; plated steel and platform.
	
Dimensions
	8” w. x 28” d. x 20” h. (203 x 711 x 508 mm),excluding weight hanger.
	
Weight
	Net 30 lbs. (13 .6 kg); Shpg. 40 lbs. (18.1 kg).

_Related Products_
Accessory: 16 Ton Weight Set (25-0544)
Accessory: 2.416" Fixed Ring Consolidometer (25-0480)
Accessory: 2.5" Floating Ring Consolidometer (25-0530)
Accessory: Consolidation Cell Complete 2.5 Inch Diameter Sample. Inc. Porous Discs and Cutting Ring. (25-0479)
Accessory: Consolidation Cell Complete 50mm Diameter Sample. (25-0455)
Accessory: Consolidation Cell Complete 75mm Diameter Sample (25-0503)
Accessory: Electronic Digital Indicator, 0.600"/15 mm range (88-4210)
Accessory: Floor Mounting Stand. (25-0429)
Accessory: Mechanical Dial Indicator - 0.4" Range (88-4070)
Accessory: Mechanical Dial Indicator - 1.0" Range Counter Clockwise Movement (88-4120)
Accessory: Mechanical Dial Indicator - 10 mm Range (88-4080)
Accessory: Mechanical Dial Indicator - 25 mm Range Counter Clockwise Movement (88-4130)
Main: Pneumatic Consolidation Apparatus (25-0560)
Accessory: Set of Weights 100Kg Total Weight. (25-0408)
Accessory: Weight Set A (25-0535)
Accessory: Weight Set B (25-0537)

[PRODUCT] Set of Weights 100Kg Total Weight. (25-0408)
9 x 10 kg, 1 x 5 kg, 2 x 2 kg, 1 x 1 kg.

_Standards_
ASTM D2435, ASTM D4546, AASHTO T216

_Attributes_
Description
	Set of weights
	
Weight, kg
	100

_Related Products_
Main: Consolidation Frame One Dimensional Consolidation Incremental Loading Device. (25-0402)

[PRODUCT] Floor Mounting Stand. (25-0429)
A versatile modular steel stand. Holes in the shelf are provided forsecuring up to three EL25-0402 Consolidation Frames. Dimensions 610 x 915 x 865 mm (l x w x h).

_Standards_
ASTM D2435, ASTM D4546, AASHTO T216

_Attributes_
Description
	Floor mounting stand
	
Table Dimensions, ”
	980mmx950mm

_Related Products_
Main: Consolidation Frame One Dimensional Consolidation Incremental Loading Device. (25-0402)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] BS EN consolidation cells and accessories

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	Sample dia.
	
25-0503
	Consolidation cell 75 mm
	75 mm
	
25-0503/13
	Upper and lower porous stones
	75 mm
	
25-0506
	Cutting ring
	75 mm
	
25-0509
	Calibration disc
	75 mm

[PRODUCT GROUP] ASTM/AASHTO consolidation cells and accessories

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	Sample dia.
	
25-0479
	Consolidation cell 2.5"
	2.5"
	
25-0479/13
	Upper and lower porous stones
	2.5"
	
25-0482
	Cutting Ring
	2.5"
	
25-0485
	Calibration disc
	2.5"

[PRODUCT GROUP] High pressure application consolidation cells and accessories

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	Sample dia.
	
25-0455
	Consolidation cell 50 mm
	50 mm
	
25-0455/13
	Upper and lower porous stones
	50 mm
	
25-0458
	Cutting ring
	50 mm
	
25-0461
	Calibration disc
	50 mm

[PRODUCT GROUP] Vertical settlement measurement
Various methods of measuring vertical settlement can be supplied. These range from dial gauges to displacement transducers. All devices comply with the accuracy specified in BS 1377, ASTM D2435 and D4546. Displacement transducers are supplied with a calibration certificate. The table below shows the range of devices available for fitting to the EL25-0402 Consolidation Frame. Transducers are supplied complete with mounting brackets as required.

[PRODUCT] Dial Gauge 10mm Travel X 0.002mm Divisions. (25-0440)
10 mm x 0.002 mm div.

_Attributes_
Description
	Vertical Dial Indicator, Metric
	
Dial Indicator
	10 mm range x 0.002 mm<br>graduations.

_Related Products_
Main: Digital Direct/Residual Shear Apparatus Complete with Lever Loading Assembly. 110-120V 50/60Hz 1Ph. (26-2114/02)
Main: Digital Direct/Residual Shear Apparatus Complete with Lever Loading Assembly. 220-240V 50/60Hz 1Ph. (26-2114/01)
Accessory: Electronic Digital Indicator, 0.600"/15 mm range (88-4210)
Accessory: Vertical Dial Indicator, English (25-0445)

[PRODUCT] Consolidation Transducer Assembly 15mm Travel Fitted with 5 Pin Din Plug. (27-1649)
Fitted with 5 pin DIN plug.

_Attributes_
Description
	Displacement tranducer
	
Mounting Bracket
	Included as standard.

_Specification_
Construction
	Fully encapsulated electronics,sealed in a stainless steel case
	
Excitation
	11 V DC
	
Connector
	5-pin DIN type
	
Mounting bracket
	Included as standard
	
Weight kg
	0.45
	
Construction
	Fully encapsulated electronics, sealed in a stainless steel case.
	
Excitation
	10vDC.
	
Connector
	5-Pin DIN type.
	
Mounting Bracket
	Included as standard.
	
Weight
	Net 1 lb. (0.45 kg).

_Related Products_
Accessory: Axial Strain Transducer Assembly 50mm Travel Fitted with 5 Pin Din Plug. (27-1617)
Main: CBR Displacement Transducer (27-1706)
Accessory: Horizontal Displacement Transducer Assembly 15mm Travel 5 Pin Din Plug Mounting Pillar (27-1697)
Main: Transducer Extension Cable 3.0 m (27-1717)
Main: Transducer Extension Cable 4.5 m (27-1719)
Accessory: Vertical Displacement Transducer Assembly 15mm Travel with 5 Pin Din Plug Bracket for Shear Box (27-1689)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Automatic data acquisition
Geotechnical laboratories make extensive use of computers and automated testing, and we offer specially written software packages designed to record and analyse test data. Presentation of results is in test report format, giving geotechnical engineers total control over all areas of analysis where an engineering judgement is required.

[PRODUCT] GDU 8 Channel Data Acquisition Unit 220-240 V 50/60 Hz, 1 Ph. (27-1500/01)
The GDU is a stand-alone, multi-tasking, multi-channel data logger, that is reliable and powerful, enabling it to co-ordinate test data from the range of ELE transducers required for various test methods.The ELE Geotechnical Software package (DS7.1), in conjunction with the GDU and a range of transducers, are the two central components required to create a modern turnkey soil testing system. Being fully modular it can be adapted to a wide range of soil testing laboratory configurations. * For performing CBR, Consolidation, Direct/Residual Shear and Total & Effective Stress Triaxial tests* 8 Channels expandable to 32 for performing multiple, concurrent tests for cost savings* Independent signal conditioning on each channel to maintain data accuracy* Field-upgradeable software, meaning no downtime for future software and functionality upgrades* Extended warranty.

_Attributes_
Description
	GDU 8 channel data acquisition unit
	
Transducer Supply
	10vDC.
	
Voltage Supply
	220-240 V 50/60 Hz

_Specification_
Case
	Aluminum, free standing; houses power supply, analog to digital conversion module and an 8-channel analog input module with transducer energization.
	
Sockets
	Standard 5-pin DIN type.
	
Input Range
	± 5 volts to ± 10 mV full scale.
	
Transducer Supply
	10vDC.
	
Dimensions
	12.8” w. x 14.3” d. x 6.1” h. (325 x 363 x 155 mm).
	
Weight
	Net 14.08 lbs. (6.4 kg).

_Related Products_
Accessory: 8-Channel Expansion Analog Input Module (27-1505)
Main: GDU 8 Channel Data Acquisition Unit 100-120 V 60 Hz (27-1500/02)
Accessory: USB to Serial Adapter (27-1701)

[PRODUCT] DS7.1 One-Dimensional Consolidation Software (27-1770)

_Standards_
ASTM D2435, ASTM D4546, AASHTO T216, BS 1377, EN 1997-2

_Attributes_
Weight, lbs
	1.1
	
Description
	DS7.1 One-Dimensional Consolidation Software

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[CATEGORY] Permeability
Knowledge of the permeability characteristics of soil is essential for construction projects where drainage is an important element. In particular, permeability is a key parameter for the design and assessment of landfill sites, the investigation of contaminated ground, the design of earth dams and sheet pile walls, and in assessing the potential for lowering groundwater levels.

[PRODUCT GROUP] Combination Permeameter
This combination permeameter has a transparent plastic chamber for soil specimens of either fine-grained or coarse-grained soils. Generally, soils containing 10 percent or more particles passing a 75 μm sieve are tested using the falling head assembly. More granular soils, containing 90 percent or more particles retained on the 75 μm sieve, are tested using the constant head assembly. Includes accessories for conducting both constant and falling head permeability studies.

[PRODUCT] Combination Permeameter (25-0623)
*Plated steel chamber head assembly*Corrosion-resistant cast aluminum base assembly*Includes accessories for conducting both constant and falling head permeability studiesThis combination permeameter has a transparent plastic chamber for soil specimens of either fine-grained or coarse-grained soils. Generally, soils containing 10 percent or more particles passing a 75 μm sieve are tested using the falling head assembly. More granular soils, containing 90 percent or more particles retained on the 75 μm sieve, are tested using the constant headassembly.The cell is sealed at the top so that a vacuum may be used to saturate the specimen. Porous stones located at the top and bottom of the cell prevent sample flaking or washout. For constant head tests, a plastic funnel reservoir is mounted on an upright attached to the cell, providing a maximum head of 550 mm. Falling head tests are performed using the grGDUated pipette falling head reservoir, which gives a maximum head of 1000 mm and is graduated 0.2 ml.

_Attributes_
Description
	Combination permeameter
	
Falling Head
	Graduated pipette; 100 cc x 0.2 cc; 100 cm. maximum<br>head.

_Specification_
Specimen size
	63.5 x 63.5 mm (dia x l max) when using lower chamber only, 63.5 x 140 mm (dia x l max) when using both lower and extension chambers
	
Chamber
	Transparent plastic, two sections
	
Base
	Cast aluminium
	
Top seal
	Plated steel with gaskets
	
Porous Stones
	62.7 x 12.7 mm (diameter x thickness)
	
Constant head
	Plastic, funnel reservoir, 550 mmmaximum head
	
Falling head
	Graduated pipette, 100 ml x 0.2 ml, 1000 mm maximum head
	
Weight kg
	5
	
Specimen Size
	2-1/2” diam. x 2-1/2” l. max. (63.5 x 63.5 mm) when using lower chamber only; 2-1/2” diam. x 5-1/2” l. max. (63.5 x 14 0 mm) when using both lower and extension chambers.
	
Capacity
	Clear lucite; 1/4” (6.3 mm) wall; two sections.
	
Base
	Cast aluminum.
	
Top Seal
	Plated steel with gaskets.
	
Porous Stones
	Mounts at top and bottom; 2.47” diam. x 1/2” thick (62.7 x 12 .7 mm); 105-120 permeability rating; 300 micron, average pore size.
	
Constant Head
	Plastic; funnel reservoir; 55 cm maximum head.
	
Falling Head
	Graduated pipette; 100 cc x 0.2 cc; 100 cm. maximumhead.
	
Weight
	Net 11 lbs. (5 kg).

_Related Products_
Spare/Consumable: Porous Stone 2.47" x .50" (T-308)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Compaction Permeameter
These Permeameters are designed for performing either constant head or falling head permeability tests on undisturbed, remoulded or compacted soils.

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	
25-0607
	Compaction permeameter
	
25-0609
	Standpipe panel
	
25-0611
	De-airing tank
	
25-0613
	Soaking tank

[PRODUCT GROUP] Constant Head Apparatus
This equipment is used for testing the permeability of granular soils (sands and gravels).The specimen is formed in a permeability cell and water is passed through it from a constant level tank. Take-off points located along the sides of the permeability cell are connected to three manometer tubes mounted on a panel complete with a metre scale. Water passing through the specimen is collected and measured, either for a specific quantity or over a period of time. The reduction of head is noted from the variation of water level in the manometer tubes.

[PRODUCT] Constant Head Permeability Cell 75mm Diameter Specimen. (25-0580)
75 mm Diameter

_Standards_
BS 1377, EN 1997-2, ASTM D2434, AASHTO T215

_Attributes_
Description
	Constant head permeability cell
	
End Plates
	Aluminium

_Specification_
Nominal Cell inside diameer
	75 mm
	
Cell wall
	Transparent plastic
	
Take-off points
	3
	
End plates
	Anodised aluminium
	
Weight kg
	2.6

[PRODUCT] Manometer Tubes & Stand. (25-0591)
Comprising three glass tubes of constant bore, metre scale and connecting tubing for cell pressure take-off points, all mounted on a free-standing panel.Comprising three glass tubes of constant bore, metre scale and connecting tubing for cell pressure take-off points, all mounted on a free-standing panel.

_Standards_
BS 1377, EN 1997-2, ASTM D2434, AASHTO T215

_Attributes_
Description
	Manometer tubes & stand
	
Weight, kg
	2.8

[PRODUCT] Constant Level Tank. (25-0593)
Manufactured from transparent plastic with attachment for wall mounting. The inlet, outlet and overflow pipes are fitted to the baseof the tank and can be adjusted for height within the tank. Supplied complete with connecting tubing.

_Standards_
BS 1377, EN 1997-2, ASTM D2434, AASHTO T215

_Attributes_
Description
	Constant level tank
	
Weight, kg
	2.4

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Falling Head Apparatus
Clays and silts are tested using the falling head technique. Flow of water through the specimen is observed by monitoring the rate of fall of water in the tube. It is essential that soils of very low permeability are sealed inside the cylinder to prevent seepage along the sides of the specimen. Before testing, the specimen must be completely saturated with water as the presence of air will restrict the flow of water.

[PRODUCT] Falling Head Permeability Cell. (25-0605)

_Attributes_
Description
	Falling head permeability cell
	
Top Plate, ”
	Machined

_Specification_
Cell
	Plated seamless tube 100 mm diameterx 130 mm height
	
Base
	Porous plate with three tie rods
	
Top plate
	Machined to accept smaller tubes
	
Weight kg
	3.4

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Guelph Permeameter
The Guelph Permeameter is used to obtain accurate measurements of hydraulic conductivity, soil sorptivity and soil matrix flux potential. These three factors govern how liquids will move through an unsaturated soil profile.

[PRODUCT] Guelph Permeameter Supplied Complete with Extension Kit. (25-0650)
* Lightweight and portable* Robust construction* Requires only 2.5 litres of water* Results usually within 2 hoursThe Guelph Permeameter is used to obtain accurate measurements of hydraulic conductivity, soil sorptivity and soil matrix flux potential. These three factors govern how liquids will move through an unsaturated soil profile.Recent significant advances in both the theoretical and practical techniques of measuring soil hydraulic conductivity have been made by the University of Guelph, Canada. This has resulted in the development of the Guelph Permeameter, utilising the Constant Head Well principle.

_Standards_
ASTM D5126

_Further Information_
Guelph Permeameter Set Includes:-*1 Field Tripod*1 Well Auger*1 Well Tripod*1 Preparation Tool*1 Hand Pump*1 Extension Kit (extends depth by 800 mm)*1 Collapsible Water Container*1 Set of Instructions and Carrying Case

_Attributes_
Description
	Guelph Permeameter
	
Hydraulic Conductivity Range, m/sec
	10-4 - 10-8

_Specification_
Cell
	Plated seamless tube 100 mm diameter x 130 mm height
	
Base
	Porous plate with three tie rods
	
Top plate
	Machined to accept smaller tubes
	
Weight kg
	3.4
	
Permeameter
	High impact polycarbonate, moldedelastomers.
	
Auger
	2” (50.8 mm) diam.; machined steel.
	
Carrying Case
	Die-cut foam for parts storage.
	
Test Time
	1/2 – 2 hours.
	
Test Depth
	15 to 75 cm (0.5 to 2.5 ft).
	
Hydraulic Conductivity Range
	10-4 to 10-8 m/sec (10-2 to 10-6 cm/sec).
	
Weight
	Net 30 lbs. (13 .6 kg).

_Related Products_
Accessory: Permeameter Extension Kit (25-0655)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[CATEGORY] Soil Strength (Triaxial)
An extension of the QU test is the unconsolidated undrained test (UU); this is similar to the QU test but is run at a slower rate in order to measure pore water pressure. By comparison, effective stresses when measured in a triaxial cell are more complex in their nature, as numerous parameters can be measured. These include back pressure, pore water pressure and volume change; all of which can be used to calculate the required engineering properties. Effective stress tests are usually referred to as consolidated drained (CD) or consolidated undrained (CU). Generally the CD test is applicable to sands, while both the CU or CD test can be used with clays. There are many special test variations within these basic test groupings. Our range of triaxial cells and accessories, used in conjunction with other equipment such as load frames, pressure sources and measurement devices, have been specifically designed to meet the wide ranging requirements of modern soil mechanics laboratories. Each system is easy to set up and use, providing accurate and repeatable measurements.

[PRODUCT GROUP] Load Frames
The range of ELE designed and manufactured load frames is the most modern of its kind available to the discerning test laboratory. The range comprises capacities of 50 kN incorporating the latest microprocessor control systems, clear on-board screen displays and a range of other high quality features.

[PRODUCT] Digital Tritest 50 (25-3518/01)
* Microprocessor control* Large on-board LED screen display* Direct entry via a touch sensitive keyboard* Rapid approach and return to datum of platen* Fully variable speed, 0.00001 to 9.99999 mm/min* Samples up to 100 mm diameterThis 50 kN capacity machine, designed primarily for triaxial testing of soil specimens up to 100 mm diameter x 200 mm long, comprises a rigid twin column construction with an integral fully variable microprocessor controlled drive unit and LCD display with a touch sensitive keyboard. The machine is normally bench mounted for ease of installation and operation.The use of a microprocessor controlled drive system and keyboard entry provides the Digital Tritest 50 with a wide variety of features which include pause and speed reset during test, RS 232C, operator programming of speed and control functions, self test diagnostics and many other features.A robustly constructed steel case houses the motor drive system with careful attention being given to the prevention of ingress of water or grit. All operating controls are mounted on the front panel of the machine, which is angled and recessed to prevent physical and environmental damage.

_Standards_
BS 1377-7, BS 1377-8, BS 1924-2, ASTM D1883, ASTM D2166, ASTM D2850, ASTM D4767, ASTM D7181, AASHTO T99, AASHTO T134, AASHTO T135, AASHTO T136, AASHTO T180, AASHTO T193, AASHTO T208, AASHTO T296, AASHTO T297

_Further Information_
Complete with RS 232C interface.

_Attributes_
Description
	Digital Tritest 50 Load Frame 220-240 V AC
	
CBR Penetration
	Yes
	
Unconfined Compression
	Yes
	
Consolidated Undrained
	Yes
	
Consolidated Drained
	Yes
	
Capacity, lbf
	11,200

_Specification_
Dimensions (l x w x h)
	500 x 500 x 1470 mm
	
Max vertical clearance
	910 mm
	
Horizontal clearance
	364 mm
	
Platen diameter
	133 mm
	
Platen travel
	100 mm
	
Platen speed range
	0.00001 to 9.99999 mm/min
	
Rapid approach speed
	25 mm/minute
	
Weight kg
	140
	
Capacity
	12 ,200 lbf. (50 kN).
	
Speed Range
	English mode: 0.000001 to 0.399999 in/min.Metric mode: 0.00001 to 9.99999 mm/min.
	
Rapid Approach Speed
	2.0 in/min. (50 mm/min.).
	
Platen Travel
	3.9” (100 mm); limit switch protection.
	
Vertical Clearance
	36 .8” (910 mm) maximum; 12 ” (305 mm) minimum.
	
Horizontal Clearance
	15 .3” (364 mm).
	
Serial Interface
	RS232 C; programmable baud rate and protocol.
	
Overall Dimensions
	19.7” w. x 19.7” d. x 57.8” h. (500 x 500 x 1,470 mm).
	
Weight
	Net 220 lbs. (100 kg); Shpg. 300 lbs. (136 kg).

_Related Products_
Accessory: 50kN Load Measuring Ring (78-0860)
Accessory: Clamped Boss Load Ring - 10.0 kN (78-0460)
Accessory: Clamped Boss Load Ring - 28.0 kN (78-0760)
Accessory: Clamped Boss Load Ring - 3.0 kN (78-0160)
Accessory: Clamped Boss Load Ring - 4.5 kN (78-0260)
Main: MultiPlex 50 Load Frame (25-3700/01)
Main: Versa-Loader (25-3525/02)

[PRODUCT] MultiPlex 50 Load Frame (25-3700/01)
Compact bench mounting load frame designed for performing laboratory CBR, unconfined compression, quick undrained triaxial and Marshall Stability tests. Has a variable speed of 0.5 to 50mm per minute and features rapid approach of platen. 

_Standards_
EN 12697-34, BS 598, BS 1377, BS 1924, ASTM D1883, EN 12697-23, EN 12697-24, EN 13286-47, AASHTO T193, ASTM D2850, ASTM D4767, AASHTO T296, AASHTO T297

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	MultiPlex 50 Load Frame
	
CBR Penetration
	Yes
	
Unconfined Compression
	Yes
	
Voltage Supply
	220-240 V 50/60 Hz
	
Consolidated Undrained
	-
	
Consolidated Drained
	-
	
Power Supply
	220 - 240 V AC, 50 - 60 Hz, 1 ph
	
Marshall stability and flow
	Yes

_Specification_
Dimensions (l x w x h)
	550 x 400 x 1470 mm
	
Max vertical clearance
	800 mm
	
Horizontal clearance
	265 mm
	
Platen diameter
	133 mm
	
Platen travel
	100 mm
	
Platen speed range
	0.5 to 50 mm/min
	
Rapid approach speed
	40 mm/min
	
Weight kg
	100

_Related Products_
Accessory: 50kN Load Measuring Ring (78-0860)
Accessory: 50kN S-type Load Cell (27-1559)
Accessory: Bracket and Adaptor. Dual Purpose Mounting Bracket for CBR Penetration Gauges EL24-9184/EL24-9186 (24-9188)
Accessory: Cbr Penetration Piston (Adjustable). (24-9183)
Accessory: CBR Penetration Transducer 50mm Travel Fitted with 5 Pin Din Plug. (27-1705)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/06)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/01)
Accessory: Clamped Boss Load Ring - 10.0 kN (78-0460)
Accessory: Clamped Boss Load Ring - 2.0 kN (78-0060)
Accessory: Clamped Boss Load Ring - 28.0 kN (78-0760)
Accessory: Clamped Boss Load Ring - 3.0 kN (78-0160)
Accessory: Clamped Boss Load Ring - 4.5 kN (78-0260)
Main: Digital Tritest 50 (25-3518/01)
Accessory: Penetration Dial Gauge BS (24-9186)
Accessory: Penetration Piston (24-9182)
Accessory: Penetration/Swell Dial Gauge ASTM. (24-9184)

[GROUPED PRODUCT MATRIX]
Model No.
	CBR
	UC
	UU
	CU
	CD
	N/A for this Product Group

[PRODUCT GROUP] De-Aired Water
It is particularly important that water from which dissolved air has been removed is used in the pore pressure measurement system and saturation procedures. Any dissolved air in the water will lead to errors in the measurement of pore pressure, particularly at low pressures, and also give slow or incorrect saturation results.

[PRODUCT] De-Aired Water Apparatus 15 Litre Capacity (25-1833/01)
This compact self-contained unit will de-air water quickly and efficiently down to levels of dissolved oxygen acceptable for geotechnical test methods. Air is removed from the water by a vacuum system, which continuously circulates the water in the tank. The unit is supplied with a clear water container, which will hold a maximum of 15 litres of water. Input and output lines are formed using standard 6 mm tube connectors.  

_Attributes_
Self-Contained
	Yes
	
Capacity, litres
	15 L

[GROUPED PRODUCT MATRIX]
Model No.
	Self-Contained
	Capacity, litres
	N/A for this Product Group

[PRODUCT GROUP] Triaxial Cells
* Working pressure up to 1700 kPa* All round visibility* Sample sizes 38 to 100 mm diameter* Rapid assembly and dismantling* Accepts a range of interchangeable submersible load transducers

[GROUPED PRODUCT MATRIX]
Model No.
	38 mm
	50 mm
	70 mm
	100 mm
	Horizontal Clearance
	
25-4047
	Yes
	Yes
	-
	-
	155
	
25-4117
	-
	Yes
	Yes
	-
	180
	
25-4157
	-
	-
	-
	Yes
	255

[PRODUCT GROUP] Automatic Data Acquisition

[PRODUCT] GDU 8 Channel Data Acquisition Unit 220-240 V 50/60 Hz, 1 Ph. (27-1500/01)
The GDU is a stand-alone, multi-tasking, multi-channel data logger, that is reliable and powerful, enabling it to co-ordinate test data from the range of ELE transducers required for various test methods.The ELE Geotechnical Software package (DS7.1), in conjunction with the GDU and a range of transducers, are the two central components required to create a modern turnkey soil testing system. Being fully modular it can be adapted to a wide range of soil testing laboratory configurations. * For performing CBR, Consolidation, Direct/Residual Shear and Total & Effective Stress Triaxial tests* 8 Channels expandable to 32 for performing multiple, concurrent tests for cost savings* Independent signal conditioning on each channel to maintain data accuracy* Field-upgradeable software, meaning no downtime for future software and functionality upgrades* Extended warranty.

_Attributes_
Description
	GDU 8 channel data acquisition unit
	
Transducer Supply
	10vDC.
	
Voltage Supply
	220-240 V 50/60 Hz

_Specification_
Case
	Aluminum, free standing; houses power supply, analog to digital conversion module and an 8-channel analog input module with transducer energization.
	
Sockets
	Standard 5-pin DIN type.
	
Input Range
	± 5 volts to ± 10 mV full scale.
	
Transducer Supply
	10vDC.
	
Dimensions
	12.8” w. x 14.3” d. x 6.1” h. (325 x 363 x 155 mm).
	
Weight
	Net 14.08 lbs. (6.4 kg).

_Related Products_
Accessory: 8-Channel Expansion Analog Input Module (27-1505)
Main: GDU 8 Channel Data Acquisition Unit 100-120 V 60 Hz (27-1500/02)
Accessory: USB to Serial Adapter (27-1701)

[PRODUCT] DS7.2 Undrained Triaxial Shear Strength Program for Windows 7, 32/64 bit (27-1753)
* Options for single or multi-stage testing on a sample* Mohr circles produced for graphical analysisOptions are available for a single test on one sample, standard three-sample procedure with linking of the results, or for a multi-stage test on one sample. Load and strain are monitored through transducers. Various printouts and graphical plots are available including basic sample data, moisture content and density. The program tabulates shearing data and plots stress against strain. Mohr circles are produced for graphical analyses.

_Attributes_
Description
	DS7.2 Undrained Triaxial Shear Strength
	
GDU Compatability
	Yes
	
DSU Compatability
	Yes

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[CATEGORY] Accessories for Triaxial Cells

[PRODUCT GROUP] Aggressive Materials
Although all products are treated to inhibit corrosion, certain aggressive materials may attack the metal components. Examples of this are samples obtained from the seabed or containing high concentrations of sulphates or chlorides.Where aggressive materials are to be tested, ELE will be pleased to offer advice on any special requirements.

[PRODUCT] Piston Restraint Clamp for Ele Triaxial Cells (25-4200)
For Ele Triaxial Cells Manufactured From July 1996.

_Standards_
BS 1377, ASTM D2850, ASTM D4767, AASHTO T296, AASHTO T297

_Further Information_
To lock the loading piston into position

_Attributes_
Description
	Piston Restraint Clamp
	
Weight, lbs
	1.075

_Related Products_
Main: 70mm Triaxial Cell 1700Kpa with 5 Pressure/ Drainage Ports. Supplied with Two Valves. (25-4117)

[PRODUCT] Silicon Grease Lubricant. (25-8090)
Silicon Grease Lucrican (Tube).

_Standards_
BS 1377, ASTM D2850, ASTM D4767, AASHTO T296, AASHTO T297

_Attributes_
Description
	Silicon Grease Lubricant

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Specimen Base Adaptors
Each cell will require the correct size of specimen base adaptor relative to the size (diameter) of sample tested. 

[GROUPED PRODUCT MATRIX]
Model No.
	100 mm Cell
	70 mm cell
	50 mm cell
	Specimen
	
25-4166
	-
	-
	Yes
	38 mm
	
25-4168
	-
	-
	Yes
	50 mm
	
25-4174
	-
	Yes
	-
	50 mm
	
25-4176
	-
	Yes
	-
	70 mm
	
25-4186
	Yes
	-
	-
	100 mm

[CATEGORY] Measurement instrumentation
Various methods of measuring axial displacement, load, pressure and volume change can be supplied. All devices comply with the accuracy specified in BS 1377; ASTM D2850, D4767. All transducers transducers are supplied with a calibration certificate.

[PRODUCT GROUP] Volume Change Measurement

[PRODUCT] Twin Burette Volume Change Unit. (26-1892)
Fitted with reversing valve and by-pass valve. The unit is fitted with burettes graduated 0 to 100 ml x 0.2 ml and is mounted on a solid panel for wall or bench mountingSupplied with 100 ml capacity x 0.2 ml burettes.

_Attributes_
Description
	Twin burette volume change unit
	
Weight, kg
	8.3

_Related Products_
Accessory: Red Dye Kerosene Soluble 10G Phial for Colouring Kerosene. (26-1900)

[PRODUCT] Red Dye Kerosene Soluble 10G Phial for Colouring Kerosene. (26-1900)
Kerosene soluble red dye to colour the kerosene in the volume change unit (10g phial)

_Attributes_
Description
	Red dye

_Related Products_
Main: Twin Burette Volume Change Unit. (26-1892)

[PRODUCT] 6mm Connector 1/4BSp. (26-1922)
With sealing washer

_Attributes_
Description
	6mm Connector

[PRODUCT] Nylon Tubing 6mm Od 3500Kpa. (26-1926)
6 mm outside diameter x 4 mm inside diameter. For use up to a pressure of 3500 kPa. Priced per metre.

_Attributes_
Description
	Nylon tubing

_Related Products_
Main: ELE-Hoek Cell ADR Touch 2000 Compression Machine. 220 - 240 V 50/60H z (70-2630/01)
Main: Ele-Hoek Cell Nx 54.74mm Diameter. (70-1710)
Main: Hand Operated Pressure System. Complete with Pressure Gauge and Flexible Hose. (70-5000)
Main: Pair of Permeability End Caps Nx. Supplied with Distance Block. (70-1750)
Main: Pressure Test 3500 Oil/Water Constant Pressure System with Digital Pressure Gauge. (70-5130/01)

[PRODUCT] 6mm Elbow Connector. (26-1928)

_Attributes_
Description
	Elbow connector

[PRODUCT] 6mm T Connector. (26-1930)

_Attributes_
Description
	T connector

[PRODUCT] Volume Change Transducer Assembly 80Cm3 Capacity Maximum Working Pressure 1700Kpa (27-1641)
*Reversing valves to increase capacity*Steel case for wall mounting and access to piping*Supplied complete with calibration certificateThe Volume Change Transducer provides continuous measurements of volume change during the triaxial test. The assembly includes a valve to reverse the flow through the unit, providing increased capacity.

_Attributes_
Description
	Volume change transducer assembly
	
Maximum Pressure, psi
	250

_Specification_
Overall dimensions (l x w x h)
	178 x 229 x 368 mm
	
Maximum pressure
	1700 kPa
	
Excitation
	10 V DC
	
Output
	1.25 full range
	
Capacity
	80 ml
	
Connector
	5-pin DIN type
	
Weight kg
	4.5
	
Maximum Pressure
	250 psi (1,700 kPa).
	
Excitation
	10vDC.
	
Output
	1.25 Volts full range.
	
Capacity
	80 cc x 0.1 cc sensitivity.
	
Case
	Steel; hinged for access to piping.
	
Connector
	5-Pin DIN type.
	
Overall Dimensions
	9” w. x 7” d. x 14 -1/2” h. (22 9 x 178 x 368 mm).
	
Weight
	Net 10 lbs. (4.5 kg).
	
Maximum Pressure
	250 psi (1,700 kPa).
	
Excitation
	10vDC.
	
Output
	1.25 Volts full range.
	
Capacity
	80 cc x 0.1 cc sensitivity.
	
Case
	Steel; hinged for access to piping.
	
Connector
	5-Pin DIN type.
	
Overall Dimensions
	9” w. x 7” d. x 14 -1/2” h. (22 9 x 178 x 368 mm).
	
Weight
	Net 10 lbs. (4.5 kg).

_Related Products_
Main: Transducer Extension Cable 3.0 m (27-1717)
Main: Transducer Extension Cable 4.5 m (27-1719)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Load Measurement
Variious methods of axial displacement and load can be supplied. All devices comply with the accuracy specified in BS 1377, ASTM D2850, D4767. All transducers are supplied with a calibration certificate

[PRODUCT] 50kN Load Measuring Ring (78-0860)
Calibrated in compression.

_Standards_
EN 12697-34

_Attributes_
Description
	Load ring - 50 kN
	
Value of CBR %
	Above 40%
	
Overall Height, mm
	248
	
Force Capacity, kN
	50
	
Load device type
	Load ring

_Specification_
Capacity: kN, kgf, lbf
	50.0, 5000, 11,200
	
Typical Design sensitivity: N/div, kgf/div, lbf/div
	45.5, 4.54, 10.18
	
Overall height mm
	248
	
Approx weight kg
	7.9
	
Capacity
	50 kN
	
Value of CBR
	Above 40%
	
Capacity - lbf
	11,200
	
Capacity - kN
	50
	
Capacity - kgf
	5,000
	
Typical Design Sensitivity - lbf/div
	10.18
	
Typical Design Sensitivity - kN/div
	45.5
	
Typical Design Sensitivity - Kgf/div
	4.54
	
Overall Height
	9.76” (248 mm)
	
Approx Weight
	17.4 lbs.(7.9 kg)

_Related Products_
Main: CBR Loading Press, Hand-Operated (24-9345)
Main: CBR-Test 50 Machine 50 kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/02)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/01)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/06)
Accessory: Clamped Boss Load Ring - 10.0 kN (78-0460)
Accessory: Clamped Boss Load Ring - 2.0 kN (78-0060)
Accessory: Clamped Boss Load Ring - 28.0 kN (78-0760)
Accessory: Clamped Boss Load Ring - 3.0 kN (78-0160)
Accessory: Clamped Boss Load Ring - 4.5 kN (78-0260)
Accessory: Digital Proving Ring, 11,200 lbs (50.0 kN) (78-0864)
Main: Digital Tritest 50 (25-3518/01)
Main: Digital Tritest 50 Load Frame 110-120vAC (25-3518/02)
Main: Marshall Test 50 (45-6810/01)
Main: MultiPlex 50 Load Frame (25-3700/01)
Spare/Consumable: Spare Dial Indicator for Load Rings (78-5461)
Main: Versa-Loader (25-3525/02)

[PRODUCT] Clamped Boss Load Ring - 28.0 kN (78-0760)

_Attributes_
Description
	Load ring - 28 kN
	
Load device type
	Load ring
	
Force Capacity, kN
	28
	
Value of CBR %
	Average range of CBR
	
Overall Height, mm
	248

_Specification_
Capacity: kN, kgf, lbf
	28.0, 2800, 6000
	
Typical Design sensitivity: N/div, kgf/div, lbf/div
	25.5, 2.54, 5.45
	
Overall height mm
	248
	
Approx weight kg
	5.4
	
Capacity
	28 kN
	
Value of CBR
	Average range of CBR
	
Capacity - lbf
	6,000
	
Capacity - kN
	28
	
Capacity - kgf
	2,800
	
Typical Design Sensitivity - lbf/div
	5.45
	
Typical Design Sensitivity - kN/div
	25.5
	
Typical Design Sensitivity - Kgf/div
	2.54
	
Overall Height
	9.76” (248 mm)
	
Approx Weight
	11 .9 lbs.(5.4 kg)

_Related Products_
Accessory: 50kN Load Measuring Ring (78-0860)
Main: CBR Loading Press, Hand-Operated (24-9345)
Main: CBR-Test 50 Machine 50 kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/02)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/01)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/06)
Accessory: Clamped Boss Load Ring - 10.0 kN (78-0460)
Accessory: Clamped Boss Load Ring - 2.0 kN (78-0060)
Accessory: Clamped Boss Load Ring - 3.0 kN (78-0160)
Accessory: Clamped Boss Load Ring - 4.5 kN (78-0260)
Main: Conversion Frame. (24-9341)
Accessory: Digital Proving Ring, 6,000 lbs (28.0 kN) (78-0764)
Main: Digital Tritest 50 (25-3518/01)
Main: Digital Tritest 50 Load Frame 110-120vAC (25-3518/02)
Main: MultiPlex 50 Load Frame (25-3700/01)
Spare/Consumable: Spare Dial Indicator for Load Rings (78-5461)
Main: Versa-Loader (25-3525/02)

[PRODUCT] Clamped Boss Load Ring - 4.5 kN (78-0260)

_Attributes_
Description
	Load ring - 4.5 kN
	
Load device type
	Load ring
	
Force Capacity, kN
	4.5
	
Weight, lbs
	9.25

_Specification_
Capacity: kN, kgf, lbf
	4.5, 450, 1000
	
Typical Design sensitivity: N/div, kgf/div, lbf/div
	3.0, 0.30, 0.66
	
Overall height mm
	248
	
Approx weight kg
	3.5
	
Capacity - lbf
	1,000
	
Capacity - kN
	4.5
	
Capacity - kgf
	450
	
Typical Design Sensitivity - lbf/div
	0.66
	
Typical Design Sensitivity - kN/div
	3
	
Typical Design Sensitivity - Kgf/div
	0.3
	
Overall Height
	9.76” (248 mm)
	
Approx Weight
	7.7 lbs.(3.5 kg)

_Related Products_
Accessory: 50kN Load Measuring Ring (78-0860)
Accessory: Clamped Boss Load Ring - 10.0 kN (78-0460)
Accessory: Clamped Boss Load Ring - 2.0 kN (78-0060)
Accessory: Clamped Boss Load Ring - 28.0 kN (78-0760)
Accessory: Clamped Boss Load Ring - 3.0 kN (78-0160)
Main: Digital Direct/Residual Shear Apparatus Complete with Lever Loading Assembly. 110-120V 50/60Hz 1Ph. (26-2114/02)
Main: Digital Direct/Residual Shear Apparatus Complete with Lever Loading Assembly. 220-240V 50/60Hz 1Ph. (26-2114/01)
Accessory: Digital Proving Ring, 1,000 lbs (4.5 kN) (78-0264)
Main: Digital Tritest 50 (25-3518/01)
Main: Digital Tritest 50 Load Frame 110-120vAC (25-3518/02)
Main: MultiPlex 50 Load Frame (25-3700/01)
Spare/Consumable: Spare Dial Indicator for Load Rings (78-5461)
Main: Versa-Loader (25-3525/02)

[PRODUCT] Distance Piece Stainless Steel for Use with Submerisble Load Cells and Axial Strain Transducers. (27-1293)
Required when using submersible load cells.

_Attributes_
Description
	Distance piece stainless steel for use with submersible load cells
	
Load device type
	Stainless Steel distance piece for use with submersible loads cells
	
Weight, lbs
	1

_Related Products_
Accessory: Submersible Load Transducer Assembly 10kN Capacity In Compression. (27-1575)
Accessory: Submersible Load Transducer Assembly 5kN Capacity In Compression. (27-1573)
Main: Transducer Extension Cable 3.0 m (27-1717)
Main: Transducer Extension Cable 4.5 m (27-1719)

[PRODUCT] S-Type Load Cell 5 kN.for Triaxial Tests. Fitted with 5 Pin Din Plug. (27-1551)
*Repeatability better than ± 0.02% of rated output*Non-Linearity better than ± 0.03% of rated output*Supplied complete with 5-pin DIN type connector for connection to GDUIdeally suited for a wide range of applications, ELE S-type load cells provide high accuracy and minimum deformation. Various models are available, with the necessary adaptors, for use with ELE Triaxial Load Frames, Multiplex 50/Marshall Test 50/CBR Test 50 and Direct Shear machine.

_Attributes_
Load device type
	S-Type
	
Force Capacity, kN
	5
	
Description
	S-Type load cell
	
Environmental Protection
	IP65

_Related Products_
Main: Digital Direct/Residual Shear Apparatus Complete with Lever Loading Assembly. 110-120V 50/60Hz 1Ph. (26-2114/02)
Main: Digital Direct/Residual Shear Apparatus Complete with Lever Loading Assembly. 220-240V 50/60Hz 1Ph. (26-2114/01)

[PRODUCT] S-Type Load Cell 10 kN.for Triaxial Tests. Fitted with 5 Pin Din Plug. (27-1553)
*Repeatability better than ± 0.02% of rated output*Non-Linearity better than ± 0.03% of rated output*Supplied complete with 5-pin DIN type connector for connection to GDUIdeally suited for a wide range of applications, ELE S-type load cells provide high accuracy and minimum deformation. Various models are available, with the necessary adaptors, for use with ELE Triaxial Load Frames, Multiplex 50/Marshall Test 50/CBR Test 50 and Direct Shear machine.

_Attributes_
Load device type
	S-Type
	
Force Capacity, kN
	10
	
Description
	S-Type load cell
	
Environmental Protection
	IP65

[PRODUCT] S-Type Load Cell 25 kN.for Triaxial Tests. 27-1293 required separately. (27-1555)
*Repeatability better than ± 0.02% of rated output*Non-Linearity better than ± 0.03% of rated output*Supplied complete with 5-pin DIN type connector for connection to GDUIdeally suited for a wide range of applications, ELE S-type load cells provide high accuracy and minimum deformation. Various models are available, with the necessary adaptors, for use with ELE Triaxial Load Frames, Multiplex 50/Marshall Test 50/CBR Test 50 and Direct Shear machine.

_Attributes_
Load device type
	S-Type
	
Force Capacity, kN
	25
	
Description
	S-Type load cell
	
Environmental Protection
	IP65

[PRODUCT] Submersible Load Transducer Assembly 5kN Capacity In Compression. (27-1573)
*Eliminates effects of piston friction on readings*Unaffected by cell confining pressures*Easily installed in triaxial cell*Supplied complete with calibration certificate and 5-pin DIN type connector for use with GDUSubmersible Load Transducers are used to measure accurately the axial loads applied to triaxial test specimens. Consisting of a load cell and piston assembly these units replace the standard triaxial cell loading piston. A major advantage is that these transducers measure loads directly on top of the specimen. All transducers are supplied complete with a 5-pin DIN type connector and calibration certificate.

_Attributes_
Load device type
	Submersible
	
Force Capacity, kN
	5
	
Description
	Submersible load transducer
	
Weight, lbs
	2.25

_Specification_
Dimensions
	75 x 50 mm (dia x h) excluding piston and adaptor
	
Overload capacity
	150%
	
Output
	26 mv full range
	
Excitation
	10 V DC (15 V DC max)
	
Non-linearity
	0.1% maximum
	
Hysteresis Deflection
	0.1% maximum 0.05 mm at full load
	
Side force
	50% full scale maximum without effect
	
Connector
	5-pin DIN plug
	
Compensated temperature range
	0 to 50°C
	
Weight g
	850

_Related Products_
Accessory: Distance Piece Stainless Steel for Use with Submerisble Load Cells and Axial Strain Transducers. (27-1293)
Main: S-Type Load Cell 10,000 lb Capacity (27-1587)
Main: S-Type Load Cell 2,000 lb Capacity (27-1583)
Main: S-Type Load Cell 500 lb Capacity (27-1581)
Main: Transducer Extension Cable 3.0 m (27-1717)
Main: Transducer Extension Cable 4.5 m (27-1719)

[PRODUCT] Submersible Load Transducer Assembly 10kN Capacity In Compression. (27-1575)
*Eliminates effects of piston friction on readings*Unaffected by cell confining pressures*Easily installed in triaxial cell*Supplied complete with calibration certificate and 5-pin DIN type connector for use with GDUSubmersible Load Transducers are used to measure accurately the axial loads applied to triaxial test specimens. Consisting of a load cell and piston assembly these units replace the standard triaxial cell loading piston. A major advantage is that these transducers measure loads directly on top of the specimen. All transducers are supplied complete with a 5-pin DIN type connector and calibration certificate.

_Attributes_
Load device type
	Submersible
	
Force Capacity, kN
	10
	
Description
	Submersible load transducer
	
Compensated Temperature Range
	0 - 50

_Specification_
Dimensions
	76 x 50 mm (dia x h) excluding piston and adaptor
	
Overload capacity
	150%
	
Output
	27 mv full range
	
Excitation
	11 V DC (15 V DC max)
	
Non-linearity
	0.1% maximum
	
Hysteresis Deflection
	0.1% maximum 0.05 mm at full load
	
Side force
	50% full scale maximum without effect
	
Connector
	5-pin DIN plug
	
Compensated temperature range
	1 to 50°C
	
Weight g
	850

_Related Products_
Accessory: Distance Piece Stainless Steel for Use with Submerisble Load Cells and Axial Strain Transducers. (27-1293)

[GROUPED PRODUCT MATRIX]
Model No.
	Type
	Capacity, kN
	N/A for this Product Group

[PRODUCT GROUP] Axial Displacement
Variious methods of axial displacement and load can be supplied. All devices comply with the accuracy specified in BS 1377, ASTM D2850, D4767. All transducers are supplied with a calibration certificate

[PRODUCT] Dial Gauge 25mm Travel X 0.01mm Divisions (25-4210)
25 mm travel x 0.01 mm

_Standards_
BS 1377

_Attributes_
Description
	Dial gauge 25mm travel x 0.01mm divisions
	
Dial Indicator
	25 mm Range

_Related Products_
Accessory: Axial Strain Transducer Assembly 50mm Travel Fitted with 5 Pin Din Plug. (27-1617)
Spare/Consumable: Dial Indicator - 1.0" Range (88-4100)
Main: Digital Tritest 50 Load Frame 110-120vAC (25-3518/02)
Main: Electronic Digital Indicator, 1.0"/25.4 mm range (88-4220)
Main: Versa-Loader (25-3525/02)

[PRODUCT] Axial Strain Transducer Assembly 50mm Travel Fitted with 5 Pin Din Plug. (27-1617)
0 to 50 mm range. For use with Triaxial Cells. *Ideally suited for use with GDU for accuratedisplacement measurements*Models available for use in consolidation, shear,CBR and triaxial test applications*Supplied complete with mounting hardware forspecified productsDisplacement Transducers are used in consolidation, shear, CBR and triaxial test applications for accuratevdisplacement measurements. They are supplied complete with a 5-pin DIN type connector for direct connection to the GDU.

_Attributes_
Description
	Axial strain transducer assembly 50mm travel
	
Mounting Bracket
	Included as standard.

_Specification_
Construction
	Fully encapsulated electronics,sealed in a stainless steel case
	
Excitation
	10 V DC
	
Connector
	5-pin DIN type
	
Mounting bracket
	Included as standard
	
Weight kg
	0.45
	
Construction
	Fully encapsulated electronics, sealed in a stainless steel case.
	
Excitation
	10vDC.
	
Connector
	5-Pin DIN type.
	
Mounting Bracket
	Included as standard.
	
Weight
	Net 1 lb. (0.45 kg).

_Related Products_
Main: CBR Displacement Transducer (27-1706)
Main: Consolidation Transducer Assembly 15mm Travel Fitted with 5 Pin Din Plug. (27-1649)
Main: Dial Gauge 25mm Travel X 0.01mm Divisions (25-4210)
Accessory: Horizontal Displacement Transducer Assembly 15mm Travel 5 Pin Din Plug Mounting Pillar (27-1697)
Main: Transducer Extension Cable 3.0 m (27-1717)
Main: Transducer Extension Cable 4.5 m (27-1719)
Accessory: Vertical Displacement Transducer Assembly 15mm Travel with 5 Pin Din Plug Bracket for Shear Box (27-1689)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[CATEGORY] Sample Preparation

[PRODUCT GROUP] Accessories for CU/CU effective stress

[PRODUCT] Filter Paper Drain 38mm/1.5 Inch Diameter. Pack of 50. (25-5200)
Filter paper drain 38 mm diameter (Pack Of 50).

_Attributes_
Description
	Filter paper drain 38 mm

[PRODUCT] Filter Paper Drain 50mm Diameter. Pack of 50 (25-5580)
Filter paper drain 50 mm diameter (Pack Of 50).

_Attributes_
Description
	Filter paper drain 50 mm

[PRODUCT] Porous Disc 70mm Diameter Pack of 2. (25-6561)
70 mm diameter porous disc (pack of 2).

_Standards_
ASTM D2850, ASTM D4767, ASTM D5084, AASHTO T296, AASHTO T297, ASTM D7181

_Attributes_
Description
	Porous disc 70 mm
	
Diameter, ”
	70 mm

_Related Products_
Accessory: 1.4" Porous Stones (25-4461)
Accessory: 4.0" Porous Stones (25-7761)
Accessory: Porous Disc 100mm Diameter Pack of 2. (25-7661)
Accessory: Porous Stones 2.8" (25-6721)
Main: Tri-Flex 2 Permeability Test Cell (25-0690)

[PRODUCT] Porous Disc 38mm/1.5 Inch Diameter. Pack of 2. (25-5181)
Porous disc For 38 mm/1.5 Inch samples (Pack Of 2).

_Attributes_
Description
	Porous disc 1.5"

[PRODUCT] Porous Disc 50mm Pack of 2 (25-5561)
50 mm diameter porous disc (Pack Of 2).

_Attributes_
Description
	Porous disc 50 mm

[PRODUCT] Porous Disc 100mm Diameter Pack of 2. (25-7661)
100 mm diameter porous disc (Pack Of 2).

_Standards_
ASTM D2850, ASTM D4767, ASTM D5084, AASHTO T296, AASHTO T297, ASTM D7181

_Attributes_
Description
	Porous disc 100 mm
	
Diameter, ”
	100 mm

_Related Products_
Accessory: 1.4" Porous Stones (25-4461)
Accessory: 4.0" Porous Stones (25-7761)
Accessory: Porous Disc 70mm Diameter Pack of 2. (25-6561)
Accessory: Porous Stones 2.8" (25-6721)
Main: Tri-Flex 2 Permeability Test Cell (25-0690)

[PRODUCT] Filter Paper Drain 70mm/2.8 Inch Diameter. Pack of 50. (25-6580)
Filter paper drain 70 mm diameter (Pack Of 50).

_Standards_
ASTM D2850, ASTM D4767, ASTM D7181, AASHTO T296, AASHTO T297

_Attributes_
Description
	Filter paper drain 70 mm
	
Diameter, ”
	2.8"

_Related Products_
Accessory: 1.4" Filter Paper Drains (25-4880)
Accessory: Filter Paper Drain 100mm/4 Inch Diameter. Pack of 50. (25-7670)

[PRODUCT] Filter Paper Drain 100mm/4 Inch Diameter. Pack of 50. (25-7670)
Filter paper drain 100 mm diameter (Pack Of 50).

_Standards_
ASTM D2850, ASTM D4767, ASTM D7181, AASHTO T296, AASHTO T297

_Attributes_
Description
	Filter paper drain 100mm
	
Diameter, ”
	4.0"

_Related Products_
Accessory: 1.4" Filter Paper Drains (25-4880)
Accessory: Filter Paper Drain 70mm/2.8 Inch Diameter. Pack of 50. (25-6580)

[PRODUCT] Valve No Volume Change 1/4 Inch BSp Fitted with 6 mm Connector and Integral Sealing Ring. (25-4520)

_Standards_
ASTM D2850, ASTM D4767, ASTM D7181, AASHTO T296, AASHTO T297

_Attributes_
Description
	No volume change valve
	
Weight, lbs
	0.292

_Related Products_
Main: 70mm Triaxial Cell 1700Kpa with 5 Pressure/ Drainage Ports. Supplied with Two Valves. (25-4117)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Membrane Placing Tools

[GROUPED PRODUCT MATRIX]
Model No.
	Sample dia.
	
25-4290
	38 mm
	
25-5470
	50 mm
	
25-6470
	70 mm
	
25-7610
	100 mm

[PRODUCT GROUP] Membrane Sealing Rings

[GROUPED PRODUCT MATRIX]
Model No.
	Sample dia.
	
25-5081
	38 mm
	
25-5461
	50 mm
	
25-6461
	70 mm
	
25-7631
	100 mm

[PRODUCT GROUP] Pressure Pads

[GROUPED PRODUCT MATRIX]
Model No.
	Sample dia.
	
25-5050
	38 mm
	
25-5430
	50 mm
	
25-6430
	70 mm
	
25-7590
	100 mm

[PRODUCT GROUP] Rubber Membranes

[GROUPED PRODUCT MATRIX]
Model No.
	Sample dia.
	
25-5061
	38 mm
	
25-5441
	50 mm
	
25-6441
	70 mm
	
25-7621
	100 mm

[PRODUCT GROUP] Suction Membrane Devices

[GROUPED PRODUCT MATRIX]
Model No.
	Sample dia.
	
25-5100
	38 mm
	
25-5480
	50 mm
	
25-6480
	70 mm
	
25-7640
	100 mm

[PRODUCT GROUP] Two-way Split Formers
For non-cohesive soils

[GROUPED PRODUCT MATRIX]
Model No.
	Sample dia.
	
25-5120
	38 mm
	
25-5500
	50 mm
	
25-6500
	70 mm
	
25-6680
	2.8"
	
25-7650
	100 mm

[PRODUCT GROUP] Two-way Split Moulds
For cohesive soils

[GROUPED PRODUCT MATRIX]
Model No.
	Sample dia.
	
25-5130
	38 mm
	
25-5530
	50 mm
	
25-6530
	70 mm

[CATEGORY] Pressure Systems
We offer a range of products designed to supply and monitor all those parameters necessary for the successfultesting of geotechnical materials. Two types of constant pressure systems are available:1. Air/water system operated by a pneumatic compressor2. A motorised oil/water system

[PRODUCT GROUP] Air/Water Pressure Systems - up to 1000 kPa
Where a laboratory requires a number of constant, but independent and variable pressure sources, the use of a pnuematic compressor is recommended. Depending on the capacity and volume of the unit, a series of pressure sources can be provded to various test stations around the laboratory. Compressed air must be controlled and delivered to a system designed to transfer the controlled pressure to the fluid (usually water), which applies the various test pressures, e.g., a confining pressure in a triaxial test. The pressure reducing panelsare used in conjunction with a bladder-type air/water interface assembly. Each individual pressure take off from the reducing panel will require a bladder interface assembly. Connection of the reducing panels to the compressor/water trap outlet and to other reducing panels requires the use of nylon tubing.

[PRODUCT] Pressure Test 1700 Oil/Water Constant Pressure System 0 to 1700Kpa 220-240V 50/60Hz 1Ph. (26-1800/01)
* 0 to 1700 kPa (250 lbf/in²) fully variable* Continuous constant pressure control* One litre capacityThe ELE oil/water constant pressure system , PressureTest 1700, is extemely versatile and can be used in conjunction of with a wide range of test equipment. The unit provides continuous variable pressure up to 1700 kPa. Pressure is increased or decreased simply by turning a control wheel.The apparatus is supplied without a gauge for those customers who have suitable pressure monitoring equipment. A digital pressure gauge is offered as an accessory. The machine features a clear hydraulic/water interface reservoir and up to one litre capacity of water is available under pressure.* 0 to 1700 kPa (250 lbf/in²) fully variable.

_Further Information_
Dimensions (without gauge) 240 x 400 x 500 mm (l x w x h).

_Attributes_
Description
	Pressure Test 1700 Oil/Water Constant Pressure System
	
Power Supply
	220 - 240 V AC, 50 - 60 Hz, 1 ph

_Related Products_
Accessory: Digital Pressure Gauge 1700 Kpa. for Use with 26-1800 Series Oil/Water Constant Pressure System. (26-1820)
Spare/Consumable: Oil 5 Litres T46 (26-1805)

[PRODUCT] Bladder-Type Air/Water Pressure Assembly. 1000 Kpa Maximum Working Pressure. (26-1746)
With transparent plastic chamber for operating continuously at pressures up to 1000 kPa. A length of tubing is provided for connecting the air/water cylinder outlet to a pressure measuring system. * Used to supply hydraulic pressure from a pneumatic pressure source. * Prevents air entering the hydraulic pressure system. * Maximum working pressure 1000kpa. * Supplied with connectors and tubing for fitting to pressure measuring systems. 

_Attributes_
Description
	Bladder-type air/water pressure assembly
	
Weight, kg
	5.6

_Related Products_
Accessory: Nylon Tubing 30 Metre Length. (26-1769)
Spare/Consumable: Pneumatic Pressure Reducing Panel. Provides Two Independent Pressure Outlets 1000 Kpa Max. (26-1760)
Spare/Consumable: Replacement Bladder Wide Neck (38mm Id) (26-1746/10)

[PRODUCT] Air Compressor (83-1730/01)

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Working Pressure, kPa
	700
	
Description
	Air Compressor Unit

_Specification_
Dimensions (l x w x h)
	483 x 457 x 864 mm
	
Free air delivery
	2.0 cfm
	
Receiver capacity
	50 litres
	
Maximum pressure
	1000 kPa
	
Continuous working pressure
	700 kPa
	
Electrical supply
	220 – 240 V AC1 ph 50 Hz
	
Water Trap
	No
	
Weight
	57 kg

[PRODUCT] Pneumatic Pressure Reducing Panel. Provides Two Independent Pressure Outlets 1000 Kpa Max. (26-1760)
Comprising two constant pressure reducing valves with inlet water trap and pressure indicator. The unit allows a maximum output pressure of 1000 kPa. Maximum input pressure should not exceed 1400 kPa. The panel has an inlet connector to accept Nylon tubing from the air compressor and two 6 mm outlets for connecting Bladdertype Air/Water Pressure Assemblies. An outlet connectoris fitted for the connection of an additional panel using Nylon tubing to increase the total capacity of the system. This outlet is blanked off when not required.

_Attributes_
Description
	Pneumaticpressure reducing panel
	
Weight, kg
	4

_Related Products_
Main: Bladder-Type Air/Water Pressure Assembly. 1000 Kpa Maximum Working Pressure. (26-1746)

[PRODUCT] Six-Way Pneumatic Pressure Control Panel. (26-1872)
The six-way pressure control systems have been designed specifically for the monitoring of up to six independent pressures. They are particularly useful for setting up and controlling a 3-cell effective stress system using three independent back pressures. The panel os used in conjunction with the Universal Pump and Pressure Indicating Panel which provides pressure monitoring and facilities for filling and de-airing the system. Comprising six pneumatic control valves mounted in a housing for controlling six independant outlets. Supplied with connection ports for coupling panel to EL26-1880. Maximum inlet pressure 1400 kPa maximum outlet pressure 1000 kPa.

_Attributes_
Description
	Six-Way Pneumatic Pressure Control Panel

[PRODUCT] Nylon Tubing 30 Metre Length. (26-1769)
30 metre length. For pressures up to 1700 kPa. Used for connecting Air Compressors to Pneumatic Pressure Reducing Panels, or for connecting two Pressure Reducing Panels together.

_Further Information_
Nylon tubing 30 metres with pressure fittings.

_Attributes_
Description
	Nylon tubing
	
Weight, kg
	2

_Related Products_
Main: Bladder-Type Air/Water Pressure Assembly. 1000 Kpa Maximum Working Pressure. (26-1746)

[PRODUCT] Air Compressor (83-1735/01)

_Attributes_
Description
	Air Compressor Unit
	
Working Pressure, kPa
	1,000

_Specification_
Dimensions (l x w x h)
	1321 x 457 x 914 mm
	
Free air delivery
	6.0 cfm
	
Receiver capacity
	116 litres
	
Maximum pressure
	1380 kPa
	
Continuous working pressure
	1000 kPa
	
Electrical supply
	221 â€“ 240 V AC1 ph 50 Hz
	
Water Trap
	Yes
	
Weight
	149 kg

[PRODUCT] Replacement Bladder Wide Neck (38mm Id) (26-1746/10)

_Attributes_
Description
	Replacement bladder

_Related Products_
Main: Bladder-Type Air/Water Pressure Assembly. 1000 Kpa Maximum Working Pressure. (26-1746)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Modular Pressure Panel System
* Modular system for flexibility* Wall mounting* Four outlets* 6 mm diameter pipework for quick filling and draining* Standard type valves on all units - on/off with no volume change* Ideal system for geotechnical laboratoriesThis modular system provides flexibility and cost saving by enabling only those units that are relevant to the particular testing requirements to be selected. It is simple to update the system with the addition of other units, which can be quickly connected together.The units may be used with a variety of pressure systems, such as pnuematic and oil/water and are designed to accept pressures of up to 1700 kPa where appropriate.

[PRODUCT] Universal Pump and Pressure Indicating Panel 1700Kpa. (26-1880)
This is the main pressure display in the system for monitoring various pressures and also provides fine control of the pressure within the system using the rotary hand pump. The unit is fitted with a dual calibrated 250 mm diamter pressure gauge, four inlet/outlet no-volume change valves, screw controlled rotary hand pump, water reservoir and isolating valves. The unit is housed in a hinged case for wall or bench mounting. By using an isolating valve the panel may be used to monitor cell or back pressure. 1700 kPa and 250 lbf/in2.

_Attributes_
Description
	Universal Pump and Pressure Indicating Panel 1700Kpa
	
Weight, kg
	12

_Related Products_
Spare/Consumable: Pressure Gauge 1700Kpa (250Psi) 250mm Diameter. (26-1865/10)

[PRODUCT] Pressure Gauge 1700Kpa (250Psi) 250mm Diameter. (26-1865/10)
250 mm diameter.

_Attributes_
Description
	Pressure Gauge 1700Kpa (250Psi) 250mm Diameter.
	
Weight, kg
	2.5

_Related Products_
Main: Universal Pump and Pressure Indicating Panel 1700Kpa. (26-1880)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Oil/Water Constant Pressure System
* 0 to 1700 kPa (250 lbf/in²) fully variable* Continuous constant pressure control* One litre capacityThe ELE oil/water constant pressure system, PressureTest 1700, is extemely versatile and can be used in conjunction of with a wide range of test equipment. The unit provides continuous variable pressure up to 1700 kPa. Pressure is increased or decreased simply by turning a control wheel.The apparatus is supplied without a gauge for those customers who have suitable pressure monitoring equipment. A digital pressure gauge is offered as an accessory. The machine features a clear hydraulic/water interface reservoir and up to one litre capacity of water is available under pressure.

[PRODUCT] Pressure Test 1700 Oil/Water Constant Pressure System 0 to 1700Kpa 220-240V 50/60Hz 1Ph. (26-1800/01)
* 0 to 1700 kPa (250 lbf/in²) fully variable* Continuous constant pressure control* One litre capacityThe ELE oil/water constant pressure system , PressureTest 1700, is extemely versatile and can be used in conjunction of with a wide range of test equipment. The unit provides continuous variable pressure up to 1700 kPa. Pressure is increased or decreased simply by turning a control wheel.The apparatus is supplied without a gauge for those customers who have suitable pressure monitoring equipment. A digital pressure gauge is offered as an accessory. The machine features a clear hydraulic/water interface reservoir and up to one litre capacity of water is available under pressure.* 0 to 1700 kPa (250 lbf/in²) fully variable.

_Further Information_
Dimensions (without gauge) 240 x 400 x 500 mm (l x w x h).

_Attributes_
Description
	Pressure Test 1700 Oil/Water Constant Pressure System
	
Power Supply
	220 - 240 V AC, 50 - 60 Hz, 1 ph

_Related Products_
Accessory: Digital Pressure Gauge 1700 Kpa. for Use with 26-1800 Series Oil/Water Constant Pressure System. (26-1820)
Spare/Consumable: Oil 5 Litres T46 (26-1805)

[PRODUCT] Oil 5 Litres T46 (26-1805)
5 litres

_Attributes_
Description
	Oil 5 Litres T46

_Related Products_
Main: Pressure Test 1700 Oil/Water Constant Pressure System 0 to 1700Kpa 220-240V 50/60Hz 1Ph. (26-1800/01)

[PRODUCT] Digital Pressure Gauge 1700Kpa. for Ele Triaxial Cells. (27-1620)
For ELE Triaxial Cells. The Digital Pressure Gauge offers highly accurate pressure measurement and digital readout for ELE triaxial cells.

_Standards_
ASTM D2850, ASTM D4767, ASTM D7181, ASTM D5084, AASHTO T296, AASHTO T297

_Attributes_
Description
	Digital pressure gauge
	
Battery Life
	1400

_Specification_
Capacity
	250 psi (1,700 kPa).
	
Display
	LCD.
	
Display Units
	PSI, kPa, MPa.
	
Accuracy
	Better than 1% of indicated pressure.
	
Read Rate
	Two samples per second.
	
Power Supply
	3 volt battery, CR 234 0 type.
	
Battery Life
	1400 hours continuous operation.
	
Dimensions
	2.30â€ w. x 1.25 â€ d. x 3.75â€ h. (59 x 32 x 95 mm.)
	
Weight
	Net 1/4 lb. (125 g).

_Related Products_
Main: 70mm Triaxial Cell 1700Kpa with 5 Pressure/ Drainage Ports. Supplied with Two Valves. (25-4117)
Main: Digital Pressure Gauge for Tri-Flex 2 and Permeability Cells (27-1622)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[CATEGORY] Direct Shear and Vane Tests
Every building or structure that is built in or on the earth imposes loads on the soil supporting the foundations. The stresses set up in the soil causes deformation of the soil with stress failure being caused by slippage of soil particles, which may lead to sliding of one body of soil relative to the surrounding mass.

[PRODUCT GROUP] Direct/Residual Shear Apparatus

[PRODUCT] Digital Direct/Residual Shear Apparatus Complete with Lever Loading Assembly. 110-120V 50/60Hz 1Ph. (26-2114/02)
* Microprocessor control* Large on-board LCD screen display* Direct entry via touch sensitive keyboard* Rapid approach and return to start datum* Fully variable speed, 0.00001 to 9.99999 mm/minute* Accepts specimens up to 100 mm squareThe ELE Direct Shear Apparatus accepts specimens 60 mm, 100 mm square or 2.5 inches in diameter. The use of a microprocessor controlled drive system and keyboard entry gives the apparatus a wide range of features that include pause and speed reset during test, RS 232C interface, operator programming of speed and control functions, self test diagnostics and many other features. A return to start datum provides a positive means of reversing the shearbox when either preparing for a new test or continuing with residual testing procedures.Safety forward/reverse travel limit switches are fitted as standard and monitored through the electronics system control.The electronics are housed in a modern moulded shroud, which includes a large LCD display and keyboard entry. The apparatus is enclosed in a robustly constructed case, has been designed for floor mounting and is supplied complete with carriage, loading hanger and 10:1 lever loading device

_Standards_
ASTM D3080, AASHTO T236

_Further Information_
for 110 - 120 V AC, 50 - 60 Hz, 1 ph.

_Attributes_
Voltage Supply
	110-120V 50/60Hz
	
Description
	Digital Direct/Residual Shear Apparatus
	
Vertical Load, lbf
	2,200

_Specification_
Sample Size
	Accepts either 2.42 ”, 2.5” diam.; 60 mm square samples using accessory shear box assemblies, not included.
	
Speed Range
	Variable in either English or Metric units between 0.000001”(0.00001 mm) to 0.399999” (9.99999 mm) per minute.
	
Shear Force
	1,000 lbf. (4.5 kN) maximum.
	
Vertical Load
	2,200 lbf. (1,000 kN) using 10:1 lever ratio.
	
Dimensions
	44.7” l. x 12 .6” w. x 49.6” h. (1,135 x 320 x 1,260 mm).
	
Weight
	Net 181 lbs. (82 kg).

_Related Products_
Accessory: Clamped Boss Load Ring - 2.0 kN (78-0060)
Accessory: Clamped Boss Load Ring - 3.0 kN (78-0160)
Accessory: Clamped Boss Load Ring - 4.5 kN (78-0260)
Accessory: Dial Gauge 10mm Travel X 0.002mm Divisions. (25-0440)
Spare/Consumable: Dial Indicator - 1.0" Range (88-4100)
Main: Digital Direct/Residual Shear Apparatus Complete with Lever Loading Assembly. 220-240V 50/60Hz 1Ph. (26-2114/01)
Accessory: Digital Proving Ring, 1,000 lbs (4.5 kN) (78-0264)
Accessory: Digital Proving Ring, 450 lbs (2.0 kN) (78-0064)
Accessory: Electronic Digital Indicator, 0.600"/15 mm range (88-4210)
Main: H60 Field Inspection Vane Tester 0-200Kpa In Carrying Case. includes calibration and certificates. (26-3335)
Main: Hand Vane Tester (26-3346)
Main: Laboratory Vane Apparatus with 4 Springs and 12.7mm Vane; Hand Operated. (26-2270)
Accessory: Mechanical Dial Indicator - 25 mm Range Clockwise Movement (88-4110)
Main: Pocket Shearmeter with 3 Vanes 0 to 1Kgf/Cm2 X 0.5Kgf/Cm2. (26-2261)
Accessory: S-Type Load Cell 5 kN.for Triaxial Tests. Fitted with 5 Pin Din Plug. (27-1551)
Accessory: Set of Weights 50 kg Slotted. (26-2132)
Accessory: Shear Box Assembly 100mm Sq. (26-2197)
Accessory: Shear Box Assembly 2.5 Inch Diameter (26-2213)
Accessory: Shear Box Assembly 60mm Sq. (26-2181)
Accessory: Vertical Dial Indicator, English (25-0445)
Accessory: Vertical Displacement Transducer Assembly 15mm Travel with 5 Pin Din Plug Bracket for Shear Box (27-1689)
Accessory: Weight Set A (25-0535)
Accessory: Weight Set B (25-0537)

[PRODUCT] Digital Direct/Residual Shear Apparatus Complete with Lever Loading Assembly. 220-240V 50/60Hz 1Ph. (26-2114/01)
* Microprocessor control* Large on-board LCD screen display* Direct entry via touch sensitive keyboard* Rapid approach and return to start datum* Fully variable speed, 0.00001 to 9.99999 mm/minute* Accepts specimens up to 100 mm squareThe ELE Direct Shear Apparatus accepts specimens 60 mm, 100 mm square or 2.5 inches in diameter. The use of a microprocessor controlled drive system and keyboard entry gives the apparatus a wide range of features that include pause and speed reset during test, RS 232C interface, operator programming of speed and control functions, self test diagnostics and many other features. A return to start datum provides a positive means of reversing the shearbox when either preparing for a new test or continuing with residual testing procedures.Safety forward/reverse travel limit switches are fitted as standard and monitored through the electronics system control.The electronics are housed in a modern moulded shroud, which includes a large LCD display and keyboard entry. The apparatus is enclosed in a robustly constructed case, has been designed for floor mounting and is supplied complete with carriage, loading hanger and 10:1 lever loading device.

_Standards_
ASTM D3080, AASHTO T236, BS 1377, EN 1997-2

_Further Information_
for 220 - 240 V AC, 50 - 60 Hz, 1 ph.

_Attributes_
Description
	Digital Direct/Residual Shear Apparatus
	
Voltage Supply
	220-240 V 50/60 Hz
	
Vertical Load, lbf
	2,200

_Specification_
Sample Size
	Accepts either 2.42 ”, 2.5” diam.; 60 mm square samples using accessory shear box assemblies, not included.
	
Speed Range
	Variable in either English or Metric unitsbetween 0.000001”(0.00001 mm) to 0.399999” (9.99999mm) per minute.
	
Shear Force
	1,000 lbf. (4.5 kN) maximum.
	
Vertical Load
	2,200 lbf. (1,000 kN) using 10:1 lever ratio.
	
Dimensions
	44.7” l. x 12 .6” w. x 49.6” h. (1,135 x 320 x 1,260 mm).
	
Weight
	Net 181 lbs. (82 kg).

_Related Products_
Accessory: Clamped Boss Load Ring - 2.0 kN (78-0060)
Accessory: Clamped Boss Load Ring - 3.0 kN (78-0160)
Accessory: Clamped Boss Load Ring - 4.5 kN (78-0260)
Accessory: Dial Gauge 10mm Travel X 0.002mm Divisions. (25-0440)
Spare/Consumable: Dial Indicator - 1.0" Range (88-4100)
Main: Digital Direct/Residual Shear Apparatus Complete with Lever Loading Assembly. 110-120V 50/60Hz 1Ph. (26-2114/02)
Accessory: Digital Proving Ring, 1,000 lbs (4.5 kN) (78-0264)
Accessory: Digital Proving Ring, 450 lbs (2.0 kN) (78-0064)
Accessory: Electronic Digital Indicator, 0.600"/15 mm range (88-4210)
Main: H60 Field Inspection Vane Tester 0-200Kpa In Carrying Case. includes calibration and certificates. (26-3335)
Main: Hand Vane Tester (26-3346)
Accessory: Horizontal Displacement Transducer Assembly 15mm Travel 5 Pin Din Plug Mounting Pillar (27-1697)
Main: Laboratory Vane Apparatus with 4 Springs and 12.7mm Vane; Hand Operated. (26-2270)
Accessory: Mechanical Dial Indicator - 25 mm Range Clockwise Movement (88-4110)
Main: Pocket Shearmeter with 3 Vanes 0 to 1Kgf/Cm2 X 0.5Kgf/Cm2. (26-2261)
Accessory: S-Type Load Cell 5 kN.for Triaxial Tests. Fitted with 5 Pin Din Plug. (27-1551)
Accessory: Set of Weights 50 kg Slotted. (26-2132)
Accessory: Shear Box Assembly 100mm Sq. (26-2197)
Accessory: Shear Box Assembly 2.5 Inch Diameter (26-2213)
Accessory: Shear Box Assembly 60mm Sq. (26-2181)
Accessory: Vertical Dial Indicator, English (25-0445)
Accessory: Vertical Displacement Transducer Assembly 15mm Travel with 5 Pin Din Plug Bracket for Shear Box (27-1689)
Accessory: Weight Set A (25-0535)
Accessory: Weight Set B (25-0537)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	Voltage
	N/A for this Product Group

[PRODUCT GROUP] Shear Box Assemblies
All shearbox assemblies are designed to fit the carriage of the Direct/Residual Shear Apparatus. They are supplied complete with twoo porous plates, on retaining plate and a loading pad. The three sizes supplied comply with the relevant requirements of BS 1377 and ASTM D3080. All assemblies can be used for quick shear tests or drained/residual shear tests. Optional accessories are available including specimen cutters and extrusion tools. The table shows the complete range of shearbox assemblies and accessories.

[PRODUCT] Shear Box Assembly 100mm Sq. (26-2197)
*Manufactured from corrosion resistant materials*Sample size 100 x 100mm x 25mm high meeting BS 1377*Incorporates PTFE faced box separation screws to reduce friction*Supplied complete with upper and lower porous plates and loading pad*Suitable for quick undrained or drained/residual tests.

_Standards_
ASTM D3080, AASHTO T236

_Further Information_
All shearbox assemblies are designed to fit the carriage of 26-2114 series Digital Direct/Residual Shear Apparatus. They are supplied complete with three porous plates, one retaining plate and a loading pad. The three sizes supplied comply with the relevant requirements of BS 1377 and ASTM D3080. All assemblies can be used for quick shear tests or drained/residual shear tests.Optional accessories are available including specimen cutters and extrusion tools.

_Attributes_
Description
	Shear box assembly
	
Specimen size
	100 x 100 mm
	
Sample Size
	100 x 100 mm

_Specification_
Specimen area
	100 x 100 mm
	
Specimen thickness
	25 mm
	
Weight kg
	5.2
	
Relevant standard
	BS 1377

_Related Products_
Main: 2.42" Diameter Shear Box Assembly (California Type) (26-2223)
Main: Digital Direct/Residual Shear Apparatus Complete with Lever Loading Assembly. 110-120V 50/60Hz 1Ph. (26-2114/02)
Main: Digital Direct/Residual Shear Apparatus Complete with Lever Loading Assembly. 220-240V 50/60Hz 1Ph. (26-2114/01)
Accessory: Shear Box Assembly 60mm Sq. (26-2181)
Spare/Consumable: Specimen Cutter 100mmsq. (26-2201)

[PRODUCT] Shear Box Assembly 60mm Sq. (26-2181)
*Manufactured from corrosion resistant materials*Sample size 60 x 60mm x 25mm high meeting BS 1377*Incorporates PTFE faced box separation screws to reduce friction*Supplied complete with upper and lower porous plates and loading pad*Suitable for quick undrained or drained/residual tests

_Standards_
BS 1377, EN 1997-2, ASTM D3080, AASHTO T236

_Further Information_
All shearbox assemblies are designed to fit the carriage of 26-2114 series Digital Direct/Residual Shear Apparatus. They are supplied complete with three porous plates, one retaining plate and a loading pad. The three sizes supplied comply with the relevant requirements of BS 1377 and ASTM D3080. All assemblies can be used for quick shear tests or drained/residual shear tests.Optional accessories are available including specimen cutters and extrusion tools. 

_Attributes_
Description
	Shear box assembly
	
Specimen size
	60 x 60 mm
	
Sample Size
	60 x 60 mm

_Specification_
Specimen area
	60 x 60 mm
	
Specimen thickness
	25 mm
	
Weight kg
	2
	
Relevant standard
	BS 1377

_Related Products_
Main: 2.42" Diameter Shear Box Assembly (California Type) (26-2223)
Main: Digital Direct/Residual Shear Apparatus Complete with Lever Loading Assembly. 110-120V 50/60Hz 1Ph. (26-2114/02)
Main: Digital Direct/Residual Shear Apparatus Complete with Lever Loading Assembly. 220-240V 50/60Hz 1Ph. (26-2114/01)
Spare/Consumable: Porous Plate 60mm Sq. (26-2181/10)
Accessory: Shear Box Assembly 100mm Sq. (26-2197)
Spare/Consumable: Specimen Cutter 60mm Sq. (26-2185)
Spare/Consumable: Specimen Extrusion Tool 60 mm sq. (26-2189)

[PRODUCT] Shear Box Assembly 2.5 Inch Diameter (26-2213)
*Manufactured from corrosion resistant materials*Sample size 2.5 inch dia x 1 inch hieght meeting ASTM D3080*Incorporates PTFE faced box separation screws to reduce friction*Supplied complete with upper and lower porous plates and loading pad*Suitable for quick undrained or drained/residual tests.

_Standards_
ASTM D3080, AASHTO T236

_Further Information_
All shearbox assemblies are designed to fit the carriage of 26-2114 series Digital Direct/Residual Shear Apparatus. They are supplied complete with three porous plates, one retaining plate and a loading pad. The three sizes supplied comply with the relevant requirements of BS 1377 and ASTM D3080. All assemblies can be used for quick shear tests or drained/residual shear tests.Optional accessories are available including specimen cutters and extrusion tools. 

_Attributes_
Description
	Shear box assembly
	
Specimen size
	2.5" dia
	
Sample Size
	2.5" dia.

_Specification_
Specimen area
	1.5 inch diameter
	
Specimen thickness
	1 inch
	
Weight kg
	2.8
	
Relevant standard
	ASTM D3080

_Related Products_
Main: 2.42" Diameter Shear Box Assembly (California Type) (26-2223)
Main: Digital Direct/Residual Shear Apparatus Complete with Lever Loading Assembly. 110-120V 50/60Hz 1Ph. (26-2114/02)
Main: Digital Direct/Residual Shear Apparatus Complete with Lever Loading Assembly. 220-240V 50/60Hz 1Ph. (26-2114/01)
Spare/Consumable: Porous Plate 2.5 Inch Diameter (26-2213/10)
Spare/Consumable: Specimen Cutter 2.5 Inch Diameter. (26-2217)
Spare/Consumable: Specimen Extrusion Tool 2.5 Inch Diameter. (26-2221)

[PRODUCT] Specimen Extrusion Tool 60 mm sq. (26-2189)

_Standards_
ASTM D3080, AASHTO T236

_Attributes_
Description
	Specimen extrusion tool
	
Specimen size
	60 x 60 mm
	
Sample Size
	60 x 60 mm

_Related Products_
Accessory: Shear Box Assembly 60mm Sq. (26-2181)
Spare/Consumable: Specimen Extrusion Tool 2.5 Inch Diameter. (26-2221)

[PRODUCT] Specimen Extrusion Tool 100 mm sq (26-2205)

_Standards_
ASTM D3080, AASHTO T236

_Attributes_
Description
	Specimen extrusion tool
	
Specimen size
	100 x 100 mm

[PRODUCT] Specimen Extrusion Tool 2.5 Inch Diameter. (26-2221)

_Standards_
ASTM D3080, AASHTO T236

_Attributes_
Description
	Specimen extrusion tool
	
Specimen size
	2.5" dia
	
Sample Size
	2.5" dia.

_Related Products_
Accessory: Shear Box Assembly 2.5 Inch Diameter (26-2213)
Spare/Consumable: Specimen Extrusion Tool 60 mm sq. (26-2189)

[PRODUCT] Porous Plate 60mm Sq. (26-2181/10)

_Standards_
ASTM D3080, AASHTO T236

_Attributes_
Description
	Porous plate
	
Specimen size
	60 x 60 mm
	
Sample Size
	60 x 60 mm

_Related Products_
Spare/Consumable: 2.42" Diameter Porous Stone (26-2223/10)
Spare/Consumable: Porous Plate 2.5 Inch Diameter (26-2213/10)
Accessory: Shear Box Assembly 60mm Sq. (26-2181)

[PRODUCT] Porous Plate 100mm Sq. (26-2197/10)

_Standards_
ASTM D3080, AASHTO T236

_Attributes_
Description
	Porous plate
	
Specimen size
	100 x 100 mm

[PRODUCT] Porous Plate 2.5 Inch Diameter (26-2213/10)

_Standards_
ASTM D3080, AASHTO T236

_Attributes_
Description
	Porous plate
	
Specimen size
	2.5" dia
	
Sample Size
	2.5" dia.

_Related Products_
Spare/Consumable: 2.42" Diameter Porous Stone (26-2223/10)
Spare/Consumable: Porous Plate 60mm Sq. (26-2181/10)
Accessory: Shear Box Assembly 2.5 Inch Diameter (26-2213)

[PRODUCT] Specimen Cutter 60mm Sq. (26-2185)

_Standards_
ASTM D3080, AASHTO T236

_Attributes_
Description
	Specimen cutter
	
Specimen size
	60 x 60 mm
	
Sample Size
	60 x 60 mm

_Related Products_
Accessory: Shear Box Assembly 60mm Sq. (26-2181)
Spare/Consumable: Specimen Cutter 100mmsq. (26-2201)
Spare/Consumable: Specimen Cutter 2.5 Inch Diameter. (26-2217)

[PRODUCT] Specimen Cutter 100mmsq. (26-2201)

_Standards_
ASTM D3080, AASHTO T236

_Attributes_
Description
	Specimen cutter
	
Specimen size
	100 x 100 mm
	
Sample Size
	100 x 100 mm

_Related Products_
Accessory: Shear Box Assembly 100mm Sq. (26-2197)
Spare/Consumable: Specimen Cutter 2.5 Inch Diameter. (26-2217)
Spare/Consumable: Specimen Cutter 60mm Sq. (26-2185)

[PRODUCT] Specimen Cutter 2.5 Inch Diameter. (26-2217)

_Standards_
ASTM D3080, AASHTO T236

_Attributes_
Description
	Specimen cutter
	
Specimen size
	2.5" dia
	
Sample Size
	2.5" dia.

_Related Products_
Accessory: Shear Box Assembly 2.5 Inch Diameter (26-2213)
Spare/Consumable: Specimen Cutter 100mmsq. (26-2201)
Spare/Consumable: Specimen Cutter 60mm Sq. (26-2185)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	Specimen
	N/A for this Product Group

[PRODUCT GROUP] Measurement of Horizontal and Vertical Movement

[PRODUCT] Dial Gauge (83-5456)

_Attributes_
Description
	Dial gauge 10 mm Travel X 0.01 mm
	
Back Type
	A

_Specification_
Diameter mm
	57
	
Travel mm
	10
	
Grad. Mm
	0.01
	
Scale
	RH
	
Anvil
	Ball
	
Back type
	A

[PRODUCT] Dial Gauge 10mm Travel X 0.002mm Divisions. (25-0440)
10 mm x 0.002 mm div.

_Attributes_
Description
	Vertical Dial Indicator, Metric
	
Dial Indicator
	10 mm range x 0.002 mm<br>graduations.

_Related Products_
Main: Digital Direct/Residual Shear Apparatus Complete with Lever Loading Assembly. 110-120V 50/60Hz 1Ph. (26-2114/02)
Main: Digital Direct/Residual Shear Apparatus Complete with Lever Loading Assembly. 220-240V 50/60Hz 1Ph. (26-2114/01)
Accessory: Electronic Digital Indicator, 0.600"/15 mm range (88-4210)
Accessory: Vertical Dial Indicator, English (25-0445)

[PRODUCT] Horizontal Displacement Transducer Assembly 15mm Travel 5 Pin Din Plug Mounting Pillar (27-1697)
*Ideally suited for use with GDU for accuratedisplacement measurements*Models available for use in consolidation, shear, CBR and triaxial test applications*Supplied complete with mounting hardware for specified productsDisplacement Transducers are used in consolidation, shear, CBR and triaxial test applications for accuratevdisplacement measurements. They are supplied complete with a 5-pin DIN type connector for direct connection to the GDU.

_Attributes_
Description
	Horizontal displacement transducer assembly 15 mm travel
	
Mounting Bracket
	Included as standard.

_Specification_
Construction
	Fully encapsulated electronics,sealed in a stainless steel case
	
Excitation
	13 V DC
	
Connector
	5-pin DIN type
	
Mounting bracket
	Included as standard
	
Weight kg
	0.45
	
Construction
	Fully encapsulated electronics, sealed in a stainless steel case.
	
Excitation
	10vDC.
	
Connector
	5-Pin DIN type.
	
Mounting Bracket
	Included as standard.
	
Weight
	Net 1 lb. (0.45 kg).

_Related Products_
Accessory: Axial Strain Transducer Assembly 50mm Travel Fitted with 5 Pin Din Plug. (27-1617)
Main: CBR Displacement Transducer (27-1706)
Main: Consolidation Transducer Assembly 15mm Travel Fitted with 5 Pin Din Plug. (27-1649)
Main: Digital Direct/Residual Shear Apparatus Complete with Lever Loading Assembly. 220-240V 50/60Hz 1Ph. (26-2114/01)
Main: Transducer Extension Cable 3.0 m (27-1717)
Main: Transducer Extension Cable 4.5 m (27-1719)
Accessory: Vertical Displacement Transducer Assembly 15mm Travel with 5 Pin Din Plug Bracket for Shear Box (27-1689)

[PRODUCT] Vertical Displacement Transducer Assembly 15mm Travel with 5 Pin Din Plug Bracket for Shear Box (27-1689)
0 to 10 mm range. For use with Direct/Residual Shear Machines. *Ideally suited for use with GDU for accurate displacement measurements *Models available for use in consolidation, shear, CBR and triaxial test applications*Supplied complete with mounting hardware for specified productsDisplacement Transducers are used in consolidation, shear, CBR and triaxial test applications for accuratevdisplacement measurements. They are supplied complete with a 5-pin DIN type connector for direct connection to the GDU.

_Attributes_
Description
	Vertical displacement transducer assembly 15 mm travel
	
Mounting Bracket
	Included as standard.

_Specification_
Construction
	Fully encapsulated electronics,sealed in a stainless steel case
	
Excitation
	12 V DC
	
Connector
	5-pin DIN type
	
Mounting bracket
	Included as standard
	
Weight kg
	0.45
	
Construction
	Fully encapsulated electronics, sealed in a stainless steel case.
	
Excitation
	10vDC.
	
Connector
	5-Pin DIN type.
	
Mounting Bracket
	Included as standard.
	
Weight
	Net 1 lb. (0.45 kg).

_Related Products_
Accessory: Axial Strain Transducer Assembly 50mm Travel Fitted with 5 Pin Din Plug. (27-1617)
Main: CBR Displacement Transducer (27-1706)
Main: Consolidation Transducer Assembly 15mm Travel Fitted with 5 Pin Din Plug. (27-1649)
Main: Digital Direct/Residual Shear Apparatus Complete with Lever Loading Assembly. 110-120V 50/60Hz 1Ph. (26-2114/02)
Main: Digital Direct/Residual Shear Apparatus Complete with Lever Loading Assembly. 220-240V 50/60Hz 1Ph. (26-2114/01)
Accessory: Horizontal Displacement Transducer Assembly 15mm Travel 5 Pin Din Plug Mounting Pillar (27-1697)
Main: Transducer Extension Cable 3.0 m (27-1717)
Main: Transducer Extension Cable 4.5 m (27-1719)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Measurement of Load (Shear Stress)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	Capacity, kN
	
27-1561
	S-Type load cell
	5
	
78-0060
	Load ring - 2 kN
	2
	
78-0160
	Load ring - 3 kN
	3

[PRODUCT GROUP] Application of Normal Stress

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	Weight, kg
	
26-2132
	Set of weights
	50 kg
	
26-2137
	Slotted surcharge weight
	10 kg
	
26-2139
	Slotted surcharge weight
	5 kg
	
26-2141
	Slotted surcharge weight
	2 kg
	
26-2143
	Slotted surcharge weight
	1 kg
	
26-2145
	Slotted surcharge weight
	0.5 kg
	
26-2147
	Slotted surcharge weight
	0.25 kg

[PRODUCT GROUP] Inspection Vane

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	
26-3335
	H60 Field Inspection Vane Tester
	
26-3335/11
	H605 extension rod

[PRODUCT GROUP] Laboratory Vane Apparatus

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	
26-2270
	Laboratory Vane Apparatus
	
26-2275/10
	Set of 4 calibrated springs (spare)
	
26-2279
	Vane 12.7 mm x 12.7 mm long
	
26-2281
	Vane 12.7 mm dia X 19 mm long
	
26-2283
	Vane 12.7 mm dia x 25.4mm long

[PRODUCT GROUP] Pocket Shearmeter

[PRODUCT] Pocket Shearmeter with 3 Vanes 0 to 1Kgf/Cm2 X 0.5Kgf/Cm2. (26-2261)
The shearmeter can be used on tube samples, on the sides of pits, cuttings etc. It is an invaluable tool for initial site investigation work.

_Further Information_
Complete with sensitive vane, standard vane and high-capacity vane. Range 0 to 1 x 0.05 kgf/cm2.

_Attributes_
Description
	Torvane Shear Device
	
Dial Scale
	1 kg/sq. cm (tons/sq. ft.) x 0.05 subdivisions.

_Specification_
Vane Driver
	1.6â€ (41 mm) diam. x 3.2â€ (81 mm) l. with vaneattached.
	
Dial Scale
	1 kg/sq. cm (tons/sq. ft.) x 0.05 subdivisions.
	
Carrying Case
	Plastic; 6â€ w. x 4â€ d. x 2â€ h. (152 x 102 x 51 mm).
	
Weight
	Net 10.5 oz. (300 g).

_Related Products_
Main: Digital Direct/Residual Shear Apparatus Complete with Lever Loading Assembly. 110-120V 50/60Hz 1Ph. (26-2114/02)
Main: Digital Direct/Residual Shear Apparatus Complete with Lever Loading Assembly. 220-240V 50/60Hz 1Ph. (26-2114/01)
Main: Hand Vane Tester (26-3346)
Spare/Consumable: High-Capacity Vane (26-2261/14)
Spare/Consumable: Sensitive Vane (26-2261/10)
Spare/Consumable: Standard Vane (26-2261/12)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Automatic Data Acquisition

[PRODUCT] GDU 8 Channel Data Acquisition Unit 220-240 V 50/60 Hz, 1 Ph. (27-1500/01)
The GDU is a stand-alone, multi-tasking, multi-channel data logger, that is reliable and powerful, enabling it to co-ordinate test data from the range of ELE transducers required for various test methods.The ELE Geotechnical Software package (DS7.1), in conjunction with the GDU and a range of transducers, are the two central components required to create a modern turnkey soil testing system. Being fully modular it can be adapted to a wide range of soil testing laboratory configurations. * For performing CBR, Consolidation, Direct/Residual Shear and Total & Effective Stress Triaxial tests* 8 Channels expandable to 32 for performing multiple, concurrent tests for cost savings* Independent signal conditioning on each channel to maintain data accuracy* Field-upgradeable software, meaning no downtime for future software and functionality upgrades* Extended warranty.

_Attributes_
Description
	GDU 8 channel data acquisition unit
	
Transducer Supply
	10vDC.
	
Voltage Supply
	220-240 V 50/60 Hz

_Specification_
Case
	Aluminum, free standing; houses power supply, analog to digital conversion module and an 8-channel analog input module with transducer energization.
	
Sockets
	Standard 5-pin DIN type.
	
Input Range
	± 5 volts to ± 10 mV full scale.
	
Transducer Supply
	10vDC.
	
Dimensions
	12.8” w. x 14.3” d. x 6.1” h. (325 x 363 x 155 mm).
	
Weight
	Net 14.08 lbs. (6.4 kg).

_Related Products_
Accessory: 8-Channel Expansion Analog Input Module (27-1505)
Main: GDU 8 Channel Data Acquisition Unit 100-120 V 60 Hz (27-1500/02)
Accessory: USB to Serial Adapter (27-1701)

[PRODUCT] DS7.2 Direct and Residual Shear Strength Program for Windows 7, 32/64 bit (27-1793)
This unique package provides test options for quick undrained or drained shear tests with the user selectable option of residual testing. Individual test results can be linked together to produce the Coulomb Envelope. Printouts and plots are available for sample description and basic test data such as moisture content, etc. Realtime plots of settlement, shear versus displacement and vertical displacement during shearing is readily available via the PC screen or printer.

_Attributes_
Description
	DS7.2 Direct and Residual Shear Strength Program
	
GDU Compatability
	Yes
	
DSU Compatability
	Yes

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[CATEGORY] Data Logging, Software and Electronic Instrumentation
At ELE we have long specialised in the development of intelligent processing and recording systems. Over the years, our knowledge, skills and resources have enabled us to help customers move from the early stages of simple digital readout units, through dedicated computer control, to the latest intelligent stand-alone data acquisition systems.In each case our expertise in both hardware and software allows us to deliver dedicated condition monitoring and software solutions that meet the exact needs of our customers, while retaining optimum system performance, functionality and reliability.  	* Multi-tasking 	* Stand-alone systems 	* Digital readout units 	* Total solutions 	* Systems consultancy service 	* Wide range of PC compatibility

[PRODUCT GROUP] Data Logging with the DSU

[PRODUCT] DSU Electronic Readout and Control System 110 V AC 60 Hz (27-1300/02)
· Download the full brochure here [/Page/catalogue-download/NTRmZS9UaGUgTkVXIERTVSBVU0EucGRm] · Download the full DS7.2 geotechnical software brochure here [/Page/catalogue-download/NTRmZS9OZXcgRFM3IFNvZnR3YXJlIFVTQTY5LnBkZg==] · 4 channel automatic control and data-logging unit · Automatic, dual-frame control · Performs CBR, Marshall, Unconfined Compression, Direct and Residual Shear, One-Dimensional Consolidation, Unconfined Undrained, Consolidated Drained and Unconsolidated Drained tests · LAN connection - software can be running anywhere on your server · Never lose data from power fails - 2 gigabytes of non-volatile memory The Data System Unit (DSU) is a versatile instrument designed to accomodate the general logging requirements of geotechnical and materials testing engineers. Its intelligent interface allows the user to work with a range of different sensors.

_Further Information_
Become a member of the ELE International web site, add this new product to a wishlist to receive a quote! Click here [/Login] This product is now available in the USA and Canada!

_Attributes_
Description
	DSU
	
Voltage Supply
	100-120 V 60 Hz

_Related Products_
Accessory: Cable, Safety/ID (27-1300/11)
Main: DSU Electronic Readout and Control System 220 - 240 V AC 50/60 Hz (27-1300/01)
Accessory: Dual Frame Comms Cable (27-1300/10)
Accessory: PC Cable (27-1300/12)

[PRODUCT] DSU Electronic Readout and Control System 220 - 240 V AC 50/60 Hz (27-1300/01)
· Download the full brochure here [/../../../Page/the-new-dsu] · 4 channel automatic control and data-logging unit · Automatic, dual-frame control · Performs CBR, Marshall, Unconfined Compression, Direct and Residual Shear, One-Dimensional Consolidation, Unconfined Undrained, Consolidated Drained and Unconsolidated Drained tests · LAN connection - software can be running anywhere on your server · Never lose data from power fails - 2 gigabytes of non-volatile memory · Extended warranty The Data System Unit (DSU) is a versatile instrument designed to accomodate the general logging requirements of geotechnical and materials testing engineers. Its intelligent interface allows the user to work with a range of different sensors.

_Further Information_
Become a member of the ELE International web site, add this new product to a wishlist to receive a quote! Click here [/../../../Login] Please note that this product is not yet available in the USA, we will let you know as soon as it is ready!

_Attributes_
Voltage Supply
	220-240 V 50/60 Hz
	
Description
	DSU

_Related Products_
Accessory: Cable, Safety/ID (27-1300/11)
Main: DSU Electronic Readout and Control System 110 V AC 60 Hz (27-1300/02)
Accessory: Dual Frame Comms Cable (27-1300/10)
Accessory: PC Cable (27-1300/12)

[PRODUCT] Dual Frame Comms Cable (27-1300/10)
This item is required if you wish to control two Multiplex 50 [/../../../Product/multiplex-50-load-frame] frames for CBR and Marshall tests

_Attributes_
Description
	Dual Frame Comms Cable
	
Voltage Supply
	n/a

_Related Products_
Accessory: Cable, Safety/ID (27-1300/11)
Main: DSU Electronic Readout and Control System 110 V AC 60 Hz (27-1300/02)
Main: DSU Electronic Readout and Control System 220 - 240 V AC 50/60 Hz (27-1300/01)
Accessory: PC Cable (27-1300/12)

[PRODUCT] Cable, Safety/ID (27-1300/11)
This is required for every CBR Test 50, Marshall Test 50 and Multplex 50 load frame that you wish to control. Please note, one of these is included with the DSU as standard. An additional will be required if you wish to connect to a second frame.

_Attributes_
Description
	Cable, Safety/ID
	
Voltage Supply
	n/a

_Related Products_
Main: DSU Electronic Readout and Control System 110 V AC 60 Hz (27-1300/02)
Main: DSU Electronic Readout and Control System 220 - 240 V AC 50/60 Hz (27-1300/01)
Accessory: Dual Frame Comms Cable (27-1300/10)
Accessory: PC Cable (27-1300/12)

[PRODUCT] PC Cable (27-1300/12)
This item is required to connect the Multiplex frame or a link to the PC when using the DSU with DS7.2.

_Attributes_
Description
	PC Cable
	
Voltage Supply
	n/a

_Related Products_
Accessory: Cable, Safety/ID (27-1300/11)
Main: DSU Electronic Readout and Control System 110 V AC 60 Hz (27-1300/02)
Main: DSU Electronic Readout and Control System 220 - 240 V AC 50/60 Hz (27-1300/01)
Accessory: Dual Frame Comms Cable (27-1300/10)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	Voltage
	N/A for this Product Group

[PRODUCT GROUP] Data Logging with the GDU

[PRODUCT] GDU 8 Channel Data Acquisition Unit 220-240 V 50/60 Hz, 1 Ph. (27-1500/01)
The GDU is a stand-alone, multi-tasking, multi-channel data logger, that is reliable and powerful, enabling it to co-ordinate test data from the range of ELE transducers required for various test methods.The ELE Geotechnical Software package (DS7.1), in conjunction with the GDU and a range of transducers, are the two central components required to create a modern turnkey soil testing system. Being fully modular it can be adapted to a wide range of soil testing laboratory configurations. * For performing CBR, Consolidation, Direct/Residual Shear and Total & Effective Stress Triaxial tests* 8 Channels expandable to 32 for performing multiple, concurrent tests for cost savings* Independent signal conditioning on each channel to maintain data accuracy* Field-upgradeable software, meaning no downtime for future software and functionality upgrades* Extended warranty.

_Attributes_
Description
	GDU 8 channel data acquisition unit
	
Transducer Supply
	10vDC.
	
Voltage Supply
	220-240 V 50/60 Hz

_Specification_
Case
	Aluminum, free standing; houses power supply, analog to digital conversion module and an 8-channel analog input module with transducer energization.
	
Sockets
	Standard 5-pin DIN type.
	
Input Range
	± 5 volts to ± 10 mV full scale.
	
Transducer Supply
	10vDC.
	
Dimensions
	12.8” w. x 14.3” d. x 6.1” h. (325 x 363 x 155 mm).
	
Weight
	Net 14.08 lbs. (6.4 kg).

_Related Products_
Accessory: 8-Channel Expansion Analog Input Module (27-1505)
Main: GDU 8 Channel Data Acquisition Unit 100-120 V 60 Hz (27-1500/02)
Accessory: USB to Serial Adapter (27-1701)

[PRODUCT] GDU 8 Channel Data Acquisition Unit 100-120 V 60 Hz (27-1500/02)
The GDU is a stand-alone, multi-tasking, multi-channel data logger, that is reliable and powerful, enabling it to co-ordinate test data from the range of ELE transducers required for various test methods.The ELE Geotechnical Software package (DS7.1), in conjunction with the GDU and a range of transducers, are the two central components required to create a modern turnkey soil testing system. Being fully modular it can be adapted to a wide range of soil testing laboratory configurations. * For performing CBR, Consolidation, Direct/Residual Shear and Total & Effective Stress Triaxial tests* 8 Channels expandable to 32 for performing multiple, concurrent tests for cost savings* Independent signal conditioning on each channel to maintain data accuracy* Field-upgradeable software, meaning no downtime for future software and functionality upgrades* Extended warranty

_Attributes_
Voltage Supply
	100-120 V 60 Hz
	
Description
	GDU 8 channel data acquisition unit
	
Transducer Supply
	10vDC.

_Specification_
Case
	Aluminum, free standing; houses power supply, analog to digital conversion module and an 8-channel analog input module with transducer energization.
	
Sockets
	Standard 5-pin DIN type.
	
Input Range
	± 5 volts to ± 10 mV full scale.
	
Transducer Supply
	10vDC.
	
Dimensions
	12.8” w. x 14.3” d. x 6.1” h. (325 x 363 x 155 mm).
	
Weight
	Net 14.08 lbs. (6.4 kg).

_Related Products_
Accessory: 8-Channel Expansion Analog Input Module (27-1505)
Main: GDU 8 Channel Data Acquisition Unit 220-240 V 50/60 Hz, 1 Ph. (27-1500/01)
Accessory: USB to Serial Adapter (27-1701)

[GROUPED PRODUCT MATRIX]
Model No.
	Voltage
	Desc
	N/A for this Product Group

[CATEGORY] Instrumentation for Triaxial testing

[PRODUCT GROUP] Axial Displacement

[PRODUCT] Axial Strain Transducer Assembly 50mm Travel Fitted with 5 Pin Din Plug. (27-1617)
0 to 50 mm range. For use with Triaxial Cells. *Ideally suited for use with GDU for accuratedisplacement measurements*Models available for use in consolidation, shear,CBR and triaxial test applications*Supplied complete with mounting hardware forspecified productsDisplacement Transducers are used in consolidation, shear, CBR and triaxial test applications for accuratevdisplacement measurements. They are supplied complete with a 5-pin DIN type connector for direct connection to the GDU.

_Attributes_
Description
	Axial strain transducer assembly 50mm travel
	
Mounting Bracket
	Included as standard.

_Specification_
Construction
	Fully encapsulated electronics,sealed in a stainless steel case
	
Excitation
	10 V DC
	
Connector
	5-pin DIN type
	
Mounting bracket
	Included as standard
	
Weight kg
	0.45
	
Construction
	Fully encapsulated electronics, sealed in a stainless steel case.
	
Excitation
	10vDC.
	
Connector
	5-Pin DIN type.
	
Mounting Bracket
	Included as standard.
	
Weight
	Net 1 lb. (0.45 kg).

_Related Products_
Main: CBR Displacement Transducer (27-1706)
Main: Consolidation Transducer Assembly 15mm Travel Fitted with 5 Pin Din Plug. (27-1649)
Main: Dial Gauge 25mm Travel X 0.01mm Divisions (25-4210)
Accessory: Horizontal Displacement Transducer Assembly 15mm Travel 5 Pin Din Plug Mounting Pillar (27-1697)
Main: Transducer Extension Cable 3.0 m (27-1717)
Main: Transducer Extension Cable 4.5 m (27-1719)
Accessory: Vertical Displacement Transducer Assembly 15mm Travel with 5 Pin Din Plug Bracket for Shear Box (27-1689)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Load Measurement

[PRODUCT] Distance Piece Stainless Steel for Use with Submerisble Load Cells and Axial Strain Transducers. (27-1293)
Required when using submersible load cells.

_Attributes_
Description
	Distance piece stainless steel for use with submersible load cells
	
Load device type
	Stainless Steel distance piece for use with submersible loads cells
	
Weight, lbs
	1

_Related Products_
Accessory: Submersible Load Transducer Assembly 10kN Capacity In Compression. (27-1575)
Accessory: Submersible Load Transducer Assembly 5kN Capacity In Compression. (27-1573)
Main: Transducer Extension Cable 3.0 m (27-1717)
Main: Transducer Extension Cable 4.5 m (27-1719)

[PRODUCT] S-Type Load Cell 5 kN.for Triaxial Tests. Fitted with 5 Pin Din Plug. (27-1551)
*Repeatability better than ± 0.02% of rated output*Non-Linearity better than ± 0.03% of rated output*Supplied complete with 5-pin DIN type connector for connection to GDUIdeally suited for a wide range of applications, ELE S-type load cells provide high accuracy and minimum deformation. Various models are available, with the necessary adaptors, for use with ELE Triaxial Load Frames, Multiplex 50/Marshall Test 50/CBR Test 50 and Direct Shear machine.

_Attributes_
Load device type
	S-Type
	
Force Capacity, kN
	5
	
Description
	S-Type load cell
	
Environmental Protection
	IP65

_Related Products_
Main: Digital Direct/Residual Shear Apparatus Complete with Lever Loading Assembly. 110-120V 50/60Hz 1Ph. (26-2114/02)
Main: Digital Direct/Residual Shear Apparatus Complete with Lever Loading Assembly. 220-240V 50/60Hz 1Ph. (26-2114/01)

[PRODUCT] S-Type Load Cell 10 kN.for Triaxial Tests. Fitted with 5 Pin Din Plug. (27-1553)
*Repeatability better than ± 0.02% of rated output*Non-Linearity better than ± 0.03% of rated output*Supplied complete with 5-pin DIN type connector for connection to GDUIdeally suited for a wide range of applications, ELE S-type load cells provide high accuracy and minimum deformation. Various models are available, with the necessary adaptors, for use with ELE Triaxial Load Frames, Multiplex 50/Marshall Test 50/CBR Test 50 and Direct Shear machine.

_Attributes_
Load device type
	S-Type
	
Force Capacity, kN
	10
	
Description
	S-Type load cell
	
Environmental Protection
	IP65

[PRODUCT] S-Type Load Cell 25 kN.for Triaxial Tests. 27-1293 required separately. (27-1555)
*Repeatability better than ± 0.02% of rated output*Non-Linearity better than ± 0.03% of rated output*Supplied complete with 5-pin DIN type connector for connection to GDUIdeally suited for a wide range of applications, ELE S-type load cells provide high accuracy and minimum deformation. Various models are available, with the necessary adaptors, for use with ELE Triaxial Load Frames, Multiplex 50/Marshall Test 50/CBR Test 50 and Direct Shear machine.

_Attributes_
Load device type
	S-Type
	
Force Capacity, kN
	25
	
Description
	S-Type load cell
	
Environmental Protection
	IP65

[PRODUCT] Submersible Load Transducer Assembly 5kN Capacity In Compression. (27-1573)
*Eliminates effects of piston friction on readings*Unaffected by cell confining pressures*Easily installed in triaxial cell*Supplied complete with calibration certificate and 5-pin DIN type connector for use with GDUSubmersible Load Transducers are used to measure accurately the axial loads applied to triaxial test specimens. Consisting of a load cell and piston assembly these units replace the standard triaxial cell loading piston. A major advantage is that these transducers measure loads directly on top of the specimen. All transducers are supplied complete with a 5-pin DIN type connector and calibration certificate.

_Attributes_
Load device type
	Submersible
	
Force Capacity, kN
	5
	
Description
	Submersible load transducer
	
Weight, lbs
	2.25

_Specification_
Dimensions
	75 x 50 mm (dia x h) excluding piston and adaptor
	
Overload capacity
	150%
	
Output
	26 mv full range
	
Excitation
	10 V DC (15 V DC max)
	
Non-linearity
	0.1% maximum
	
Hysteresis Deflection
	0.1% maximum 0.05 mm at full load
	
Side force
	50% full scale maximum without effect
	
Connector
	5-pin DIN plug
	
Compensated temperature range
	0 to 50°C
	
Weight g
	850

_Related Products_
Accessory: Distance Piece Stainless Steel for Use with Submerisble Load Cells and Axial Strain Transducers. (27-1293)
Main: S-Type Load Cell 10,000 lb Capacity (27-1587)
Main: S-Type Load Cell 2,000 lb Capacity (27-1583)
Main: S-Type Load Cell 500 lb Capacity (27-1581)
Main: Transducer Extension Cable 3.0 m (27-1717)
Main: Transducer Extension Cable 4.5 m (27-1719)

[PRODUCT] Submersible Load Transducer Assembly 10kN Capacity In Compression. (27-1575)
*Eliminates effects of piston friction on readings*Unaffected by cell confining pressures*Easily installed in triaxial cell*Supplied complete with calibration certificate and 5-pin DIN type connector for use with GDUSubmersible Load Transducers are used to measure accurately the axial loads applied to triaxial test specimens. Consisting of a load cell and piston assembly these units replace the standard triaxial cell loading piston. A major advantage is that these transducers measure loads directly on top of the specimen. All transducers are supplied complete with a 5-pin DIN type connector and calibration certificate.

_Attributes_
Load device type
	Submersible
	
Force Capacity, kN
	10
	
Description
	Submersible load transducer
	
Compensated Temperature Range
	0 - 50

_Specification_
Dimensions
	76 x 50 mm (dia x h) excluding piston and adaptor
	
Overload capacity
	150%
	
Output
	27 mv full range
	
Excitation
	11 V DC (15 V DC max)
	
Non-linearity
	0.1% maximum
	
Hysteresis Deflection
	0.1% maximum 0.05 mm at full load
	
Side force
	50% full scale maximum without effect
	
Connector
	5-pin DIN plug
	
Compensated temperature range
	1 to 50°C
	
Weight g
	850

_Related Products_
Accessory: Distance Piece Stainless Steel for Use with Submerisble Load Cells and Axial Strain Transducers. (27-1293)

[PRODUCT] Clamped Boss Load Ring - 4.5 kN (78-0260)

_Attributes_
Description
	Load ring - 4.5 kN
	
Load device type
	Load ring
	
Force Capacity, kN
	4.5
	
Weight, lbs
	9.25

_Specification_
Capacity: kN, kgf, lbf
	4.5, 450, 1000
	
Typical Design sensitivity: N/div, kgf/div, lbf/div
	3.0, 0.30, 0.66
	
Overall height mm
	248
	
Approx weight kg
	3.5
	
Capacity - lbf
	1,000
	
Capacity - kN
	4.5
	
Capacity - kgf
	450
	
Typical Design Sensitivity - lbf/div
	0.66
	
Typical Design Sensitivity - kN/div
	3
	
Typical Design Sensitivity - Kgf/div
	0.3
	
Overall Height
	9.76” (248 mm)
	
Approx Weight
	7.7 lbs.(3.5 kg)

_Related Products_
Accessory: 50kN Load Measuring Ring (78-0860)
Accessory: Clamped Boss Load Ring - 10.0 kN (78-0460)
Accessory: Clamped Boss Load Ring - 2.0 kN (78-0060)
Accessory: Clamped Boss Load Ring - 28.0 kN (78-0760)
Accessory: Clamped Boss Load Ring - 3.0 kN (78-0160)
Main: Digital Direct/Residual Shear Apparatus Complete with Lever Loading Assembly. 110-120V 50/60Hz 1Ph. (26-2114/02)
Main: Digital Direct/Residual Shear Apparatus Complete with Lever Loading Assembly. 220-240V 50/60Hz 1Ph. (26-2114/01)
Accessory: Digital Proving Ring, 1,000 lbs (4.5 kN) (78-0264)
Main: Digital Tritest 50 (25-3518/01)
Main: Digital Tritest 50 Load Frame 110-120vAC (25-3518/02)
Main: MultiPlex 50 Load Frame (25-3700/01)
Spare/Consumable: Spare Dial Indicator for Load Rings (78-5461)
Main: Versa-Loader (25-3525/02)

[PRODUCT] Clamped Boss Load Ring - 28.0 kN (78-0760)

_Attributes_
Description
	Load ring - 28 kN
	
Load device type
	Load ring
	
Force Capacity, kN
	28
	
Value of CBR %
	Average range of CBR
	
Overall Height, mm
	248

_Specification_
Capacity: kN, kgf, lbf
	28.0, 2800, 6000
	
Typical Design sensitivity: N/div, kgf/div, lbf/div
	25.5, 2.54, 5.45
	
Overall height mm
	248
	
Approx weight kg
	5.4
	
Capacity
	28 kN
	
Value of CBR
	Average range of CBR
	
Capacity - lbf
	6,000
	
Capacity - kN
	28
	
Capacity - kgf
	2,800
	
Typical Design Sensitivity - lbf/div
	5.45
	
Typical Design Sensitivity - kN/div
	25.5
	
Typical Design Sensitivity - Kgf/div
	2.54
	
Overall Height
	9.76” (248 mm)
	
Approx Weight
	11 .9 lbs.(5.4 kg)

_Related Products_
Accessory: 50kN Load Measuring Ring (78-0860)
Main: CBR Loading Press, Hand-Operated (24-9345)
Main: CBR-Test 50 Machine 50 kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/02)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/01)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/06)
Accessory: Clamped Boss Load Ring - 10.0 kN (78-0460)
Accessory: Clamped Boss Load Ring - 2.0 kN (78-0060)
Accessory: Clamped Boss Load Ring - 3.0 kN (78-0160)
Accessory: Clamped Boss Load Ring - 4.5 kN (78-0260)
Main: Conversion Frame. (24-9341)
Accessory: Digital Proving Ring, 6,000 lbs (28.0 kN) (78-0764)
Main: Digital Tritest 50 (25-3518/01)
Main: Digital Tritest 50 Load Frame 110-120vAC (25-3518/02)
Main: MultiPlex 50 Load Frame (25-3700/01)
Spare/Consumable: Spare Dial Indicator for Load Rings (78-5461)
Main: Versa-Loader (25-3525/02)

[PRODUCT] 50kN Load Measuring Ring (78-0860)
Calibrated in compression.

_Standards_
EN 12697-34

_Attributes_
Description
	Load ring - 50 kN
	
Value of CBR %
	Above 40%
	
Overall Height, mm
	248
	
Force Capacity, kN
	50
	
Load device type
	Load ring

_Specification_
Capacity: kN, kgf, lbf
	50.0, 5000, 11,200
	
Typical Design sensitivity: N/div, kgf/div, lbf/div
	45.5, 4.54, 10.18
	
Overall height mm
	248
	
Approx weight kg
	7.9
	
Capacity
	50 kN
	
Value of CBR
	Above 40%
	
Capacity - lbf
	11,200
	
Capacity - kN
	50
	
Capacity - kgf
	5,000
	
Typical Design Sensitivity - lbf/div
	10.18
	
Typical Design Sensitivity - kN/div
	45.5
	
Typical Design Sensitivity - Kgf/div
	4.54
	
Overall Height
	9.76” (248 mm)
	
Approx Weight
	17.4 lbs.(7.9 kg)

_Related Products_
Main: CBR Loading Press, Hand-Operated (24-9345)
Main: CBR-Test 50 Machine 50 kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/02)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/01)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/06)
Accessory: Clamped Boss Load Ring - 10.0 kN (78-0460)
Accessory: Clamped Boss Load Ring - 2.0 kN (78-0060)
Accessory: Clamped Boss Load Ring - 28.0 kN (78-0760)
Accessory: Clamped Boss Load Ring - 3.0 kN (78-0160)
Accessory: Clamped Boss Load Ring - 4.5 kN (78-0260)
Accessory: Digital Proving Ring, 11,200 lbs (50.0 kN) (78-0864)
Main: Digital Tritest 50 (25-3518/01)
Main: Digital Tritest 50 Load Frame 110-120vAC (25-3518/02)
Main: Marshall Test 50 (45-6810/01)
Main: MultiPlex 50 Load Frame (25-3700/01)
Spare/Consumable: Spare Dial Indicator for Load Rings (78-5461)
Main: Versa-Loader (25-3525/02)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	Capacity, kN
	N/A for this Product Group

[PRODUCT GROUP] Pressure Measurement

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	
27-1620
	Digital pressure gauge
	
27-1633
	Pressure transducer

[PRODUCT GROUP] Volume Change Measurement

[PRODUCT] Volume Change Transducer Assembly 80Cm3 Capacity Maximum Working Pressure 1700Kpa (27-1641)
*Reversing valves to increase capacity*Steel case for wall mounting and access to piping*Supplied complete with calibration certificateThe Volume Change Transducer provides continuous measurements of volume change during the triaxial test. The assembly includes a valve to reverse the flow through the unit, providing increased capacity.

_Attributes_
Description
	Volume change transducer assembly
	
Maximum Pressure, psi
	250

_Specification_
Overall dimensions (l x w x h)
	178 x 229 x 368 mm
	
Maximum pressure
	1700 kPa
	
Excitation
	10 V DC
	
Output
	1.25 full range
	
Capacity
	80 ml
	
Connector
	5-pin DIN type
	
Weight kg
	4.5
	
Maximum Pressure
	250 psi (1,700 kPa).
	
Excitation
	10vDC.
	
Output
	1.25 Volts full range.
	
Capacity
	80 cc x 0.1 cc sensitivity.
	
Case
	Steel; hinged for access to piping.
	
Connector
	5-Pin DIN type.
	
Overall Dimensions
	9” w. x 7” d. x 14 -1/2” h. (22 9 x 178 x 368 mm).
	
Weight
	Net 10 lbs. (4.5 kg).
	
Maximum Pressure
	250 psi (1,700 kPa).
	
Excitation
	10vDC.
	
Output
	1.25 Volts full range.
	
Capacity
	80 cc x 0.1 cc sensitivity.
	
Case
	Steel; hinged for access to piping.
	
Connector
	5-Pin DIN type.
	
Overall Dimensions
	9” w. x 7” d. x 14 -1/2” h. (22 9 x 178 x 368 mm).
	
Weight
	Net 10 lbs. (4.5 kg).

_Related Products_
Main: Transducer Extension Cable 3.0 m (27-1717)
Main: Transducer Extension Cable 4.5 m (27-1719)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[CATEGORY] Instrumentation for Direct and Residual Shear Testing

[PRODUCT GROUP] Displacement Measurement

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	
27-1689
	Vertical displacement transducer assembly 15 mm travel
	
27-1697
	Horizontal displacement transducer assembly 15 mm travel

[PRODUCT GROUP] Load Measurement

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	Capacity, kN
	
27-1561
	S-Type load cell
	5
	
78-0260
	Load ring - 4.5 kN
	4.5

[CATEGORY] Instrumentation for Consolidation Testing

[PRODUCT GROUP] Displacement Measurement

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	
27-1649
	Displacement tranducer

[CATEGORY] Instrumentation for CBR testing

[PRODUCT GROUP] Load Measurement

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	Capacity, kN
	
27-1559
	S-type load cell - 50 kN
	50

[PRODUCT GROUP] Penetration Measurement

[PRODUCT] CBR Penetration Transducer 50mm Travel Fitted with 5 Pin Din Plug. (27-1705)
* Ideally suited for use with GDU for accurate displacement measurements* Models available for use in consolidation, shear, CBR and triaxial test applications* Supplied complete with mounting hardware for specified productsDisplacement Transducers are used in consolidation, shear, CBR and triaxial test applications for accuratevdisplacement measurements. They are supplied complete with a 5-pin DIN type connector for direct connection to the GDU.

_Attributes_
Description
	Penetration transducer
	
Mounting Bracket
	Included

_Specification_
Construction
	Fully encapsulated electronics,sealed in a stainless steel case
	
Excitation
	14 V DC
	
Connector
	5-pin DIN type
	
Mounting bracket
	Included as standard
	
Weight kg
	0.45

_Related Products_
Main: CBR-Test 50 Machine 50 kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/02)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/06)
Main: Cbr-Test 50 Machine 50kN Capacity BS and ASTM Supplied with Stabilising Bar. (24-9150/01)
Main: MultiPlex 50 Load Frame (25-3700/01)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[CATEGORY] Accessories for transducers

[PRODUCT GROUP] Extension cables

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	
27-1715
	Transducer extension cable 1.5 m
	
27-1717
	Transducer extension cable 3.0 m
	
27-1719
	Transducer extension cable 4.5 m

[CATEGORY] Geotechnical Testing Software

[PRODUCT GROUP] DS7
ELE International is pleased to present a NEW version of its geotechnical data acquisition and analysis testing software, DS7 (DataSystem 7), compatible with Microsoft Windows 7.* Now supports Ethernet comminucations in conjunction with the DSU [/../../../Product/dsu-220v]* Programs available for Triaxial, Permeability Consolidation, Direct/Residual Shear and CBR tests* Full support for Windows XP/7 and MS Word 2007/2010* Accurate and repeatable test procedures* 24 hour unsupervised logging* Eliminate the possibility of errors while taking manual readings* Tests are run with step-by-step instructions selectable between BS and ASTM/AASHTO standards* Automatic report generation in accordance with the above standards* Real-time graphical outputs to both screen and printer as required

[PRODUCT] DS7.2 California Bearing Ratio (CBR) Penetration Program for Windows 7, 32/64 bit (27-1798)
This program provides the classical data for the CBR test. Load and penetration are monitored simultaneously. The program tabulates the results and provides a graphical presentation report.

_Attributes_
Description
	DS7.2 California Bearing Ratio (CBR) Penetration Program
	
GDU Compatability
	Yes
	
DSU Compatability
	Yes

[PRODUCT] DS7.2 Software-UU/CU/CD Triaxial, Permeability, Consolidation, Direct/Residual Shear, CBR (S1160)
 	* Programs available for Triaxial, Permeability Consolidation, Direct/Residual Shear and CBR tests 	* Full support for Windows 7 and MS Word 2007/2010 	* Accurate and repeatable test procedures 	* 24 hour unsupervised logging 	* Eliminate the possibility of errors while taking manual readings 	* Tests are run with step-by-step instructions selectable between BS and ASTM/AASHTO standards 	* Automatic report generation in accordance with the above standards 	* Real-time graphical outputs to both screen and printer as required

_Attributes_
Description
	DS7.2 Complete Software Suite
	
GDU Compatability
	Yes
	
DSU Compatability
	No

[PRODUCT] DS7.2 Undrained Triaxial Shear Strength Program for Windows 7, 32/64 bit (27-1753)
* Options for single or multi-stage testing on a sample* Mohr circles produced for graphical analysisOptions are available for a single test on one sample, standard three-sample procedure with linking of the results, or for a multi-stage test on one sample. Load and strain are monitored through transducers. Various printouts and graphical plots are available including basic sample data, moisture content and density. The program tabulates shearing data and plots stress against strain. Mohr circles are produced for graphical analyses.

_Attributes_
Description
	DS7.2 Undrained Triaxial Shear Strength
	
GDU Compatability
	Yes
	
DSU Compatability
	Yes

[PRODUCT] DS7.2 CU/CD Triaxial Shear Strength Program for Windows 7, 32/64 bit (27-1763)
* Complete package for consolidated drained and consolidated undrained triaxial testsThis advanced package includes procedures for consolidated drained and consolidated undrained tests. Standard options are available for saturation, consolidation and shearing with automatic monitoring of the various parameters through transducers linked to the system. Load, strain, volume-change, pore-pressure, cell pressure and back pressure can all be monitored. Various prints and graphical plots are available to the engineer and include saturation data such as pore pressure build-up and B values, consolidation, volume change against time, shearing load versus strain with pore pressure monitoring.

_Attributes_
Description
	DS7.2 CU/CD Triaxial Shear Strength Program
	
GDU Compatability
	Yes
	
DSU Compatability
	No

[PRODUCT] DS7.2 Permeability in a Triaxial Cell Program for Windows 7, 32/64 bit (27-1768)
This program provides data for the determination of permeability of soil specimens using a triaxial cell and two volume change units in accordance with BS 1377.

_Attributes_
Description
	DS7.2 Permeability in a Triaxial Cell Program
	
GDU Compatability
	Yes
	
DSU Compatability
	No

[PRODUCT] DS7.2 One-Dimensional Consolidation Program for Windows 7, 32/64 bit (27-1773)
DS7.1 Consolidation Software provides all basic functions needed to record and analyse consolidation test data. Options are available for monitoring settlement on a log time or square-root time basis. Printouts and graphical plots are available for all stages including Mv and Cv moisture content, voids ratio plots, and initial sample conditions.

_Attributes_
Description
	DS7.2 One-Dimensional Consolidation Program
	
GDU Compatability
	Yes
	
DSU Compatability
	Yes

[PRODUCT] DS7.2 Direct and Residual Shear Strength Program for Windows 7, 32/64 bit (27-1793)
This unique package provides test options for quick undrained or drained shear tests with the user selectable option of residual testing. Individual test results can be linked together to produce the Coulomb Envelope. Printouts and plots are available for sample description and basic test data such as moisture content, etc. Realtime plots of settlement, shear versus displacement and vertical displacement during shearing is readily available via the PC screen or printer.

_Attributes_
Description
	DS7.2 Direct and Residual Shear Strength Program
	
GDU Compatability
	Yes
	
DSU Compatability
	Yes

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	GDU
	DSU
	N/A for this Product Group

[CATEGORY] Bearing Capacity
The design of foundations is a prerequisite of economic design and construction. In order to guard against shear failure and unacceptable ground movements due to loading it is often necessary to determine the ground bearing capacity.

[PRODUCT GROUP] In-situ Testing

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	
29-3720
	Dynamic Cone Penetrometer
	
29-3720/10
	Spare Cone for Dynamic Cone Penetrometer
	
29-3729
	Pocket Penetrometer
	
29-3800
	Plate Bearing Apparatus

[CATEGORY] In-situ Density
Many civil engineering projects require the use of fill material. Whenever soil is placed as an engineering fill, it is usually compacted to a dense state, to obtain satisfactory engineering properties. Compaction on site is is usually effected by mechanical means such as rolling, ramming or vibrating. Control of compaction is necessary to achieve a satisfactory result at a reasonable cost. Laboratory compaction tests provide the basis for control procedures used on site.

[PRODUCT GROUP] Proctor Penetrometer
This spring-type penetrometer can be used in the field to control soil compaction. The stem is calibrated to 150 lbf x 2 lbf divisions, and a sliding collar indicates the applied load. A rapid estimate of the moisture content of soil can be obtained by comparing the amount of penetration of the needle for a corresponding load, with a laboratory determined moisture/density curve for a similar soil.

[PRODUCT] Case for Proctor Penetrometer. (29-3933)
An optional carrying case for the penetrometer and needle points.

_Standards_
ASTM D1558

_Attributes_
Description
	Case for Proctor Penetrometer

_Related Products_
Main: Proctor Penetrometer Spring Type with Adaptor Stem.Supplied Complete with Set of Needle Points (29-3925)

[PRODUCT] Proctor Penetrometer Spring Type with Adaptor Stem.Supplied Complete with Set of Needle Points (29-3925)
Supplied without needle points

_Standards_
ASTM D1558

_Further Information_
**NOT AVAILABLE FOR SALE IN THE USA**

_Attributes_
Description
	Proctor Penetrometer - complete with set of needle points
	
Weight, kg
	2

_Related Products_
Accessory: Case for Proctor Penetrometer. (29-3933)
Accessory: Set of Needle Points 1 1/2 1/4 1/10 1/20 1/40 Inch Sq. (34-0810)
Accessory: Syringe with Rubber Bulb. (82-2820)

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group

[PRODUCT GROUP] Sand Replacement
This equipment is used to determine the dry density of insitu soils. Apparatus is included which satisfies BS, ASTM and AASHTO specifications.

[PRODUCT] 100mm Sand Pouring Cylinder. (29-4000)

_Standards_
BS 1377, BS 1924

_Attributes_
Description
	Sand Pouring Cylinder
	
Diameter, mm
	100 mm
	
Weight, kg
	3

[PRODUCT] 150mm Sand Pouring Cylinder. (29-4100)

_Standards_
BS 1377, BS 1924

_Attributes_
Description
	Sand Pouring Cylinder
	
Diameter, mm
	150 mm
	
Weight, kg
	7.5

[PRODUCT] 200mm Sand Pouring Cylinder. (29-4200)

_Standards_
BS 1377, BS 1924

_Attributes_
Description
	Sand Pouring Cylinder
	
Diameter, mm
	200 mm
	
Weight, kg
	16

[PRODUCT] Metal Tray 300mm Sq. X 40mm Deep with A 100mm Dia Hole. (29-4040)

_Standards_
BS 1377, BS 1924

_Attributes_
Description
	Metal Tray
	
Diameter, mm
	100 mm
	
Internal diameter mm
	100

[PRODUCT] Metal Tray 300mm Sq X 40mm Deep with A 150mm Dia Hole. (29-4140)

_Standards_
BS 1377, BS 1924

_Attributes_
Description
	Metal Tray
	
Diameter, mm
	150 mm
	
Internal diameter mm
	150

[PRODUCT] Metal Tray 500mm Sq X 50mm Deep with A 200mm Dia Hole. (29-4240)

_Standards_
BS 1377, BS 1924

_Attributes_
Description
	Metal Tray
	
Diameter, mm
	200 mm
	
Internal diameter mm
	200

[PRODUCT] 100mm Calibrating Container 100mm Id X 150mm Deep with 200mm Dia Rim. (29-4020)

_Standards_
BS 1377, BS 1924

_Attributes_
Description
	Calibrating Container
	
Diameter, mm
	100 mm
	
Internal diameter mm
	100

[PRODUCT] 150mm Calibrating Container 150mm Id X Deep with 250mm Dia Rim. (29-4120)

_Standards_
BS 1377, BS 1924

_Attributes_
Description
	Calibrating Container
	
Diameter, mm
	150 mm
	
Internal diameter mm
	150

[PRODUCT] 200mm Calibrating Container 200mm Id X 250mm Deep with A 350mm Dia Rim. (29-4220)

_Standards_
BS 1377, BS 1924

_Attributes_
Description
	Calibrating Container
	
Diameter, mm
	200 mm
	
Internal diameter mm
	200

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	Diameter, mm
	N/A for this Product Group

[PRODUCT GROUP] Sand Cone 6"

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	
29-4300
	6 Inch (152mm) Sand Cone
	
29-4320
	Plastic Container for Sand Cone
	
29-4340
	Density Plate
	
82-7401
	Standard Sand - 600/300 μm

[PRODUCT GROUP] Core Cutter Apparatus
In this method of determining the dry density of in-situ soil, a core-cutter of known volume is driven into the soil by a rammer. The core-cutter is removed, trimmed and the soil obtained is weighed and dried for a moisture/density check.

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	
29-5300
	Core Cutter 100mm
	
29-5320
	Driving Dolly
	
29-5340
	Driving Rammer

[PRODUCT GROUP] Field density tools

[PRODUCT] Density Spoon. (29-5000)
For removing soil from the hole

_Attributes_
Description
	Density Spoon
	
Weight, kg
	0.11

[PRODUCT] Soft Headed Mallet. (29-5020)

_Attributes_
Description
	Soft Headed Mallet
	
Weight, kg
	0.62

_Related Products_
Main: 100 X 100 X 500mm Beam Mould. (34-5003)
Main: 100mm Cube Mould 2-Part Clamp Type. Cast Iron Construction. BS EN Compliant. (34-4650)
Main: 100mm Cube Mould 4-Part Clamp Type. Cast Iron Construction. BS EN Compliant. (34-4520)
Main: 100mm Dia Cylinder Mould 200mm Long. (34-5210)
Main: 150 X 150 X 750mm Beam Mould. (34-5053)
Main: 150mm Cube Mould 2-Part Clamp Type. Cast Iron Construction. BS EN Compliant. (34-4670)
Main: 150mm Cube Mould 4-Part Clamp Type. Cast Iron Construction. BS EN Compliant. (34-4570)
Main: 150mm Dia Cylinder Mould 150mm Long. (34-5230)
Main: 150mm Dia Cylinder Mould 300mm Long. (34-5260)
Main: 200mm Cube Mould Clamp Type. Cast Iron Construction. Stamped Mould Sections. EN Compliant. (34-4620)
Main: Air Entrainment Meter B Type Complete with Carrying Case. Supplied with Aluminium Tamping Bar. (34-3265)
Main: Bulk Density Measure 10 Litre (34-2830)

[PRODUCT] Density Chisel. (29-5060)
With hardened tip

_Attributes_
Description
	Density Chisel
	
Weight, kg
	0.75

[PRODUCT] Metal Dibber Tool (29-5080)
For excavating hole

_Attributes_
Description
	Metal Dibber Tool
	
Weight, kg
	0.27

[PRODUCT] Density Hand Pick. (29-5120)
For excavating in difficult ground

_Attributes_
Description
	Density Hand Pick
	
Weight, kg
	0.76

[PRODUCT] Steel Pointed Rod. (29-5140)
With wooden handle

_Attributes_
Description
	Steel Pointed Rod
	
Weight, kg
	0.25

[GROUPED PRODUCT MATRIX]
Model No.
	Desc
	N/A for this Product Group